{"text_format":"1","workbook":"xlsx","n_sheets":18,"sheets":["Introduction","Data Input","Results","Calculation sheet","Sheet2","Data Quality Matrix","DATA ------------>","User Defined Excipient EFs","Original Excipient EFs","Reference Data","FPX Reference Data","Typical heat sources","Packaging EFs","TRANSPORT ----->","Transport EFs","TransportDefaults - ctry to UK","TransportDefault - between ctrs","TransDefaults - Input to form"],"not_rendered":{"charts":2,"images":2,"macros":1,"external_links":1,"defined_names":161,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Introduction","index":0,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":false,"merged":[[98,1,105,6],[77,1,84,6],[64,1,75,6],[85,1,96,6],[0,2,0,5],[41,2,41,6],[58,1,63,6],[56,1,56,6],[7,1,15,6],[19,1,28,6],[49,1,51,6],[30,1,39,6]]}
[]
[]
[]
[null,"INTRODUCTION"]
[]
[null,"Version: 1.2"]
[]
[null,"This tool was developed for ABPI by the Carbon Trust with contributions from ABPI members.\n\nThe aim of the tool is to provide a quick approximation of the carbon impacts of pharmaceutical tablets in blister packs. This information can be used for internal evaluations, assessing the carbon hot spots for individual products and screening product portfolios to prioritise more detailed footprinting studies and carbon reduction initiatives. In addition, it can be used to engage stakeholders in broader discussions around the impacts of the products. The tool is specific to the UK market.\n\nThe tool is not intended for direct product comparisons."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"USER GUIDE"]
[]
[null,"1. Navigating the Tool\n\nThe blue tabs at the top of each sheet allow the user to navigate between the various sections of the tool. User inputs are limited to the Data Input and User Defined Excipient emission factors tabs. Only light blue cells can be modified by the user. Most input fields have associated help boxes that can be displayed by clicking on the relevant i button.\n\nFor some fields, inputs are limited to values within a drop-down menu. This can be accessed by clicking on the arrow that appears next to the cell when it is selected. In some cases, selection of a specific input option will drive subsequent data entry options. In this case, all entry fields that are not applicable will be greyed out."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2. Uncertainty and Data Quality\n\nAs this tool is designed to provide a quick view of a product's carbon impact, it is important to also recognise and interpret the uncertainty associated with the result. The modelling uncertainty will be automatically estimated through statistical evaluation and a data quality matrix based on Greenhouse Gas Protocol guidance. \nIn most cases, the uncertainty data is calculated in the background of the tool. The user is encouraged to use their own calculated emission factors for the API or excipients,where available, as this is likely to reduce the measurement uncertainty and allow greater confidence in the results. Additional information is required for the tool to evaluate the data quality when a company uses their own emission factors. The assessment criteria are shown in the table below, adapted from the GHG Protocol Product Standard. A sixth uncertainty criterion is a basic uplift applied to different activities. For excipients this will typically be industrial products, but may also be agricultural products.\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Representativeness of the data in terms of:"]
[null,null,"Precision","Completeness ","Geography","Technology","Time"]
[null,"Very Good","Verified data based on measurements","Data from all relevant sites over an adequate time period","Data from the same area","Data based on same technology","Data with less than 3 years of difference"]
[null,"Good","Verified data partly based on assumptions or non-verified data based on measurements","Data from more than 50 per cent of sites for an adequate time period","Data from a similar area","Data based on similar technology","Data with less than 6 yearsof difference"]
[null,"Fair","Non-verified data partly based on assumptions or a qualified estimate","Data from less than 50 per cent of sites for an adequate time period or for more than 50 per cent of sites but for a shorter time period","Data from a different area","Data based on a different technology","Data with less than 10 years of difference"]
[null,"Poor","Non-qualified estimate","Data from less than 50 percent of sites for a limited time periods or representativenss is unknown","Area unknown","Data where technology is unknown","Data with more than 10 years of difference or age of data unknown"]
[]
[]
[null,"The User Defined Excipient EFs table provides the uncertainty value associated with the default factor provided in the tool. This way, the user can decide whether to use an alternative emission factor, which may have a lower uncertainty. Once the user has defined a bespoke emission factor, they are able to switch between this and the default value in the Data Input sheet."]
[]
[]
[]
[]
[null,"MODEL ASSUMPTIONS"]
[]
[null,"This section sets out some of the key assumptions used in the development of the tool."]
[]
[null,"1. API\n\nThe default emission factors and calculation model for APIs are based on the statistical assessment of 29 APIs that had been previously footprinted. Two regression models are used to provide the user with the option to include or exclude the number of chemical process steps involved in the manufacture of the API. Both regression models have an r2 value of 73%."]
[]
[]
[]
[]
[]
[null,"2. Transport and Distribution\n\nWith the exception of air freight, transport does not usually contribute a significant amount to the overall footprint of pharmaceuticals. As a result, transport data is requested in three distance bands (short, medium and long haul). The distances vary by mode of transport and are listed in the information box next to the input table for transport to formulation site.\n\nThe default transport route for APIs to formulation site is long-haul shipping and domestic road freight, whereas for excipients it is only domestic road freight. Defaults for transport from formulation site to packaging and packaging site to the UK are based on the country locations of the sites. Where formulation and packaging are co-located the user can set all transport modes to \"none\".\n\nUK transport and distribution is based on typical distances for transport from UK port to main distribution centre, regional distribution centres and on to pharmacies and hospitals. All journeys are done by road. The impact of storage at the distribution centres has also been included."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"3. Formulation and Packaging\n\nThe energy figures for formulation and packaging are based on average data from multiple facilities of one pharmaceutical company. Probably the largest variable affecting energy use per product output is the utilisation rate of the facility, due to the large overhead energy requirements for HVAC. This variable is not currently accounted for within the tool.\n\nThe carbon impact of the energy use is calculated based on the specific emission factors for the country location specified by the user."]
[]
[]
[]
[]
[]
[]
[]
[null,"4. Retail and Use Phase\n\nThe model distinguishes between pharmacies and hospitals in terms of the retail and use phase of the products. For pharmacies, it is assumed that each pack is sold in a paper bag with two adhesive labels. This is conservative, as it does not account for multiple prescriptions in one bag or non-prescription tablets which may not have the bag and labels.\n\nFor hospitals, the use phase includes the use of a disposable 30ml polypropylene cup in which tablets are presented to the patient. An average of two tablets per cup has been assumed. In practice, cups of other materials and sizes are used and the average number of tablets may not be representative, but no statistical data on these points was available from the NHS.\n\nWastage from unused tablets has not been taken into account. The functional units for this model are effectively per tablet or pack sold, rather than per tablet taken."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"5. End of Life\n\nThe end of life of the packaging is fully modelled within this tool, including the wastage during the packaging process and waste transport. For the cardboard and paper elements of the packaging, average commercial and domestic recycling rates have been applied, but the blister strip materials are assumed to be non-recyclable.\n\nThe emissions from disposal of the chemical waste arising at the various life cycle stages has not been modelled beyond a transport component."]

{"sheet":"Data Input","index":1,"n_rows":138,"n_cols":15,"rows_kept":138,"cut":false,"hidden":false,"merged":[[80,6,80,7],[81,6,81,7],[82,6,82,7],[75,6,75,7],[79,6,79,7],[78,6,78,7],[77,6,77,10],[55,6,55,7],[54,6,54,7],[72,6,72,7],[73,6,73,7],[74,6,74,7],[70,6,70,10],[71,6,71,7]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"1. Product Details"]
[]
[null,null,"Product Name"]
[]
[null,null,"Tablets per pack"]
[]
[null,null,"Weight per tablet (mg)",null,null,null,null,{"$f":"IF(G14<>(SUM(OFFSET(G25,0,0,1,APINumber))+SUM(OFFSET(I56,0,0,ExcipientNumber,1))),\"ERROR: The API and Excipient input weights do not add up to this number\",\"\")","v":""}]
[]
[]
[]
[null,null,"2. API Characteristics"]
[]
[null,null,"Number of APIs",null,"i",null,1]
[]
[null,null,null,null,null,null,"API 1","API 2","API 3"]
[null,null,"API Name"]
[]
[null,null,"API content per tablet (mg)"]
[]
[null,null,"Type of API Emission Factor:",null,"i",null,"Specific",null,"Specific"]
[]
[null,null,"SPECIFIC"]
[null,null,"Emission Factor (kg CO2e/kg API)"]
[]
[null,null,"Data Quality:"]
[null,null,"Precision"]
[null,null,"Completeness"]
[null,null,"Temporal representativeness"]
[null,null,"Geographical representativeness"]
[null,null,"Technological representativeness"]
[]
[null,null,"CALCULATED"]
[null,null,"Chiral?",null,"i"]
[]
[null,null,"Production scale (tpa)",null,"i"]
[]
[null,null,"Number of chemical steps (optional)",null,"i"]
[]
[null,null,"HIGH/MEDIUM/LOW"]
[null,null,"Average API emission factor",null,"i"]
[]
[]
[]
[null,null,"3. Formulation"]
[]
[null,null,"Number of excipients",null,"i",null,1]
[]
[null,null,null,null,null,null,"Excipient",null,"Content per tablet (mg)","Default/User Defined Emission Factor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J56=\"\",\"PLEASE SPECIFY THE TYPE OF EMISSION FACTOR FOR THIS EXCIPIENT (DEFAULT/USER DEFINED)\",IF(J56=\"User Defined\",IF(VLOOKUP(G56,'User Defined Excipient EFs'!A:C,2,FALSE)=\"\",\"PLEASE SPECIFY THE USER DEFINED EMISSION FACTOR FOR THIS EXCIPIENT IN THE 'User Defined Excipient EFs' TAB\",\"\"),\"\"))","v":"PLEASE SPECIFY THE TYPE OF EMISSION FACTOR FOR THIS EXCIPIENT (DEFAULT/USER DEFINED)"}]
[]
[]
[null,null,"Number of formulation sites",null,"i",null,1]
[]
[null,null,null,null,null,null,"Site 1",{"$f":"IF($G$59>=2,\"Site 2\",\"\")","v":""}]
[null,null,"Site name"]
[]
[null,null,"Country"]
[]
[null,null,"Process wastage rate",null,"i",null,0.02,0.02]
[null,null,null,null,null,null,"Default","Default"]
[]
[null,null,"Production share",null,"i",null,1,{"$f":"1-G69","v":0}]
[]
[null,null,"Transport of inputs to formulation",null,"i",null,"Site 1",null,null,null,null,null,null,null,"HIDE THIS COLUMN"]
[null,null,null,null,null,null,"Ingredient",null,"Air","Sea","Road",null,null,null,"Weight (mg)"]
[null,null,null,null,"i",null,{"$f":"IF(G23=\"\",\"\",G23)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I73=\"None\",I73=\"\"),IF(OR(J73=\"None\",J73=\"\"),IF(OR(K73=\"None\",K73=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,$G$25,FormulationSite1ProductionShare*$G$25)","v":0}]
[null,null,null,null,null,null,{"$f":"IF(H23=\"\",\"\",H23)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I74=\"None\",I74=\"\"),IF(OR(J74=\"None\",J74=\"\"),IF(OR(K74=\"None\",K74=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,$H$25,FormulationSite1ProductionShare*$H$25)","v":0}]
[null,null,null,null,null,null,{"$f":"IF(I23=\"\",\"\",I23)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I75=\"None\",I75=\"\"),IF(OR(J75=\"None\",J75=\"\"),IF(OR(K75=\"None\",K75=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,$I$25,FormulationSite1ProductionShare*$I$25)","v":0}]
[null,null,null,null,null,null,{"$f":"IF(G56=\"\",\"\",G56)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I76=\"None\",I76=\"\"),IF(OR(J76=\"None\",J76=\"\"),IF(OR(K76=\"None\",K76=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,I56,FormulationSite1ProductionShare*I56)","v":0}]
[]
[null,null,null,null,null,null,"Site 2"]
[null,null,null,null,null,null,"Ingredient",null,"Air","Sea","Road"]
[null,null,null,null,null,null,{"$f":"IF(G23=\"\",\"\",G23)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I80=\"None\",I80=\"\"),IF(OR(J80=\"None\",J80=\"\"),IF(OR(K80=\"None\",K80=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,$G$25,FormulationSite2ProductionShare*$G$25)","v":0}]
[null,null,null,null,null,null,{"$f":"IF(H23=\"\",\"\",H23)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I81=\"None\",I81=\"\"),IF(OR(J81=\"None\",J81=\"\"),IF(OR(K81=\"None\",K81=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,$H$25,FormulationSite2ProductionShare*$H$25)","v":0}]
[null,null,null,null,null,null,{"$f":"IF(I23=\"\",\"\",I23)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I82=\"None\",I82=\"\"),IF(OR(J82=\"None\",J82=\"\"),IF(OR(K82=\"None\",K82=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,$I$25,FormulationSite2ProductionShare*$I$25)","v":0}]
[null,null,null,null,null,null,{"$f":"IF(G56=\"\",\"\",G56)","v":""},null,null,null,null,"User Defined",{"$f":"IF(OR(I83=\"None\",I83=\"\"),IF(OR(J83=\"None\",J83=\"\"),IF(OR(K83=\"None\",K83=\"\"),\"Please enter at least one transport mode\",\"\"),\"\"),\"\")","v":"Please enter at least one transport mode"},null,{"$f":"IF(FormulationNumber=1,0,FormulationSite2ProductionShare*I56)","v":0}]
[]
[]
[]
[]
[null,null,"4. Packaging"]
[]
[null,null,"Packaging country"]
[]
[null,null,"Packaging split dropdown:",null,"i",null,"User Defined"]
[]
[null,null,"No. of blister strips per retail pack",null,"i"]
[]
[null,null,"No. of retail packs per outer box",null,"i"]
[]
[null,null,"No. of outer boxes per pallet",null,"i"]
[]
[null,null,"% of product lost during packaging",null,"i",null,5.0000000000000001E-3,"Default"]
[]
[null,null,"% of packaging lost during packaging",null,"i",null,2.5000000000000001E-2,"Default"]
[]
[null,null,"Select packaging calculation method",null,"i"]
[]
[null,null,"Select default blister pack size",null,"i",null,"Medium"]
[]
[null,null,null,null,null,null,"Material","Weight (g)"]
[null,null,"Bill of Materials per blister pack"]
[]
[]
[]
[]
[null,null,"Bill of Materials per retail pack",null,"i"]
[]
[]
[]
[null,null,"Bill of Materials per outer box"]
[]
[]
[null,null,"Packaging Transport"]
[null,null,null,null,null,null,"Air","Sea","Road"]
[null,null,"Formulation site 1 to packaging",null,"i",null,null,null,null,"User Defined"]
[null,null,"Formulation site 2 to packaging",null,"i",null,null,null,null,"User Defined"]
[null,null,"From Packaging to UK",null,"i",null,null,null,null,"User Defined"]
[]
[]
[]
[null,null,"5. Distribution and Retail"]
[]
[null,null,"Sales split",null,null,null,"Default Split"]
[null,null,"NHS hospital",null,null,null,0.3]
[null,null,"Other hospital",null,null,null,0.1]
[null,null,"Pharmacy (NHS prescription)",null,null,null,0.5]
[null,null,"Pharmacy (non-NHS)/retail",null,null,null,0.1]
[null,null,null,null,null,null,{"$f":"IF(SUM(G132:G135)<>1,\"Error: Total does not sum to 100%\",\"\")","v":""}]
[]
[null,null,"Distribution and retail wastage rate",null,"i",null,0.02,"Default"]

{"sheet":"Results","index":2,"n_rows":71,"n_cols":15,"rows_kept":71,"cut":false,"hidden":false,"merged":[[0,3,0,6]]}
[]
[]
[]
[]
[null,"Results"]
[]
[null,"Product Name",{"$f":"ProductName","v":0}]
[null,"Tablet size (mg)",{"$f":"IF('Data Input'!G14=\"\",\"\",'Data Input'!G14)","v":""}]
[null,"Tablets per pack",{"$f":"IF('Data Input'!G12=\"\",\"\",'Data Input'!G12)","v":""}]
[]
[null,"Summary Overview"]
[null,null,null,"Emissions per pack (gCO2e)","Emissions per tablet (gCO2e)","Percentage ","Uncertainty factor","High (gCO2e)","Low (gCO2e)","Wastage emissions per tablet","Waste %ge of total",null,"High Error Bar","Low Error Bar"]
[null,"Total Footprint",null,{"$f":"IFERROR(E13*$C$9,\"\")","v":""},{"$f":"IFERROR(E17+E21+E25+E29+E32+E33,\"\")","v":""},{"$f":"IFERROR(E13/$E$13,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!F47,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G47/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H47/1000,\"\")","v":""},{"$f":"IFERROR(J17+J21+J25+J29+J32+J33,\"\")","v":0},{"$f":"J13/E13","v":{"$error":"#VALUE!"}},null,{"$f":"H13-E13","v":{"$error":"#VALUE!"}},{"$f":"E13-I13","v":{"$error":"#VALUE!"}},"i"]
[null,"Material inputs","API",{"$f":"IFERROR(E14*$C$9,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!D48/1000,\"\")","v":0},{"$f":"IFERROR(E14/$E$13,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!F48,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G48/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H48/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I48/1000,\"\")","v":0},{"$f":"J14/E14","v":{"$error":"#DIV/0!"}},null,{"$f":"H14-E14","v":{"$error":"#VALUE!"}},{"$f":"E14-I14","v":{"$error":"#VALUE!"}}]
[null,"Material inputs","Excipients","",{"$f":"IFERROR('Calculation sheet'!D49/1000,\"\")","v":0},"",{"$f":"IFERROR('Calculation sheet'!F49,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G49/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H49/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I49/1000,\"\")","v":0},{"$f":"J15/E15","v":{"$error":"#DIV/0!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Material inputs","Packaging Materials","",{"$f":"IFERROR('Calculation sheet'!D50/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F50,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G50/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H50/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I50/1000,\"\")","v":""},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Material inputs",null,"",{"$f":"IFERROR('Calculation sheet'!D51/1000,\"\")","v":0},"",{"$f":"IFERROR('Calculation sheet'!F51,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G51/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H51/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I51/1000,\"\")","v":0},{"$error":"#DIV/0!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Formulation","Energy","",{"$f":"IFERROR('Calculation sheet'!D52/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F52,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G52/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H52/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I52/1000,\"\")","v":""},{"$f":"IFERROR(J18/E18,0)","v":0},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Formulation","In-bound Transport","",{"$f":"IFERROR('Calculation sheet'!D53/1000,\"\")","v":0},"",{"$f":"IFERROR('Calculation sheet'!F53,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G53/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H53/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I53/1000,\"\")","v":0},{"$f":"IFERROR(J19/E19,0)","v":0},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Formulation","Waste","",{"$f":"IFERROR('Calculation sheet'!D54/1000,\"\")","v":0},"",{"$f":"IFERROR('Calculation sheet'!F54,\"\")","v":1},{"$f":"IFERROR('Calculation sheet'!G54/1000,\"\")","v":0},{"$f":"IFERROR('Calculation sheet'!H54/1000,\"\")","v":0},{"$f":"IFERROR('Calculation sheet'!I54/1000,\"\")","v":0},{"$f":"IFERROR(J20/E20,0)","v":0},null,0,0]
[null,"Formulation",null,"",{"$f":"IFERROR('Calculation sheet'!D55/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F55,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G55/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H55/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I55/1000,\"\")","v":0},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Packaging","Energy","",{"$f":"IFERROR('Calculation sheet'!D56/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F56,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G56/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H56/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I56/1000,\"\")","v":""},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Packaging","In-bound Transport","",{"$f":"IFERROR('Calculation sheet'!D57/1000,\"\")","v":0},"",{"$f":"IFERROR('Calculation sheet'!F57,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G57/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H57/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I57/1000,\"\")","v":0},{"$error":"#DIV/0!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Packaging","Waste","",{"$f":"IFERROR('Calculation sheet'!D58/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F58,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G58/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H58/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I58/1000,\"\")","v":""},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Packaging Process",null,"",{"$f":"IFERROR('Calculation sheet'!D59/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F59,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G59/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H59/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I59/1000,\"\")","v":0},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Distibution","RDC","",{"$f":"IFERROR('Calculation sheet'!D60/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F60,\"\")","v":4.1132503787829275},{"$f":"IFERROR('Calculation sheet'!G60/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H60/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I60/1000,\"\")","v":""},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Distibution","Transport","",{"$f":"IFERROR('Calculation sheet'!D61/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F61,\"\")","v":1.3220579299510793},{"$f":"IFERROR('Calculation sheet'!G61/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H61/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I61/1000,\"\")","v":""},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,"Waste","",{"$f":"IFERROR('Calculation sheet'!D62/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F62,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G62/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H62/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I62/1000,\"\")","v":""},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Distribution",null,"",{"$f":"IFERROR('Calculation sheet'!D63/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F63,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G63/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H63/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I63/1000,\"\")","v":0},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Retail & Use ","NHS","",{"$f":"IFERROR('Calculation sheet'!D64/1000,\"\")","v":3.5247291884818313},"",{"$f":"IFERROR('Calculation sheet'!F64,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G64/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H64/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I64/1000,\"\")","v":0},{"$f":"IFERROR(J30/E30,0)","v":0},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Retail & Use ","Retail Pharmacies","",{"$f":"IFERROR('Calculation sheet'!D65/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F65,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G65/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H65/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I65/1000,\"\")","v":0},{"$f":"IFERROR(J31/E31,0)","v":0},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Retail & Use ",null,"",{"$f":"IFERROR('Calculation sheet'!D66/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F66,\"\")","v":0},{"$f":"IFERROR('Calculation sheet'!G66/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H66/1000,\"\")","v":0},{"$f":"IFERROR('Calculation sheet'!I66/1000,\"\")","v":0},{"$f":"IFERROR(J32/E32,0)","v":0},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"End of Life",null,"",{"$f":"IFERROR('Calculation sheet'!D67/1000,\"\")","v":""},"",{"$f":"IFERROR('Calculation sheet'!F67,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!G67/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!H67/1000,\"\")","v":""},{"$f":"IFERROR('Calculation sheet'!I67/1000,\"\")","v":0},{"$error":"#VALUE!"},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Key Model Parameters and Assumptions"]
[]
[null,"API"]
[]
[null,{"$f":"'Data Input'!G23&\" is based on \"&API1_Type&\" data\"","v":" is based on Specific data"},null,"Emission factor:",{"$f":"'Calculation sheet'!B99","v":0},"kgCO2e/kg"]
[null,{"$f":"'Data Input'!H23&\" is based on \"&API2_Type&\" data\"","v":" is based on  data"},null,"Emission factor:",{"$f":"'Calculation sheet'!B100","v":""},"kgCO2e/kg"]
[null,{"$f":"'Data Input'!I23&\" is based on \"&API3_Type&\" data\"","v":" is based on Specific data"},null,"Emission factor:",{"$f":"'Calculation sheet'!B101","v":0},"kgCO2e/kg"]
[]
[null,"Excipients"]
[]
[null,{"$f":"COUNTIFS(OFFSET('Data Input'!$J$56,0,0,ExcipientNumber),\"User Defined\")&\" excipient(s) have a user defined emission factors\"","v":"0 excipient(s) have a user defined emission factors"}]
[null,{"$f":"COUNTIFS(OFFSET('Data Input'!$J$56,0,0,ExcipientNumber),\"Default\")&\" excipient(s) use default emission factors\"","v":"0 excipient(s) use default emission factors"}]
[]
[null,"Packaging"]
[]
[null,{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",\"Packaging is user defined\",\"Packaging is based on default data for \"&WasteDefault&\" pack size\")","v":"Packaging is based on default data for Medium pack size"}]

{"sheet":"Calculation sheet","index":3,"n_rows":534,"n_cols":15,"rows_kept":534,"cut":false,"hidden":true,"merged":[[508,11,508,14],[515,11,515,14],[521,11,521,14],[515,3,515,6],[521,3,521,6],[515,7,515,10],[521,7,521,10],[508,7,508,10],[474,10,474,13],[483,2,483,5],[483,6,483,9],[483,10,483,13],[492,10,492,13],[293,5,293,7],[311,5,311,7],[510,0,513,0],[517,0,519,0],[523,0,524,0],[293,2,293,4],[311,2,311,4],[374,1,374,3],[391,1,391,3],[374,4,374,6],[391,4,391,6],[492,2,492,5],[492,6,492,9],[474,2,474,5],[474,6,474,9],[508,3,508,6]]}
[]
[]
[]
["WEIGHTS:"]
[]
["CHEMICALS:"]
[]
["Formulation Site 1"]
["Total Chemical Weight Per Tablet (mg)",{"$f":"IF(FormulationNumber=1,(SUM(OFFSET('Data Input'!G25,0,0,1,APINumber))+SUM(OFFSET(ExcipientStart,0,2,ExcipientNumber,1))),(FormulationSite1ProductionShare*(SUM(OFFSET('Data Input'!G25,0,0,1,APINumber))+SUM(OFFSET(ExcipientStart,0,2,ExcipientNumber,1)))))","v":0}]
[]
["Formulation Site 2"]
["Total Chemical Weight Per Tablet (mg)",{"$f":"IF(FormulationNumber=1,0,(FormulationSite2ProductionShare*(SUM(OFFSET('Data Input'!G25,0,0,1,APINumber))+SUM(OFFSET(ExcipientStart,0,2,ExcipientNumber,1)))))","v":0}]
[]
["Total Chemical Weight Per Tablet (mg)",{"$f":"SUM(OFFSET(API1Mass,0,0,1,APINumber))+SUM(OFFSET(ExcipientStart,0,2,ExcipientNumber,1))","v":0}]
[]
["PACKAGING:"]
[]
["NOTE: DOES NOT INCLUDE PALLET WEIGHT"]
["Weight per tablet (mg):",{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",SUM(B211:B214,B219:B221,B226:B227),IF(PackagingCalculationMethod=\"Use defaults\",'Reference Data'!$B$35,\"\"))","v":""}]
["Weight per pack (mg):",{"$f":"B19*TabletsPerPack","v":{"$error":"#VALUE!"}}]
[]
["CONVERSION FACTORS:"]
[]
["WASTAGE UPLIFTS:"]
[]
["(ln(U))2","Uplift","U (uncertainty factor)","(ln U)2"]
["Formulation Site 1",{"$f":"1/(1-'Data Input'!G66)","v":1.0204081632653061},{"$f":"IF(Site1ProcessWastageRateDropdown=\"User Defined\",'Data Quality Matrix'!$N$51,IF(Site1ProcessWastageRateDropdown=\"Default\",'Data Quality Matrix'!$N$52,\"\"))","v":1.6400080773205654},{"$f":"LN(C27)^2","v":0.24472924465040088}]
["Formulation Site 2",{"$f":"1/(1-'Data Input'!H66)","v":1.0204081632653061},{"$f":"IF(Site2ProcessWastageRateDropdown=\"User Defined\",'Data Quality Matrix'!$N$51,IF(Site2ProcessWastageRateDropdown=\"Default\",'Data Quality Matrix'!$N$52,\"\"))","v":1.6400080773205654},{"$f":"LN(C28)^2","v":0.24472924465040088}]
["Product Wastage during Packaging",{"$f":"1/(1-'Data Input'!G100)","v":1.0050251256281406},{"$f":"IF(PercentProductLostInPackagingDropdown=\"User Defined\",'Data Quality Matrix'!$N$51,IF(PercentProductLostInPackagingDropdown=\"Default\",'Data Quality Matrix'!$N$52,\"\"))","v":1.6400080773205654},{"$f":"LN(C29)^2","v":0.24472924465040088}]
["Packaging Wastage during Packaging",{"$f":"1/(1-'Data Input'!G102)","v":1.0256410256410258},{"$f":"IF(PercentPackagingLostInPackagingDropdown=\"User Defined\",'Data Quality Matrix'!$N$51,IF(PercentPackagingLostInPackagingDropdown=\"Default\",'Data Quality Matrix'!$N$52,\"\"))","v":1.6400080773205654},{"$f":"LN(C30)^2","v":0.24472924465040088}]
["RDC",{"$f":"1/(1-'Data Input'!G138)","v":1.0204081632653061},{"$f":"IF(RDCWastageDropdown=\"User Defined\",'Data Quality Matrix'!$N$51,IF(RDCWastageDropdown=\"Default\",'Data Quality Matrix'!$N$52,\"\"))","v":1.6400080773205654},{"$f":"LN(C31)^2","v":0.24472924465040088}]
[]
[]
["EFFECT OF WASTAGE FACTORS:"]
[]
["Before RDC:",{"$f":"(1/(1-'Data Input'!G138))-1","v":2.0408163265306145E-2}]
["Before packaging - chemical:",{"$f":"(1/((1-'Data Input'!G138)*(1-'Data Input'!G100)))-1","v":2.5535842477694581E-2}]
["Before packaging - packaging:",{"$f":"(1/((1-'Data Input'!G138)*(1-'Data Input'!G102)))-1","v":4.6572475143903613E-2}]
["Before Formulation Site 1:",{"$f":"(1/((1-'Data Input'!G138)*(1-'Data Input'!G100)*(1-'Data Input'!G66)))-1","v":4.6465145385402806E-2}]
["Before Formulation Site 2:",{"$f":"(1/((1-'Data Input'!G138)*(1-'Data Input'!G100)*(1-'Data Input'!H66)))-1","v":4.6465145385402806E-2}]
[]
["SUMMARY FIGURES"]
[]
["Total emissions (mg CO2e per tablet):",{"$f":"D47","v":{"$error":"#N/A"}}]
[]
[null,null,"Emissions per pack","Emissions per tablet","Percentage ","Uncertainty factor","High ","Low","Waste emissions per tablet","%ge of total",null,{"$f":"EXP(SQRT(SUM(K48:K50,K52:K54,K56:K58,K60:K62)))","v":{"$error":"#DIV/0!"}},{"$f":"EXP(SQRT(SUM(K51,K55,K59,K63)))","v":{"$error":"#N/A"}}]
["Total Footprint",null,null,{"$f":"D51+D55+D59+D63+D66+D67","v":{"$error":"#N/A"}},{"$f":"D47/$D$47","v":{"$error":"#N/A"}},{"$f":"EXP(SQRT(SUM(K51,K55,K59,K63,K66,K67)))","v":{"$error":"#N/A"}},{"$f":"F47*D47","v":{"$error":"#N/A"}},{"$f":"D47/F47","v":{"$error":"#N/A"}}]
["Material inputs","API",null,{"$f":"B85","v":0},{"$f":"D48/$D$47","v":{"$error":"#N/A"}},{"$f":"EXP(SQRT(B86))","v":{"$error":"#DIV/0!"}},{"$f":"F48*D48","v":{"$error":"#DIV/0!"}},{"$f":"D48/F48","v":{"$error":"#DIV/0!"}},{"$f":"B87+B88","v":0},null,{"$f":"(D48/$D$51)^2*LN(F48)^2","v":{"$error":"#DIV/0!"}}]
["Material inputs","Excipients",null,{"$f":"B116","v":0},{"$error":"#N/A"},{"$f":"EXP(SQRT(B164))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"B118+B119","v":0},null,{"$f":"(D49/$D$51)^2*LN(F49)^2","v":{"$error":"#DIV/0!"}}]
["Material inputs","Packaging",null,{"$f":"B163","v":""},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(B164))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"B165","v":{"$error":"#VALUE!"}},null,{"$f":"(D50/$D$51)^2*LN(F50)^2","v":{"$error":"#VALUE!"}}]
["Material inputs",null,null,{"$f":"SUM(D48:D50)","v":0},{"$error":"#N/A"},{"$f":"EXP(SQRT(SUM(K48:K50)))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"E51^2*LN(F51)^2","v":{"$error":"#N/A"}}]
["Formulation","Energy",null,{"$f":"B236","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"EXP(SQRT(B237))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"B238","v":{"$error":"#N/A"}},null,{"$f":"(D52/$D$55)^2*LN(F52)^2","v":{"$error":"#N/A"}}]
["Formulation","In-bound Transport",null,{"$f":"B305+B323+B344+B363","v":0},{"$error":"#N/A"},{"$f":"EXP(SQRT(B306+B345+IF(FormulationNumber=2,B324+B364)))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"B307+B325+B346+B365","v":0},null,{"$f":"(D53/$D$55)^2*LN(F53)^2","v":{"$error":"#N/A"}}]
["Formulation","Waste",null,0,{"$error":"#N/A"},1,0,0,null,null,{"$f":"(D54/$D$55)^2*LN(F54)^2","v":{"$error":"#N/A"}}]
["Formulation",null,null,{"$f":"SUM(D52:D54)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"EXP(SQRT(SUM(K52:K54)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$f":"E55^2*LN(F55)^2","v":{"$error":"#N/A"}}]
["Packaging","Energy",null,{"$f":"B271","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"EXP(SQRT(B272))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"B273","v":{"$error":"#N/A"}},null,{"$f":"(D56/$D$59)^2*LN(F56)^2","v":{"$error":"#N/A"}}]
["Packaging","In-bound Transport",null,{"$f":"SUM(B377:D378)","v":0},{"$error":"#N/A"},{"$f":"EXP(SQRT(SUM(H377:H378)))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"B382","v":0},null,{"$f":"(D57/$D$59)^2*LN(F57)^2","v":{"$error":"#N/A"}}]
["Packaging","Waste",null,{"$f":"D458+D534","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(D459))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"D58","v":{"$error":"#VALUE!"}},null,{"$f":"(D58/$D$59)^2*LN(F58)^2","v":{"$error":"#VALUE!"}}]
["Packaging",null,null,{"$f":"SUM(D56:D58)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"EXP(SQRT(SUM(K56:K58)))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$f":"E59^2*LN(F59)^2","v":{"$error":"#N/A"}}]
["Distibution","RDC",null,{"$f":"B404","v":""},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(B406*B407))","v":4.1132503787829275},{"$f":"F60*D60","v":{"$error":"#VALUE!"}},{"$f":"D60/F60","v":{"$error":"#VALUE!"}},{"$f":"B409","v":{"$error":"#VALUE!"}},null,{"$f":"(D60/$D$63)^2*LN(F60)^2","v":{"$error":"#VALUE!"}}]
["Distibution","Transport",null,{"$f":"B414","v":""},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(B416*B417))","v":1.3220579299510793},{"$f":"F61*D61","v":{"$error":"#VALUE!"}},{"$f":"D61/F61","v":{"$error":"#VALUE!"}},{"$f":"B419","v":{"$error":"#VALUE!"}},null,{"$f":"(D61/$D$63)^2*LN(F61)^2","v":{"$error":"#VALUE!"}}]
[null,"Waste",null,{"$f":"C458+D533","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(C459))","v":{"$error":"#VALUE!"}},{"$f":"F62*D62","v":{"$error":"#VALUE!"}},{"$f":"D62/F62","v":{"$error":"#VALUE!"}},{"$f":"D62","v":{"$error":"#VALUE!"}},null,{"$f":"(D62/$D$63)^2*LN(F62)^2","v":{"$error":"#VALUE!"}}]
["Distribution",null,null,{"$f":"SUM(D60:D62)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(SUM(K60:K62)))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,{"$f":"E63^2*LN(F63)^2","v":{"$error":"#VALUE!"}}]
["Retail & Use ","NHS",null,{"$f":"B436","v":3524.7291884818314},{"$error":"#N/A"},{"$f":"EXP(SQRT(F436))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"(D64/$D$66)^2*LN(F64)^2","v":{"$error":"#DIV/0!"}}]
["Retail & Use ","Retail Pharmacies",null,{"$f":"B450","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"EXP(SQRT(F450))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,{"$f":"(D65/$D$66)^2*LN(F65)^2","v":{"$error":"#DIV/0!"}}]
["Retail & Use ",null,null,{"$f":"SUM(D64:D65)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"IFERROR(EXP(SQRT(SUM(K64:K65))),0)","v":0},{"$error":"#DIV/0!"},{"$f":"IFERROR(D66/F66,0)","v":0},null,null,{"$f":"IFERROR(E66^2*LN(F66)^2,)","v":0}]
["End of Life",null,null,{"$f":"B458+D532","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"EXP(SQRT(B459))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},0,null,{"$f":"E67^2*LN(F67)^2","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
["MATERIAL EMISSIONS"]
[]
[]
[]
[]
["APIs"]
[]
["API Summary:"]
[]
["API Material Emissions per tablet (mg CO2e):",{"$f":"SUM(OFFSET(C99,0,0,APINumber,FormulationNumber))","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(OFFSET(K99,0,0,APINumber,FormulationNumber))","v":{"$error":"#DIV/0!"}}]
["Effect of waste - Site 1 (mg CO2e per tablet):",{"$f":"SUM(OFFSET(C99,0,0,APINumber,1))*$B$39","v":0}]
["Effect of waste - Site 2 (mg CO2e per tablet):",{"$f":"SUM(OFFSET(D99,0,0,APINumber,1))*$B$40","v":0}]
[]
["Coefficients for calculated EF:"]
[]
[null,"Intercept","log10scale - coefficient","(log10scale)2 - coefficient","Chirality - coefficient","No. of chemical steps","Standard Error (log domain)","API 1","API 2","API 3"]
["Excluding no. of steps",3.3316320390420344,-0.13419641795442108,-0.10869884907885852,0.40654263943547142,null,0.32641669685673314,{"$f":"10^($B$93+($C$93*LOG10('Data Input'!G42))+($D$93*(LOG10('Data Input'!G42)^2))+IF('Data Input'!G40=\"YES\",$E$93,0))","v":{"$error":"#NUM!"}},{"$f":"10^($B$93+($C$93*LOG10('Data Input'!H42))+($D$93*(LOG10('Data Input'!H42)^2))+IF('Data Input'!H40=\"YES\",$E$93,0))","v":{"$error":"#NUM!"}},{"$f":"10^($B$93+($C$93*LOG10('Data Input'!I42))+($D$93*(LOG10('Data Input'!I42)^2))+IF('Data Input'!I40=\"YES\",$E$93,0))","v":{"$error":"#NUM!"}}]
["Including no.of steps",3.0571824565617072,null,-0.13133272418518982,0.32541912808779583,3.2694382839110914E-2,0.32632254550446516,{"$f":"10^($B$94+($D$94*(LOG10('Data Input'!G42)^2))+'Data Input'!G44*$F$94+IF('Data Input'!G40=\"YES\",$E$94,0))","v":{"$error":"#NUM!"}},{"$f":"10^($B$94+($D$94*(LOG10('Data Input'!H42)^2))+'Data Input'!H44*$F$94+IF('Data Input'!H40=\"YES\",$E$94,0))","v":{"$error":"#NUM!"}},{"$f":"10^($B$94+($D$94*(LOG10('Data Input'!I42)^2))+'Data Input'!I44*$F$94+IF('Data Input'!I40=\"YES\",$E$94,0))","v":{"$error":"#NUM!"}}]
[]
["Calculations:"]
[]
[null,"Emission Factor","Material Emissions Site 1 (mg CO2e per tablet)","Material Emissions Site 2 (mg CO2e per tablet)","UA","UEF","S Site 12","S Site 22","(ln UE Site 1)2","(ln UE Site 2)2","S Site 12 x (ln UE Site 1)2","S Site 22 x (ln UE Site 2)2"]
["API 1",{"$f":"IF(API1_Type='Reference Data'!$A$5,API1_Specific,IF(API1_Type='Reference Data'!$A$6,IF('Data Input'!G44=\"\",H93,H94),IF(API1_Type='Reference Data'!$A$7,VLOOKUP(API1_HighMediumLow,APIGenericEFs,2,FALSE),IF(API1_Type='Reference Data'!$A$8,'Reference Data'!$B$18,\"\"))))","v":0},{"$f":"IF(FormulationNumber=1,1,FormulationSite1ProductionShare)*B99*API1Mass*$B$27*$B$29*$B$31","v":0},{"$f":"IF(FormulationNumber=1,0,FormulationSite2ProductionShare)*B99*API1Mass*$B$28*$B$29*$B$31","v":0},{"$f":"'Data Quality Matrix'!$N$45","v":1},{"$f":"IF(API1_Type='Reference Data'!$A$5,G105,IF(API1_Type='Reference Data'!$A$6,10^(2*$G$93),IF(API1_Type='Reference Data'!$A$7,'Data Quality Matrix'!N28,IF(API1_Type='Reference Data'!$A$8,'Data Quality Matrix'!N27,\"\"))))","v":{"$error":"#N/A"}},{"$f":"(C99/$B$85)^2","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"LN($E99)^2+LN($F99)^2+$D$27+$D$29+$D$31","v":{"$error":"#N/A"}},{"$f":"LN($E99)^2+LN($F99)^2+$D$28+$D$29+$D$31","v":{"$error":"#N/A"}},{"$f":"G99*I99","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
["API 2",{"$f":"IF(API2_Type='Reference Data'!$A$5,API2_Specific,IF(API2_Type='Reference Data'!$A$6,IF('Data Input'!H44=\"\",I93,I94),IF(API2_Type='Reference Data'!$A$7,VLOOKUP(API2_HighMediumLow,APIGenericEFs,2,FALSE),IF(API2_Type='Reference Data'!$A$8,'Reference Data'!$B$18,\"\"))))","v":""},{"$f":"IF(FormulationNumber=1,1,FormulationSite1ProductionShare)*B100*API2Mass*$B$27*$B$29*$B$31","v":{"$error":"#VALUE!"}},{"$f":"IF(FormulationNumber=1,0,FormulationSite2ProductionShare)*B100*API2Mass*$B$28*$B$29*$B$31","v":{"$error":"#VALUE!"}},{"$f":"'Data Quality Matrix'!$N$45","v":1},{"$f":"IF(API2_Type='Reference Data'!$A$5,G106,IF(API2_Type='Reference Data'!$A$6,10^(2*$G$93),IF(API2_Type='Reference Data'!$A$7,'Data Quality Matrix'!N28,IF(API2_Type='Reference Data'!$A$8,'Data Quality Matrix'!N27,\"\"))))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"LN($E100)^2+LN($F100)^2+$D$27+$D$29+$D$31","v":{"$error":"#VALUE!"}},{"$f":"LN($E100)^2+LN($F100)^2+$D$28+$D$29+$D$31","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["API 3",{"$f":"IF(API3_Type='Reference Data'!$A$5,API3_Specific,IF(API3_Type='Reference Data'!$A$6,IF('Data Input'!I44=\"\",J93,J94),IF(API3_Type='Reference Data'!$A$7,VLOOKUP(API3_HighMediumLow,APIGenericEFs,2,FALSE),IF(API3_Type='Reference Data'!$A$8,'Reference Data'!$B$18,\"\"))))","v":0},{"$f":"IF(FormulationNumber=1,1,FormulationSite1ProductionShare)*B101*API3Mass*$B$27*$B$29*$B$31","v":0},{"$f":"IF(FormulationNumber=1,0,FormulationSite2ProductionShare)*B101*API3Mass*$B$28*$B$29*$B$31","v":0},{"$f":"'Data Quality Matrix'!$N$45","v":1},{"$f":"IF(API3_Type='Reference Data'!$A$5,G107,IF(API3_Type='Reference Data'!$A$6,10^(2*$G$93),IF(API3_Type='Reference Data'!$A$7,'Data Quality Matrix'!N28,IF(API3_Type='Reference Data'!$A$8,'Data Quality Matrix'!N27,\"\"))))","v":{"$error":"#N/A"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"LN($E101)^2+LN($F101)^2+$D$27+$D$29+$D$31","v":{"$error":"#N/A"}},{"$f":"LN($E101)^2+LN($F101)^2+$D$28+$D$29+$D$31","v":{"$error":"#N/A"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
["U for Specific Efs","U Precision","U Completeness","U Temporal representativeness","U Geographical representativeness","U Technological representativeness","U E"]
["API 1",{"$f":"HLOOKUP('Data Input'!$G$33,'Data Quality Matrix'!$B$3:$E$8,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$G$34,'Data Quality Matrix'!$B$3:$E$8,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$G$35,'Data Quality Matrix'!$B$3:$E$8,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$G$36,'Data Quality Matrix'!$B$3:$E$8,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$G$37,'Data Quality Matrix'!$B$3:$E$8,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"EXP(SQRT((LN(B105)^2+LN(C105)^2+LN(D105)^2+LN(E105)^2+LN(F105)^2)))","v":{"$error":"#N/A"}}]
["API 2",{"$f":"HLOOKUP('Data Input'!$H$33,'Data Quality Matrix'!$B$3:$E$8,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$H$34,'Data Quality Matrix'!$B$3:$E$8,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$H$35,'Data Quality Matrix'!$B$3:$E$8,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$H$36,'Data Quality Matrix'!$B$3:$E$8,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$H$37,'Data Quality Matrix'!$B$3:$E$8,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"EXP(SQRT((LN(B106)^2+LN(C106)^2+LN(D106)^2+LN(E106)^2+LN(F106)^2)))","v":{"$error":"#N/A"}}]
["API 3",{"$f":"HLOOKUP('Data Input'!$I$33,'Data Quality Matrix'!$B$3:$E$8,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$I$34,'Data Quality Matrix'!$B$3:$E$8,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$I$35,'Data Quality Matrix'!$B$3:$E$8,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$I$36,'Data Quality Matrix'!$B$3:$E$8,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"HLOOKUP('Data Input'!$I$37,'Data Quality Matrix'!$B$3:$E$8,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"EXP(SQRT((LN(B107)^2+LN(C107)^2+LN(D107)^2+LN(E107)^2+LN(F107)^2)))","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
["EXCIPIENTS"]
[]
["Summary:"]
[]
["Material Emissions per tablet (mg CO2e):",{"$f":"SUM(OFFSET(F122,0,0,ExcipientNumber,FormulationNumber))","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(OFFSET(N122,0,0,ExcipientNumber,FormulationNumber))","v":{"$error":"#DIV/0!"}}]
["Effect of waste - Site 1 (mg CO2e per tablet):",{"$f":"SUM(OFFSET(F122,0,0,ExcipientNumber,1))*$B$39","v":0}]
["Effect of waste - Site 2 (mg CO2e per tablet):",{"$f":"SUM(OFFSET(G122,0,0,ExcipientNumber,1))*$B$40","v":0}]
[]
["Offset Number (to drive formulae)","Excipient name","Weight","Default/User Defined?","Emission Factor","Material Emissions Site 1 (mg CO2e per tablet)","Material Emissions Site 2 (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S Site 12","S Site 22","(ln UE Site 1)2","(ln UE Site 2)2","S Site 12 x (ln UE Site 1)2","S Site 22 x (ln UE Site 2)2"]
[0,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A122,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A122,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A122,3,1,1)","v":0},{"$f":"IF(D122=\"Default\",VLOOKUP(B122,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B122,'Original Excipient EFs'!A:C,3,FALSE))","v":false},{"$f":"IF(FormulationNumber=1,1,FormulationSite1ProductionShare)*$C122*$E122*$B$27*$B$29*$B$31","v":0},{"$f":"IF(FormulationNumber=1,0,FormulationSite2ProductionShare)*$C122*$E122*$B$28*$B$29*$B$31","v":0},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D122=\"Default\",LN(VLOOKUP(B122,'Original Excipient EFs'!A2:R47,18,FALSE))^2,IF(D122=\"User Defined\",VLOOKUP(B122,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$f":"(F122/$B$116)^2","v":{"$error":"#DIV/0!"}},{"$f":"(G122/$B$116)^2","v":{"$error":"#DIV/0!"}},{"$f":"H122+I122+$D$27+$D$29+$D$31","v":{"$error":"#VALUE!"}},{"$f":"H122+I122+$D$28+$D$29+$D$31","v":{"$error":"#VALUE!"}},{"$f":"J122*L122","v":{"$error":"#DIV/0!"}},{"$f":"K122*M122","v":{"$error":"#DIV/0!"}}]
[{"$f":"A122+1","v":1},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A123,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A123,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A123,3,1,1)","v":0},{"$f":"IF(D123=\"Default\",VLOOKUP(B123,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B123,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D123=\"Default\",LN(VLOOKUP(B123,'Original Excipient EFs'!A3:R48,18,FALSE))^2,IF(D123=\"User Defined\",VLOOKUP(B123,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$f":"(F123/$B$116)^2","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"H123+I123+$D$27+$D$29+$D$31","v":{"$error":"#VALUE!"}},{"$f":"H123+I123+$D$28+$D$29+$D$31","v":{"$error":"#VALUE!"}},{"$f":"J123*L123","v":{"$error":"#DIV/0!"}},{"$f":"K123*M123","v":{"$error":"#DIV/0!"}}]
[{"$f":"A123+1","v":2},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A124,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A124,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A124,3,1,1)","v":0},{"$f":"IF(D124=\"Default\",VLOOKUP(B124,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B124,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D124=\"Default\",LN(VLOOKUP(B124,'Original Excipient EFs'!A4:R49,18,FALSE))^2,IF(D124=\"User Defined\",VLOOKUP(B124,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[3,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A125,0,1,1)","v":1},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A125,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A125,3,1,1)","v":0},{"$f":"IF(D125=\"Default\",VLOOKUP(B125,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B125,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D125=\"Default\",LN(VLOOKUP(B125,'Original Excipient EFs'!A5:R50,18,FALSE))^2,IF(D125=\"User Defined\",VLOOKUP(B125,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[4,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A126,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A126,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A126,3,1,1)","v":0},{"$f":"IF(D126=\"Default\",VLOOKUP(B126,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B126,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D126=\"Default\",LN(VLOOKUP(B126,'Original Excipient EFs'!A6:R51,18,FALSE))^2,IF(D126=\"User Defined\",VLOOKUP(B126,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[{"$f":"A126+1","v":5},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A127,0,1,1)","v":"Site 1"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A127,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A127,3,1,1)","v":0},{"$f":"IF(D127=\"Default\",VLOOKUP(B127,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B127,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D127=\"Default\",LN(VLOOKUP(B127,'Original Excipient EFs'!A7:R52,18,FALSE))^2,IF(D127=\"User Defined\",VLOOKUP(B127,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[{"$f":"A127+1","v":6},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A128,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A128,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A128,3,1,1)","v":0},{"$f":"IF(D128=\"Default\",VLOOKUP(B128,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B128,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D128=\"Default\",LN(VLOOKUP(B128,'Original Excipient EFs'!A8:R53,18,FALSE))^2,IF(D128=\"User Defined\",VLOOKUP(B128,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[{"$f":"A128+1","v":7},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A129,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A129,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A129,3,1,1)","v":0},{"$f":"IF(D129=\"Default\",VLOOKUP(B129,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B129,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D129=\"Default\",LN(VLOOKUP(B129,'Original Excipient EFs'!A9:R54,18,FALSE))^2,IF(D129=\"User Defined\",VLOOKUP(B129,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[8,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A130,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A130,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A130,3,1,1)","v":0},{"$f":"IF(D130=\"Default\",VLOOKUP(B130,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B130,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D130=\"Default\",LN(VLOOKUP(B130,'Original Excipient EFs'!A10:R55,18,FALSE))^2,IF(D130=\"User Defined\",VLOOKUP(B130,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[{"$f":"A130+1","v":9},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A131,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A131,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A131,3,1,1)","v":0},{"$f":"IF(D131=\"Default\",VLOOKUP(B131,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B131,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D131=\"Default\",LN(VLOOKUP(B131,'Original Excipient EFs'!A11:R56,18,FALSE))^2,IF(D131=\"User Defined\",VLOOKUP(B131,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[10,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A132,0,1,1)","v":0.02},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A132,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A132,3,1,1)","v":0},{"$f":"IF(D132=\"Default\",VLOOKUP(B132,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B132,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D132=\"Default\",LN(VLOOKUP(B132,'Original Excipient EFs'!A12:R57,18,FALSE))^2,IF(D132=\"User Defined\",VLOOKUP(B132,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[11,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A133,0,1,1)","v":"Default"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A133,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A133,3,1,1)","v":0},{"$f":"IF(D133=\"Default\",VLOOKUP(B133,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B133,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D133=\"Default\",LN(VLOOKUP(B133,'Original Excipient EFs'!A13:R58,18,FALSE))^2,IF(D133=\"User Defined\",VLOOKUP(B133,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[12,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A134,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A134,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A134,3,1,1)","v":0},{"$f":"IF(D134=\"Default\",VLOOKUP(B134,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B134,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D134=\"Default\",LN(VLOOKUP(B134,'Original Excipient EFs'!A14:R59,18,FALSE))^2,IF(D134=\"User Defined\",VLOOKUP(B134,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A135,0,1,1)","v":1},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A135,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A135,3,1,1)","v":0},{"$f":"IF(D135=\"Default\",VLOOKUP(B135,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B135,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D135=\"Default\",LN(VLOOKUP(B135,'Original Excipient EFs'!A15:R60,18,FALSE))^2,IF(D135=\"User Defined\",VLOOKUP(B135,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[14,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A136,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A136,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A136,3,1,1)","v":0},{"$f":"IF(D136=\"Default\",VLOOKUP(B136,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B136,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D136=\"Default\",LN(VLOOKUP(B136,'Original Excipient EFs'!A16:R61,18,FALSE))^2,IF(D136=\"User Defined\",VLOOKUP(B136,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A137,0,1,1)","v":"Site 1"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A137,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A137,3,1,1)","v":0},{"$f":"IF(D137=\"Default\",VLOOKUP(B137,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B137,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D137=\"Default\",LN(VLOOKUP(B137,'Original Excipient EFs'!A17:R62,18,FALSE))^2,IF(D137=\"User Defined\",VLOOKUP(B137,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[16,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A138,0,1,1)","v":"Ingredient"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A138,2,1,1)","v":"Air"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A138,3,1,1)","v":"Sea"},{"$f":"IF(D138=\"Default\",VLOOKUP(B138,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B138,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D138=\"Default\",LN(VLOOKUP(B138,'Original Excipient EFs'!A18:R63,18,FALSE))^2,IF(D138=\"User Defined\",VLOOKUP(B138,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[17,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A139,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A139,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A139,3,1,1)","v":0},{"$f":"IF(D139=\"Default\",VLOOKUP(B139,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B139,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D139=\"Default\",LN(VLOOKUP(B139,'Original Excipient EFs'!A19:R64,18,FALSE))^2,IF(D139=\"User Defined\",VLOOKUP(B139,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[18,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A140,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A140,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A140,3,1,1)","v":0},{"$f":"IF(D140=\"Default\",VLOOKUP(B140,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B140,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D140=\"Default\",LN(VLOOKUP(B140,'Original Excipient EFs'!A20:R65,18,FALSE))^2,IF(D140=\"User Defined\",VLOOKUP(B140,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[19,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A141,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A141,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A141,3,1,1)","v":0},{"$f":"IF(D141=\"Default\",VLOOKUP(B141,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B141,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D141=\"Default\",LN(VLOOKUP(B141,'Original Excipient EFs'!A21:R66,18,FALSE))^2,IF(D141=\"User Defined\",VLOOKUP(B141,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[20,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A142,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A142,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A142,3,1,1)","v":0},{"$f":"IF(D142=\"Default\",VLOOKUP(B142,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B142,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D142=\"Default\",LN(VLOOKUP(B142,'Original Excipient EFs'!A22:R67,18,FALSE))^2,IF(D142=\"User Defined\",VLOOKUP(B142,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[21,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A143,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A143,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A143,3,1,1)","v":0},{"$f":"IF(D143=\"Default\",VLOOKUP(B143,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B143,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D143=\"Default\",LN(VLOOKUP(B143,'Original Excipient EFs'!A23:R68,18,FALSE))^2,IF(D143=\"User Defined\",VLOOKUP(B143,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[22,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A144,0,1,1)","v":"Site 2"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A144,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A144,3,1,1)","v":0},{"$f":"IF(D144=\"Default\",VLOOKUP(B144,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B144,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D144=\"Default\",LN(VLOOKUP(B144,'Original Excipient EFs'!A24:R69,18,FALSE))^2,IF(D144=\"User Defined\",VLOOKUP(B144,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[{"$f":"A144+1","v":23},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A145,0,1,1)","v":"Ingredient"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A145,2,1,1)","v":"Air"},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A145,3,1,1)","v":"Sea"},{"$f":"IF(D145=\"Default\",VLOOKUP(B145,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B145,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D145=\"Default\",LN(VLOOKUP(B145,'Original Excipient EFs'!A25:R70,18,FALSE))^2,IF(D145=\"User Defined\",VLOOKUP(B145,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[24,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A146,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A146,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A146,3,1,1)","v":0},{"$f":"IF(D146=\"Default\",VLOOKUP(B146,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B146,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D146=\"Default\",LN(VLOOKUP(B146,'Original Excipient EFs'!A26:R71,18,FALSE))^2,IF(D146=\"User Defined\",VLOOKUP(B146,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[25,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A147,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A147,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A147,3,1,1)","v":0},{"$f":"IF(D147=\"Default\",VLOOKUP(B147,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B147,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D147=\"Default\",LN(VLOOKUP(B147,'Original Excipient EFs'!A27:R72,18,FALSE))^2,IF(D147=\"User Defined\",VLOOKUP(B147,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[26,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A148,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A148,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A148,3,1,1)","v":0},{"$f":"IF(D148=\"Default\",VLOOKUP(B148,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B148,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D148=\"Default\",LN(VLOOKUP(B148,'Original Excipient EFs'!A28:R73,18,FALSE))^2,IF(D148=\"User Defined\",VLOOKUP(B148,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[{"$f":"A148+1","v":27},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A149,0,1,1)","v":""},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A149,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A149,3,1,1)","v":0},{"$f":"IF(D149=\"Default\",VLOOKUP(B149,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B149,'Original Excipient EFs'!A:C,3,FALSE))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D149=\"Default\",LN(VLOOKUP(B149,'Original Excipient EFs'!A29:R74,18,FALSE))^2,IF(D149=\"User Defined\",VLOOKUP(B149,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#N/A"}]
[28,{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A150,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A150,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A150,3,1,1)","v":0},{"$f":"IF(D150=\"Default\",VLOOKUP(B150,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B150,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D150=\"Default\",LN(VLOOKUP(B150,'Original Excipient EFs'!A30:R75,18,FALSE))^2,IF(D150=\"User Defined\",VLOOKUP(B150,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[{"$f":"A150+1","v":29},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A151,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A151,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A151,3,1,1)","v":0},{"$f":"IF(D151=\"Default\",VLOOKUP(B151,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B151,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D151=\"Default\",LN(VLOOKUP(B151,'Original Excipient EFs'!A31:R76,18,FALSE))^2,IF(D151=\"User Defined\",VLOOKUP(B151,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[{"$f":"A151+1","v":30},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A152,0,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A152,2,1,1)","v":0},{"$f":"OFFSET(ExcipientStart,'Calculation sheet'!$A152,3,1,1)","v":0},{"$f":"IF(D152=\"Default\",VLOOKUP(B152,'Original Excipient EFs'!A:C,2,FALSE),VLOOKUP(B152,'Original Excipient EFs'!A:C,3,FALSE))","v":false},0,0,{"$f":"LN('Data Quality Matrix'!$N$45)^2","v":0},{"$f":"IF(D152=\"Default\",LN(VLOOKUP(B152,'Original Excipient EFs'!A32:R77,18,FALSE))^2,IF(D152=\"User Defined\",VLOOKUP(B152,'User Defined Excipient EFs'!A:J,9,FALSE),\"\"))","v":""},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
[]
[]
["PACKAGING"]
[]
["PACKAGING SUMMARY:"]
[]
["NEED FORMULAE THAT VARIES DEPENDING ON WHETHER IT IS SPECIFIED OR DEFAULT"]
[]
["Total Packaging (including uplift) (mg CO2e per tablet):",{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",$B$205,IF(PackagingCalculationMethod=\"Use Defaults\",$B$171,\"\"))","v":""}]
["Σ Si2 x (ln Ui)2",{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",$B$206,IF(PackagingCalculationMethod=\"Use Defaults\",$B$172,\"\"))","v":""}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B163*$B$38","v":{"$error":"#VALUE!"}}]
[]
["Default Packaging:"]
[]
["Default Summary:"]
[]
["Emissions (mg CO2e per tablet):",{"$f":"IF(WasteDefault=\"Small\",SUM($D$177:$D$181),IF(WasteDefault=\"Medium\",SUM($D$186:$D$190),IF(WasteDefault=\"Large\",SUM($D$195:$D$199),\"\")))","v":11019.916274201991}]
["Σ Si2 x (ln Ui)2",{"$f":"IF(WasteDefault=\"Small\",SUM($I$177:$I$181),IF(WasteDefault=\"Medium\",SUM($I$186:$I$190),IF(WasteDefault=\"Large\",SUM($I$195:$I$199),\"\")))","v":1.4451053482287444}]
[]
[{"$f":"'Reference Data'!A38","v":"Small:"}]
[]
[{"$f":"'Reference Data'!A40","v":"Material"},{"$f":"'Reference Data'!E40","v":"Total weight per tablet (mg)"},"Emission Factor (kg CO2e/kg material)","Emissions including wastage (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"'Reference Data'!A42","v":"PVC - blister"},{"$f":"'Reference Data'!E42","v":1486},{"$f":"VLOOKUP(A177,'Packaging EFs'!A:C,3,FALSE)","v":1.9},{"$f":"IFERROR(B177*C177*$B$30*$B$31,\"\")","v":2954.8927263212981},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D177/$B$171)^2","v":7.1899661901651216E-2},{"$f":"E177+F177+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G177*H177,\"\")","v":0.25746661880661909}]
[{"$f":"'Reference Data'!A43","v":"PVdC - blister"},{"$f":"'Reference Data'!E43","v":178},{"$f":"VLOOKUP(A178,'Packaging EFs'!A:C,3,FALSE)","v":4.4000000000000004},{"$f":"IFERROR(B178*C178*$B$30*$B$31,\"\")","v":819.6755625327055},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D178/$B$171)^2","v":5.5325759560138996E-3},{"$f":"E178+F178+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G178*H178,\"\")","v":1.9811687385041563E-2}]
[{"$f":"'Reference Data'!A44","v":"Aluminium"},{"$f":"'Reference Data'!E44","v":239},{"$f":"VLOOKUP(A179,'Packaging EFs'!A:C,3,FALSE)","v":12.79},{"$f":"IFERROR(B179*C179*$B$30*$B$31,\"\")","v":3199.1732077446368},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D179/$B$171)^2","v":8.4278911579950974E-2},{"$f":"E179+F179+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G179*H179,\"\")","v":0.30179566672890934}]
[{"$f":"'Reference Data'!A45","v":"Paper"},{"$f":"'Reference Data'!E45","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A180,'Packaging EFs'!A:C,3,FALSE)","v":0.69},{"$f":"IFERROR(B180*C180*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D180/$B$171)^2","v":{"$error":"#VALUE!"}},{"$f":"E180+F180+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G180*H180,\"\")","v":""}]
[{"$f":"'Reference Data'!A46","v":"Cardboard"},{"$f":"'Reference Data'!E46","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A181,'Packaging EFs'!A:C,3,FALSE)","v":0.58225000000000005},{"$f":"IFERROR(B181*C181*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D181/$B$171)^2","v":{"$error":"#VALUE!"}},{"$f":"E181+F181+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G181*H181,\"\")","v":""}]
[]
[{"$f":"'Reference Data'!A48","v":"Medium:"}]
[]
[{"$f":"'Reference Data'!A50","v":"Material"},{"$f":"'Reference Data'!E50","v":"Total weight per tablet (mg)"},"Emission Factor (kg CO2e/kg material)","Emissions including wastage (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"'Reference Data'!A52","v":"PVC - blister"},{"$f":"'Reference Data'!E52","v":2351},{"$f":"VLOOKUP(A186,'Packaging EFs'!A:C,3,FALSE)","v":1.9},{"$f":"IFERROR(B186*C186*$B$30*$B$31,\"\")","v":4674.9345892203037},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D186/$B$171)^2","v":0.17996766734586442},{"$f":"E186+F186+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G186*H186,\"\")","v":0.64444902215861433}]
[{"$f":"'Reference Data'!A53","v":"PVdC - blister"},{"$f":"'Reference Data'!E53","v":282},{"$f":"VLOOKUP(A187,'Packaging EFs'!A:C,3,FALSE)","v":4.4000000000000004},{"$f":"IFERROR(B187*C187*$B$30*$B$31,\"\")","v":1298.5871271585561},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D187/$B$171)^2","v":1.3886269736335359E-2},{"$f":"E187+F187+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G187*H187,\"\")","v":4.9725559512941726E-2}]
[{"$f":"'Reference Data'!A54","v":"Aluminium"},{"$f":"'Reference Data'!E54","v":377},{"$f":"VLOOKUP(A188,'Packaging EFs'!A:C,3,FALSE)","v":12.79},{"$f":"IFERROR(B188*C188*$B$30*$B$31,\"\")","v":5046.3945578231296},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D188/$B$171)^2","v":0.20970356653326888},{"$f":"E188+F188+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G188*H188,\"\")","v":0.75093076655718838}]
[{"$f":"'Reference Data'!A55","v":"Paper"},{"$f":"'Reference Data'!E55","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A189,'Packaging EFs'!A:C,3,FALSE)","v":0.69},{"$f":"IFERROR(B189*C189*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D189/$B$171)^2","v":{"$error":"#VALUE!"}},{"$f":"E189+F189+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G189*H189,\"\")","v":""}]
[{"$f":"'Reference Data'!A56","v":"Cardboard"},{"$f":"'Reference Data'!E56","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A190,'Packaging EFs'!A:C,3,FALSE)","v":0.58225000000000005},{"$f":"IFERROR(B190*C190*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D190/$B$171)^2","v":{"$error":"#VALUE!"}},{"$f":"E190+F190+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G190*H190,\"\")","v":""}]
[]
[{"$f":"'Reference Data'!A58","v":"Large:"}]
[]
[{"$f":"'Reference Data'!A60","v":"Material"},{"$f":"'Reference Data'!E60","v":"Total weight per tablet (mg)"},"Emission Factor (kg CO2e/kg material)","Emissions including wastage (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"'Reference Data'!A62","v":"PVC - blister"},{"$f":"'Reference Data'!E62","v":3634},{"$f":"VLOOKUP(A195,'Packaging EFs'!A:C,3,FALSE)","v":1.9},{"$f":"IFERROR(B195*C195*$B$30*$B$31,\"\")","v":7226.1643118785987},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D195/$B$171)^2","v":0.42999071254910448},{"$f":"E195+F195+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G195*H195,\"\")","v":1.5397604376735508}]
[{"$f":"'Reference Data'!A63","v":"PVdC - blister"},{"$f":"'Reference Data'!E63","v":436},{"$f":"VLOOKUP(A196,'Packaging EFs'!A:C,3,FALSE)","v":4.4000000000000004},{"$f":"IFERROR(B196*C196*$B$30*$B$31,\"\")","v":2007.7446363160652},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D196/$B$171)^2","v":3.319405879732415E-2},{"$f":"E196+F196+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G196*H196,\"\")","v":0.11886512199049555}]
[{"$f":"'Reference Data'!A64","v":"Aluminium"},{"$f":"'Reference Data'!E64","v":583},{"$f":"VLOOKUP(A197,'Packaging EFs'!A:C,3,FALSE)","v":12.79},{"$f":"IFERROR(B197*C197*$B$30*$B$31,\"\")","v":7803.8409209837791},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D197/$B$171)^2","v":0.50148763113387296},{"$f":"E197+F197+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G197*H197,\"\")","v":1.7957848666658895}]
[{"$f":"'Reference Data'!A65","v":"Paper"},{"$f":"'Reference Data'!E65","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A198,'Packaging EFs'!A:C,3,FALSE)","v":0.69},{"$f":"IFERROR(B198*C198*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D198/$B$171)^2","v":{"$error":"#VALUE!"}},{"$f":"E198+F198+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G198*H198,\"\")","v":""}]
[{"$f":"'Reference Data'!A66","v":"Cardboard"},{"$f":"'Reference Data'!E66","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A199,'Packaging EFs'!A:C,3,FALSE)","v":0.58225000000000005},{"$f":"IFERROR(B199*C199*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$43)^2","v":0.21819164483328232},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D199/$B$171)^2","v":{"$error":"#VALUE!"}},{"$f":"E199+F199+$C$30+$C$31","v":3.5809155703513289},{"$f":"IFERROR(G199*H199,\"\")","v":""}]
[]
["Specified Packaging:"]
[]
["Specified Summary:"]
[]
["Emissions (mg CO2e per tablet):",{"$f":"SUM(D211:D214,D219:D221,D226:D227)","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(I211:I214,I219:I221,I226:I227)","v":0}]
[]
["Blister Pack Emissions per tablet"]
[]
["Material","Weight (mg per tablet)","Emission Factor (kg CO2e/kg material)","Emissions including wastage (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"'Data Input'!G109","v":0},{"$f":"('Data Input'!H109*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A211,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B211*C211*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D211/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E211+F211+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G211*H211,\"\")","v":""}]
[{"$f":"'Data Input'!G110","v":0},{"$f":"('Data Input'!H110*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A212,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B212*C212*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D212/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E212+F212+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G212*H212,\"\")","v":""}]
[{"$f":"'Data Input'!G111","v":0},{"$f":"('Data Input'!H111*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A213,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B213*C213*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D213/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E213+F213+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G213*H213,\"\")","v":""}]
[{"$f":"'Data Input'!G112","v":0},{"$f":"('Data Input'!H112*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A214,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B214*C214*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D214/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E214+F214+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G214*H214,\"\")","v":""}]
[]
["Retail Pack emissions per tablet"]
[]
["Material","Weight (mg per tablet)","Emission Factor (kg CO2e/kg material)","Emissions including wastage (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"'Data Input'!G114","v":0},{"$f":"'Data Input'!H114*1000/(BlistersPerRetail*TabletsPerPack)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A219,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B219*C219*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D219/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E219+F219+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G219*H219,\"\")","v":""}]
[{"$f":"'Data Input'!G115","v":0},{"$f":"'Data Input'!H115*1000/(BlistersPerRetail*TabletsPerPack)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A220,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B220*C220*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D220/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E220+F220+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G220*H220,\"\")","v":""}]
[{"$f":"'Data Input'!G116","v":0},{"$f":"'Data Input'!H116*1000/(BlistersPerRetail*TabletsPerPack)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A221,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B221*C221*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D221/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E221+F221+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G221*H221,\"\")","v":""}]
[]
["Outer Box emissions per tablet"]
[]
["Material","Weight (mg per tablet)","Emission Factor (kg CO2e/kg material)","Emissions including wastage (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"'Data Input'!G118","v":0},{"$f":"('Data Input'!H118*1000)/(RetailsPerOuter*BlistersPerRetail*TabletsPerPack)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A226,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B226*C226*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D226/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E226+F226+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G226*H226,\"\")","v":""}]
[{"$f":"'Data Input'!G119","v":0},{"$f":"('Data Input'!H119*1000)/(RetailsPerOuter*BlistersPerRetail*TabletsPerPack)","v":{"$error":"#DIV/0!"}},{"$f":"VLOOKUP(A227,'Packaging EFs'!A:C,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(B227*C227*$B$30*$B$31,\"\")","v":""},{"$f":"LN('Data Quality Matrix'!$N$44)^2","v":0},{"$f":"LN('Data Quality Matrix'!$N$30)^2","v":8.2707770876915582E-2},{"$f":"(D227/$B$205)^2","v":{"$error":"#VALUE!"}},{"$f":"E227+F227+$C$30+$C$31","v":3.3627239255180461},{"$f":"IFERROR(G227*H227,\"\")","v":""}]
[]
[]
[]
[]
["FORMULATION EMISSIONS"]
["NEED TO CHECK WHETHER ELECTRICIY EMISSION FACTORS ALREADY INCLUDE EFFECT OF WASTAGE?"]
["Formulation Summary:"]
[]
["Total emissions (mg CO2e per tablet):",{"$f":"C245+C250+IF(FormulationNumber=1,0,C259+C264)","v":{"$error":"#N/A"}}]
["Σ Si2 x (ln Ui)2",{"$f":"H245+H250+IF(FormulationNumber=1,0,H259+H264)","v":{"$error":"#N/A"}}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B252+IF(FormulationNumber=1,0,B266)","v":{"$error":"#N/A"}}]
[]
["Formulation Site 1"]
[]
["Electricity"]
[]
["Electricity Use (kWh per tablet)","Electricity emission factor (kg CO2(e)/kWh)","Emissions (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"('Reference Data'!$B$22*'Calculation sheet'!$B$9)/1000000","v":0},{"$f":"VLOOKUP(FormSite1Country,ElectricityFactors,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"B245*A245*$B$27*$B$29*$B$31*1000000","v":{"$error":"#N/A"}},{"$f":"LN('Data Quality Matrix'!$N$40)^2","v":8.0327290757235409E-2},{"$f":"LN('Data Quality Matrix'!$N$31)^2","v":1.1464510494012894E-2},{"$f":"(C245/$B$236)^2","v":{"$error":"#N/A"}},{"$f":"D245+E245+$D$27+$D$29+$D$31","v":0.82597953520245104},{"$f":"F245*G245","v":{"$error":"#N/A"}}]
[]
["Gas"]
[]
["Gas Use (kWh per tablet)","Gas emission factor (kg CO2(e)/kWh)","Emissions (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"('Reference Data'!$B$23*'Calculation sheet'!$B$9)/1000000","v":0},{"$f":"VLOOKUP(VLOOKUP(FormSite1Country,'Typical heat sources'!A:D,4,FALSE),FuelReferenceDatabase,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"B250*A250*$B$27*$B$29*$B$31*1000000","v":{"$error":"#N/A"}},{"$f":"LN('Data Quality Matrix'!$N$41)^2","v":8.0327290757235409E-2},{"$f":"LN('Data Quality Matrix'!$N$32)^2","v":2.0940684916177059E-2},{"$f":"(C250/$B$236)^2","v":{"$error":"#N/A"}},{"$f":"D250+E250+$D$27+$D$29+$D$31","v":0.83545570962461513},{"$f":"F250*G250","v":{"$error":"#N/A"}}]
[]
["Effect of waste (mg CO2e per tablet):",{"$f":"(C245+C250)*$B$39","v":{"$error":"#N/A"}}]
[]
["Formulation Site 2"]
[]
["Electricity"]
[]
["Electricity Use (kWh per tablet)","Electricity emission factor (kg CO2(e)/kWh)","Emissions (mg CO2e per tablet)","(ln UA)2","(ln(UEF))2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"('Reference Data'!$B$22*$B$12)/1000000","v":0},{"$f":"VLOOKUP(FormSite2Country,ElectricityFactors,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"B259*A259*$B$27*$B$29*$B$31*1000000","v":{"$error":"#N/A"}},{"$f":"LN('Data Quality Matrix'!$N$40)^2","v":8.0327290757235409E-2},{"$f":"LN('Data Quality Matrix'!$N$31)^2","v":1.1464510494012894E-2},{"$f":"(C259/$B$236)^2","v":{"$error":"#N/A"}},{"$f":"D259+E259+$D$27+$D$29+$D$31","v":0.82597953520245104},{"$f":"F259*G259","v":{"$error":"#N/A"}}]
[]
["Gas"]
[]
["Gas Use (kWh per tablet)","Gas emission factor (kg CO2(e)/kWh)","Emissions (mg CO2e per tablet)","(ln UA)2","(ln(UEF))2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"('Reference Data'!$B$23*$B$12)/1000000","v":0},{"$f":"VLOOKUP(VLOOKUP(FormSite2Country,'Typical heat sources'!A:D,4,FALSE),FuelReferenceDatabase,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"B264*A264*$B$27*$B$29*$B$31*1000000","v":{"$error":"#N/A"}},{"$f":"LN('Data Quality Matrix'!$N$41)^2","v":8.0327290757235409E-2},{"$f":"LN('Data Quality Matrix'!$N$32)^2","v":2.0940684916177059E-2},{"$f":"(C264/$B$236)^2","v":{"$error":"#N/A"}},{"$f":"D264+E264+$D$27+$D$29+$D$31","v":0.83545570962461513},{"$f":"F264*G264","v":{"$error":"#N/A"}}]
[]
["Effect of waste (mg CO2e per tablet):",{"$f":"(C259+C264)*$B$40","v":{"$error":"#N/A"}}]
[]
["PACKAGING PROCESS EMISSIONS"]
["Packaging Process Summary:"]
[]
["Total emissions (mg CO2e per tablet):",{"$f":"C278+C283","v":{"$error":"#N/A"}}]
["Σ Si2 x (ln Ui)2",{"$f":"H278+H283","v":{"$error":"#N/A"}}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B285","v":{"$error":"#N/A"}}]
[]
["Electricity"]
[]
["Electricity Use (kWh per tablet)","Electricity emission factor (kg CO2(e)/kWh)","Emissions (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"('Reference Data'!$B$27*'Calculation sheet'!$B$9)/1000000","v":0},{"$f":"VLOOKUP(PackagingCountry,ElectricityFactors,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"B278*A278*$B$27*$B$29*$B$31*1000000","v":{"$error":"#N/A"}},{"$f":"LN('Data Quality Matrix'!$N$40)^2","v":8.0327290757235409E-2},{"$f":"LN('Data Quality Matrix'!$N$31)^2","v":1.1464510494012894E-2},{"$f":"(C278/$B$271)^2","v":{"$error":"#N/A"}},{"$f":"D278+E278+$D$27+$D$29+$D$31","v":0.82597953520245104},{"$f":"F278*G278","v":{"$error":"#N/A"}}]
[]
["Gas"]
[]
["Gas Use (kWh per tablet)","Gas emission factor (kg CO2(e)/kWh)","Emissions (mg CO2e per tablet)","(ln UA)2","(ln UEF)2","S2","(ln UE)2","S2 x (ln UE)2"]
[{"$f":"('Reference Data'!$B$28*'Calculation sheet'!$B$9)/1000000","v":0},{"$f":"VLOOKUP(VLOOKUP(PackagingCountry,'Typical heat sources'!A:D,4,FALSE),FuelReferenceDatabase,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"B283*A283*$B$27*$B$29*$B$31*1000000","v":{"$error":"#N/A"}},{"$f":"LN('Data Quality Matrix'!$N$41)^2","v":8.0327290757235409E-2},{"$f":"LN('Data Quality Matrix'!$N$32)^2","v":2.0940684916177059E-2},{"$f":"(C283/$B$271)^2","v":{"$error":"#N/A"}},{"$f":"D283+E283+$D$27+$D$29+$D$31","v":0.83545570962461513},{"$f":"F283*G283","v":{"$error":"#N/A"}}]
[]
["Effect of waste (mg CO2e per tablet):",{"$f":"(C278+C283)*$B$39","v":{"$error":"#N/A"}}]
[]
["TRANSPORT EMISSIONS"]
[]
[]
["APIs - TRANSPORT TO FORMULATION SITES"]
[]
["Formulation site 1"]
[]
[null,"Weight (mg)","Emissions per tablet (mg CO2e)",null,null,"S2"]
[null,null,"Air","Sea","Road","Air","Sea","Road"]
["API1",{"$f":"API1Site1Weight*$B$27*$B$29*$B$31","v":0},{"$f":"IF(ISERROR($B296*VLOOKUP('Data Input'!I73,Air_EF,2,FALSE)),0,$B296*VLOOKUP('Data Input'!I73,Air_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B296*VLOOKUP('Data Input'!J73,Sea_EF,2,FALSE)),0,$B296*VLOOKUP('Data Input'!J73,Sea_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B296*VLOOKUP('Data Input'!K73,Road_EF,2,FALSE)),0,$B296*VLOOKUP('Data Input'!K73,Road_EF,2,FALSE))","v":0},{"$f":"IFERROR((C296/$B$305)^2,0)","v":0},{"$f":"IFERROR((D296/$B$305)^2,0)","v":0},0]
["API2",{"$f":"API2Site1Weight*$B$27*$B$29*$B$31","v":0},{"$f":"IF(ISERROR($B297*VLOOKUP('Data Input'!I74,Air_EF,2,FALSE)),0,$B297*VLOOKUP('Data Input'!I74,Air_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B297*VLOOKUP('Data Input'!J74,Sea_EF,2,FALSE)),0,$B297*VLOOKUP('Data Input'!J74,Sea_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B297*VLOOKUP('Data Input'!K74,Road_EF,2,FALSE)),0,$B297*VLOOKUP('Data Input'!K74,Road_EF,2,FALSE))","v":0},{"$f":"IFERROR((C297/$B$305)^2,0)","v":0},0,0]
["API3",{"$f":"API3Site1Weight*$B$27*$B$29*$B$31","v":0},{"$f":"IF(ISERROR($B298*VLOOKUP('Data Input'!I75,Air_EF,2,FALSE)),0,$B298*VLOOKUP('Data Input'!I75,Air_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B298*VLOOKUP('Data Input'!J75,Sea_EF,2,FALSE)),0,$B298*VLOOKUP('Data Input'!J75,Sea_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B298*VLOOKUP('Data Input'!K75,Road_EF,2,FALSE)),0,$B298*VLOOKUP('Data Input'!K75,Road_EF,2,FALSE))","v":0},0,0,0]
[]
[null,"(ln UE)2","Σ(S2 x (ln UE)2)"]
["Air",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"B301*SUM(OFFSET(F296,0,0,APINumber,1))","v":0}]
["Sea",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"B302*SUM(OFFSET(G296,0,0,APINumber,1))","v":0}]
["Road",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"B303*SUM(OFFSET(H296,0,0,APINumber,1))","v":0}]
[]
["Total Emissions (mg CO2e per tablet):",{"$f":"SUM(OFFSET(C296,0,0,APINumber,3))","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(C301:C303)","v":0}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B305*$B$39","v":0}]
[]
[]
["Formulation site 2"]
[]
[null,"Weight (mg)","Emissions per tablet (mg CO2e)",null,null,"S2"]
[null,null,"Air","Sea","Road","Air","Sea","Road"]
["API1",{"$f":"API1Site2Weight*$B$28*$B$29*$B$31","v":0},{"$f":"IF(ISERROR($B314*VLOOKUP('Data Input'!I80,Air_EF,2,FALSE)),0,$B314*VLOOKUP('Data Input'!I80,Air_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B314*VLOOKUP('Data Input'!J80,Sea_EF,2,FALSE)),0,$B314*VLOOKUP('Data Input'!J80,Sea_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B314*VLOOKUP('Data Input'!K80,Road_EF,2,FALSE)),0,$B314*VLOOKUP('Data Input'!K80,Road_EF,2,FALSE))","v":0},{"$f":"IFERROR((C314/$B$323)^2,0)","v":0},{"$f":"IFERROR((D314/$B$323)^2,0)","v":0},0]
["API2",{"$f":"API2Site2Weight*$B$28*$B$29*$B$31","v":0},{"$f":"IF(ISERROR($B315*VLOOKUP('Data Input'!I81,Air_EF,2,FALSE)),0,$B315*VLOOKUP('Data Input'!I81,Air_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B315*VLOOKUP('Data Input'!J81,Sea_EF,2,FALSE)),0,$B315*VLOOKUP('Data Input'!J81,Sea_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B315*VLOOKUP('Data Input'!K81,Road_EF,2,FALSE)),0,$B315*VLOOKUP('Data Input'!K81,Road_EF,2,FALSE))","v":0},{"$f":"IFERROR((C315/$B$323)^2,0)","v":0},0,0]
["API3",{"$f":"API3Site2Weight*$B$28*$B$29*$B$31","v":0},{"$f":"IF(ISERROR($B316*VLOOKUP('Data Input'!I82,Air_EF,2,FALSE)),0,$B316*VLOOKUP('Data Input'!I82,Air_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B316*VLOOKUP('Data Input'!J82,Sea_EF,2,FALSE)),0,$B316*VLOOKUP('Data Input'!J82,Sea_EF,2,FALSE))","v":0},{"$f":"IF(ISERROR($B316*VLOOKUP('Data Input'!K82,Road_EF,2,FALSE)),0,$B316*VLOOKUP('Data Input'!K82,Road_EF,2,FALSE))","v":0},0,0,0]
[]
[null,"(ln UE)2","Σ(S2 x (ln UE)2)"]
["Air",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"B319*SUM(OFFSET(F314,0,0,APINumber,1))","v":0}]
["Sea",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"B320*SUM(OFFSET(G314,0,0,APINumber,1))","v":0}]
["Road",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"B321*SUM(OFFSET(H314,0,0,APINumber,1))","v":0}]
[]
["Total Emissions (mg CO2e per tablet):",{"$f":"SUM(OFFSET(C314,0,0,APINumber,3))","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(C319:C321)","v":0}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B323*$B$40","v":0}]
[]
[]
["EXCIPIENTS - TRANSPORT TO FORMULATION SITES"]
[]
["Formulation site 1"]
[]
["Uplift due to wastage:",{"$f":"$B$27*$B$29*$B$31","v":1.0464651453854026}]
[]
[null,null,"Emission Factor (UNITS)","Emissions  per tablet (mg CO2e)","S2","(ln UE)2","S2 x (ln UE)2"]
["Air","Long Haul",{"$f":"SUMPRODUCT((Transport_EF_Mode=(A335&\" EF\"))*(Transport_EF_Type=B335)*Transport_EF_Value)","v":0.74448000000000003},{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,2,ExcipientNumber,1)=B335)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C335*$B$332)","v":0},{"$f":"(D335/$B$344)^2","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"F335*E335","v":{"$error":"#DIV/0!"}}]
["Air","Short Haul",3.518173640552996,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,2,ExcipientNumber,1)=B336)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C336*$B$332)","v":0},{"$f":"(D336/$B$344)^2","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$f":"F336*E336","v":{"$error":"#DIV/0!"}}]
["Air","Domestic",7.2800000000000017E-2,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,2,ExcipientNumber,1)=B337)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C337*$B$332)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Sea","Long haul",9.4162354838709661E-2,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,3,ExcipientNumber,1)=B338)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C338*$B$332)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Sea","Short haul",3.380187096774193E-3,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,3,ExcipientNumber,1)=B339)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C339*$B$332)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Road","Long haul",0.60209424083769636,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,4,ExcipientNumber,1)=B340)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C340*$B$332)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Road","Short haul",0.12041884816753928,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,4,ExcipientNumber,1)=B341)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C341*$B$332)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Road","Domestic",2.4083769633507855E-2,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport1,0,4,ExcipientNumber,1)=B342)*(OFFSET(Excipient1Site1Weight,0,0,ExcipientNumber,1))*C342*$B$332)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$27+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
[]
["Total (including wastage uplifts):",{"$f":"SUM(D335:D342)","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(G335:G342)","v":{"$error":"#DIV/0!"}}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B344*$B$39","v":0}]
[]
["Formulation site 2"]
[]
["Uplift due to wastage:",{"$f":"$B$28*$B$29*$B$31","v":1.0464651453854026}]
[]
[null,null,"Emission Factor (UNITS)","Emissions  per tablet (mg CO2e)","S2","(ln UE)2","S2 x (ln UE)2"]
["Air","Long Haul",{"$f":"SUMPRODUCT((Transport_EF_Mode=(A353&\" EF\"))*(Transport_EF_Type=B353)*Transport_EF_Value)","v":0.74448000000000003},{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,2,ExcipientNumber,1)=B353)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C353*$B$350)","v":0},{"$f":"(D353/$B$363)^2","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$f":"F353*E353","v":{"$error":"#DIV/0!"}}]
["Air","Short Haul",3.518173640552996,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,2,ExcipientNumber,1)=B354)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C354*$B$350)","v":0},{"$f":"(D354/$B$363)^2","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$f":"F354*E354","v":{"$error":"#DIV/0!"}}]
["Air","Domestic",7.2800000000000017E-2,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,2,ExcipientNumber,1)=B355)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C355*$B$350)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Sea","Long haul",9.4162354838709661E-2,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,3,ExcipientNumber,1)=B356)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C356*$B$350)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Sea","Medium haul",{"$f":"SUMPRODUCT((Transport_EF_Mode=(A357&\" EF\"))*(Transport_EF_Type=B357)*Transport_EF_Value)","v":3.8630709677419349E-2},{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,3,ExcipientNumber,1)=B357)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C357*$B$350)","v":0},{"$f":"(D357/$B$363)^2","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$f":"F357*E357","v":{"$error":"#DIV/0!"}}]
["Sea","Short haul",3.380187096774193E-3,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,3,ExcipientNumber,1)=B358)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C358*$B$350)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Road","Long haul",0.60209424083769636,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,4,ExcipientNumber,1)=B359)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C359*$B$350)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Road","Short haul",0.12041884816753928,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,4,ExcipientNumber,1)=B360)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C360*$B$350)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
["Road","Domestic",2.4083769633507855E-2,{"$f":"SUMPRODUCT((OFFSET(Excipient1Transport2,0,4,ExcipientNumber,1)=B361)*(OFFSET(Excipient1Site2Weight,0,0,ExcipientNumber,1))*C361*$B$350)","v":0},{"$error":"#DIV/0!"},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$28+$C$29+$C$31","v":5.663766695326796},{"$error":"#DIV/0!"}]
[]
["Total (including wastage uplifts):",{"$f":"SUM(D353:D361)","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(G353:G361)","v":{"$error":"#DIV/0!"}}]
["Effect of waste (mg CO2e per tablet):",{"$f":"B363*$B$40","v":0}]
[]
[]
["CHEMICAL - TRANSPORT FROM FORMULATION TO PACKAGING"]
[]
["Wastage Uplift Factor:",{"$f":"$B$29*$B$31","v":1.0255358424776946}]
[]
[null,"Air","Sea","Road"]
["(ln UE)2",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$29+$C$31","v":4.0237586180062301},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$29+$C$31","v":4.0237586180062301},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$29+$C$31","v":4.0237586180062301}]
[]
[null,"Emissions per tablet (mg CO2e)",null,null,"S2",null,null,"Σ(S2 x (ln UE)2)"]
[null,"Air","Sea","Road","Air","Sea","Road"]
["Formulation site 1 to packaging",{"$f":"IFERROR(B9*VLOOKUP('Data Input'!G123,Air_EF,2,FALSE),0)*$B$370","v":0},{"$f":"IFERROR(B9*VLOOKUP('Data Input'!H123,Sea_EF,2,FALSE),0)*$B$370","v":0},{"$f":"IFERROR(B9*VLOOKUP('Data Input'!I123,Road_EF,2,FALSE),0)*$B$370","v":0},{"$f":"(B377/$B$380)^2","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"E377*$B$373+F377*$C$373+G377*$D$373","v":{"$error":"#DIV/0!"}}]
["Formulation site 2 to packaging",{"$f":"IFERROR(B12*VLOOKUP('Data Input'!G124,Air_EF,2,FALSE),0)*$B$370","v":0},{"$f":"IFERROR(B12*VLOOKUP('Data Input'!H124,Sea_EF,2,FALSE),0)*$B$370","v":0},{"$f":"IFERROR(B12*VLOOKUP('Data Input'!I124,Road_EF,2,FALSE),0)*$B$370","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},{"$f":"E378*$B$373+F378*$C$373+G378*$D$373","v":{"$error":"#DIV/0!"}}]
[]
["Total (including wastage uplifts):",{"$f":"SUM(B377:D378)","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(H377:H378)","v":{"$error":"#DIV/0!"}}]
["Effect of waste (mg CO2e per tablet):",{"$f":"SUM(B377:D378)*$B$37","v":0}]
[]
["CHEMICAL AND PACKAGING - TRANSPORT FROM PACKAGING TO UK"]
[null,null,null,null,null,"Need to include weight of pallet?"]
["Wastage Uplift Factor:",{"$f":"$B$31","v":1.0204081632653061},null,null,null,"Need to include a distribution figure from RDC to point of sale?"]
[]
[null,"Air","Sea","Road"]
["(ln UE)2",{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$35)^2+$C$31","v":2.3837505406856647},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$34)^2+$C$31","v":2.3837505406856647},{"$f":"LN('Data Quality Matrix'!$N$39)^2+LN('Data Quality Matrix'!$N$33)^2+$C$31","v":2.3837505406856647}]
[]
[]
[null,"Emissions per tablet (mg CO2e)",null,null,"S2",null,null,"Σ(S2 x (ln UE)2)"]
[null,"Air","Sea","Road","Air","Sea","Road"]
["Packaging to UK",{"$f":"IFERROR((B19+B14)*VLOOKUP('Data Input'!G125,Air_EF,2,FALSE),0)*B386","v":0},{"$f":"IFERROR((B19+B14)*VLOOKUP('Data Input'!H125,Sea_EF,2,FALSE),0)*B386","v":0},{"$f":"IFERROR((B19+B14)*VLOOKUP('Data Input'!I125,Road_EF,2,FALSE),0)*B386","v":0},{"$f":"(B394/$B$396)^2","v":{"$error":"#DIV/0!"}},{"$f":"(C394/$B$396)^2","v":{"$error":"#DIV/0!"}},{"$f":"(D394/$B$396)^2","v":{"$error":"#DIV/0!"}},{"$f":"E394*$B$373+F394*$C$373+G394*$D$373","v":{"$error":"#DIV/0!"}}]
[]
["Total (including wastage uplifts):",{"$f":"SUM(B394:D394)","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(H393:H394)","v":{"$error":"#DIV/0!"}}]
["Effect of waste (mg CO2e per tablet):",{"$f":"SUM(B394:D394)*$B$36","v":0}]
[]
[]
["RDC"]
[]
["Emission factor per pallet:",2.8128578313966561,"kg CO2e/pallet","Source: FPX Calculator"]
["Emission factor per tablet (mg CO2e):",{"$f":"IFERROR((B403/(BlistersPerRetail*RetailsPerOuter*OuterPerPallet*TabletsPerPack))*1000000*$B$31,\"\")","v":""},"mg CO2e/tablet"]
[]
["S2",1]
["(ln U)2",2]
[]
["Effect of waste (mg CO2e per tablet):",{"$f":"B404*$B$36","v":{"$error":"#VALUE!"}}]
[]
["Distribution"]
[]
["Emissions factor for road transport:",5.7700000000000001E-2,"kgCO2e/kg","based on 500km artic and 50km 3.5t van"]
["Emission factor per tablet (mg CO2e):",{"$f":"IFERROR(B413*(B14+B19)*$B$31,\"\")","v":""},"mg CO2e/tablet"]
[]
["S2",1]
["(ln U)2",{"$f":"LN('Data Quality Matrix'!N48)^2","v":7.7946810637555305E-2}]
[]
["Effect of waste (mg CO2e per tablet):",{"$f":"B414*$B$36","v":{"$error":"#VALUE!"}}]
[]
["Use Phase"]
["Use Phase Summary:"]
[]
["Total  emissions (mgCO2e/tablet):",{"$f":"B436+B450","v":{"$error":"#DIV/0!"}}]
["Σ Si2 x (ln Ui)2",{"$f":"F436+F450","v":{"$error":"#DIV/0!"}}]
[]
["HOSPITAL"]
[]
[null,null,null,"(ln U)2"]
["Dispensing Cup Weight",{"$f":"'Reference Data'!B74","v":4.0000000000000001E-3},"kg",{"$f":"LN('Data Quality Matrix'!$N$54)^2","v":0.37350956835211491}]
["Material EF",{"$f":"VLOOKUP('Reference Data'!B73,'Packaging EFs'!A2:C12,3,FALSE)","v":4.4059114856022896},"kgCO2e/kg",{"$f":"LN('Data Quality Matrix'!$N$37)^2","v":0.21386857469830975}]
["Avg. no. of tablets per cup",{"$f":"'Reference Data'!B75","v":2},null,{"$f":"LN('Data Quality Matrix'!$N$54)^2","v":0.37350956835211491}]
["Hospital share",{"$f":"NHSSplit+OtherHospitalSplit","v":0.4},null,{"$f":"LN('Data Quality Matrix'!$N$54)^2","v":0.37350956835211491}]
[]
[null,null,null,"(ln U)2","S2","S2 x (ln UE)2"]
["Hospital emissions (mgCO2e/tablet):",{"$f":"B430*B431/B432*B433*1000000","v":3524.7291884818314},null,{"$f":"SUM(D430:D433)","v":1.3343972797546546},{"$f":"B436/($B$436+$B$450)","v":{"$error":"#DIV/0!"}},{"$f":"D436*E436","v":{"$error":"#DIV/0!"}}]
[]
["PHARMACY"]
[null,null,null,"(ln U)2"]
["Paper bag weight",0.01,"kg",{"$f":"LN('Data Quality Matrix'!$N$54)^2","v":0.37350956835211491}]
["2 paper labels weight",{"$f":"'Reference Data'!B80","v":8.0000000000000004E-4},"kg",{"$f":"LN('Data Quality Matrix'!$N$54)^2","v":0.37350956835211491}]
["EF Paper bag",{"$f":"'FPX Reference Data'!D893","v":0.69},"kgCO2e/kg",{"$f":"LN('Data Quality Matrix'!$N$37)^2","v":0.21386857469830975}]
["EF paper labels",{"$f":"'FPX Reference Data'!D1023","v":2},"kgCO2e/kg",{"$f":"LN('Data Quality Matrix'!$N$37)^2","v":0.21386857469830975}]
["Pharmacy share:",{"$f":"PharmacyNHSSplit+PharmacyNonNHSSplit","v":0.6},null,{"$f":"LN('Data Quality Matrix'!$N$54)^2","v":0.37350956835211491}]
[]
[null,null,null,"(ln U)2","S2","S2 x (ln UE)2"]
["Paper bag emissions",{"$f":"B440*B442","v":6.8999999999999999E-3},"kgCO2e",{"$f":"D440+D442","v":0.58737814305042468},{"$f":"B447/($B$447+$B$448)","v":0.81176470588235283},{"$f":"D447*E447","v":0.47681284553505054}]
["Label emissions",{"$f":"B441*B443","v":1.6000000000000001E-3},"kgCO2e",{"$f":"D441+D443","v":0.58737814305042468},{"$f":"B448/($B$447+$B$448)","v":0.18823529411764706},{"$f":"D448*E448","v":0.11056529751537406}]
[]
["Pharmacy emissions (mgCO2e/tablet):",{"$f":"(B440*B442+B441*B443)/TabletsPerPack*1000000","v":{"$error":"#DIV/0!"}},null,{"$f":"F447+F448","v":0.58737814305042457},{"$f":"B450/($B$436+$B$450)","v":{"$error":"#DIV/0!"}},{"$f":"D450*E450","v":{"$error":"#DIV/0!"}}]
[]
[]
["WASTE - END OF LIFE EMISSIONS"]
[]
["WASTE MATERIAL EMISSIONS"]
[]
[null,"End of Life - After Use","At RDC stage","At Packaging Stage"]
["Emissions (mg CO2e per tablet):",{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",B$506,IF(PackagingCalculationMethod=\"Use Defaults\",B$471,\"\"))","v":""},{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",C$506,IF(PackagingCalculationMethod=\"Use Defaults\",C$471,\"\"))","v":""},{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",D$506,IF(PackagingCalculationMethod=\"Use Defaults\",D$471,\"\"))","v":""}]
["Σ Si2 x (ln Ui)2",{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",B$507,IF(PackagingCalculationMethod=\"Use Defaults\",B$472,\"\"))","v":""},{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",C$507,IF(PackagingCalculationMethod=\"Use Defaults\",C$472,\"\"))","v":""},{"$f":"IF(PackagingCalculationMethod=\"Specified Materials\",D$507,IF(PackagingCalculationMethod=\"Use Defaults\",D$472,\"\"))","v":""}]
[]
["NEED WASTE TREATMENT FOR CHEMICALS IN WASTED TABLETS?"]
[]
["Percentage Commercial Sales:",{"$f":"SUM(CommercialPercentage)","v":0.4}]
["Percentage Domestic Sales:",{"$f":"SUM(DomesticPercentage)","v":0.6}]
[]
["Default packaging"]
[]
["Default Summary:","INCLUDES EFFECT OF WASTAGE FROM PREVIOUS STAGES, BUT STILL NEED TO ACCOUNT FOR THIS IN TRANSPORT SOMEWHERE?"]
[]
[null,"End of Life - After Use","At RDC stage","At Packaging Stage"]
["Emissions (mg CO2e per tablet):",{"$f":"IF(WasteDefault=\"Small\",SUM($C$477:$C$481),IF(WasteDefault=\"Medium\",SUM($C$486:$C$490),IF(WasteDefault=\"Large\",SUM($C$495:$C$499),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"IF(WasteDefault=\"Small\",SUM($G$477:$G$481),IF(WasteDefault=\"Medium\",SUM($G$486:$G$490),IF(WasteDefault=\"Large\",SUM($G$495:$G$499),\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"IF(WasteDefault=\"Small\",SUM($K$477:$K$481),IF(WasteDefault=\"Medium\",SUM($K$486:$K$490),IF(WasteDefault=\"Large\",SUM($K$495:$K$499),\"\")))","v":{"$error":"#DIV/0!"}}]
["Σ Si2 x (ln Ui)2",{"$f":"IF(WasteDefault=\"Small\",SUM($F$477:$F$481),IF(WasteDefault=\"Medium\",SUM($F$486:$F$490),IF(WasteDefault=\"Large\",SUM($F$495:$F$499),\"\")))","v":0},{"$f":"IF(WasteDefault=\"Small\",SUM($J$477:$J$481),IF(WasteDefault=\"Medium\",SUM($J$486:$J$490),IF(WasteDefault=\"Large\",SUM($J$495:$J$499),\"\")))","v":0},{"$f":"IF(WasteDefault=\"Small\",SUM($N$477:$N$481),IF(WasteDefault=\"Medium\",SUM($N$486:$N$490),IF(WasteDefault=\"Large\",SUM($N$495:$N$499),\"\")))","v":0}]
[]
[{"$f":"'Reference Data'!A38","v":"Small:"}]
[null,null,"End of Life After Use Phase",null,null,null,"From RDC",null,null,null,"Waste from packaging process"]
[{"$f":"'Reference Data'!A40","v":"Material"},{"$f":"'Reference Data'!E40","v":"Total weight per tablet (mg)"},"Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
[{"$f":"'Reference Data'!A42","v":"PVC - blister"},{"$f":"'Reference Data'!E42","v":1486},{"$f":"IF(ISERROR(MATCH($A477,'Packaging EFs'!$A:$A,0)),\"\",$B477*(($B$463*VLOOKUP($A477,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A477,'Packaging EFs'!$A:$E,5,FALSE))))","v":1594.4423359999998},{"$f":"C477/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E477*D477,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A477,'Packaging EFs'!$A:$A,0)),\"\",$B477*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A477,'Packaging EFs'!$A:$E,3,FALSE))","v":23.048163265306123},{"$f":"G477/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I477*H477,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A477,'Packaging EFs'!$A:$A,0)),\"\",$B477*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP($A477,'Packaging EFs'!$A:$E,3,FALSE))","v":29.548927263212978},{"$f":"K477/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M477*L477,\"\")","v":""}]
[{"$f":"'Reference Data'!A43","v":"PVdC - blister"},{"$f":"'Reference Data'!E43","v":178},{"$f":"IF(ISERROR(MATCH($A478,'Packaging EFs'!$A:$A,0)),\"\",$B478*(($B$463*VLOOKUP($A478,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A478,'Packaging EFs'!$A:$E,5,FALSE))))","v":368.98972800000001},{"$f":"C478/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E478*D478,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A478,'Packaging EFs'!$A:$A,0)),\"\",$B478*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A478,'Packaging EFs'!$A:$E,3,FALSE))","v":6.3934693877551032},{"$f":"G478/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I478*H478,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A478,'Packaging EFs'!$A:$A,0)),\"\",$B478*(($B$463*VLOOKUP($A478,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A478,'Packaging EFs'!$A:$E,4,FALSE))))","v":866.76459200000011},{"$f":"K478/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M478*L478,\"\")","v":""}]
[{"$f":"'Reference Data'!A44","v":"Aluminium"},{"$f":"'Reference Data'!E44","v":239},{"$f":"IF(ISERROR(MATCH($A479,'Packaging EFs'!$A:$A,0)),\"\",$B479*(($B$463*VLOOKUP($A479,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A479,'Packaging EFs'!$A:$E,5,FALSE))))","v":0},{"$f":"C479/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E479*D479,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A479,'Packaging EFs'!$A:$A,0)),\"\",$B479*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A479,'Packaging EFs'!$A:$E,3,FALSE))","v":24.953551020408167},{"$f":"G479/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I479*H479,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A479,'Packaging EFs'!$A:$A,0)),\"\",$B479*(($B$463*VLOOKUP($A479,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A479,'Packaging EFs'!$A:$E,4,FALSE))))","v":1222.7239999999999},{"$f":"K479/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M479*L479,\"\")","v":""}]
[{"$f":"'Reference Data'!A45","v":"Paper"},{"$f":"'Reference Data'!E45","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($A480,'Packaging EFs'!$A:$A,0)),\"\",$B480*(($B$463*VLOOKUP($A480,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A480,'Packaging EFs'!$A:$E,5,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"C480/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E480*D480,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A480,'Packaging EFs'!$A:$A,0)),\"\",$B480*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A480,'Packaging EFs'!$A:$E,3,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"G480/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I480*H480,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A480,'Packaging EFs'!$A:$A,0)),\"\",$B480*(($B$463*VLOOKUP($A480,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A480,'Packaging EFs'!$A:$E,4,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"K480/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M480*L480,\"\")","v":""}]
[{"$f":"'Reference Data'!A46","v":"Cardboard"},{"$f":"'Reference Data'!E46","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($A481,'Packaging EFs'!$A:$A,0)),\"\",$B481*(($B$463*VLOOKUP($A481,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A481,'Packaging EFs'!$A:$E,5,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"C481/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E481*D481,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A481,'Packaging EFs'!$A:$A,0)),\"\",$B481*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A481,'Packaging EFs'!$A:$E,3,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"G481/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I481*H481,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A481,'Packaging EFs'!$A:$A,0)),\"\",$B481*(($B$463*VLOOKUP($A481,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A481,'Packaging EFs'!$A:$E,4,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"K481/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M481*L481,\"\")","v":""}]
[]
[{"$f":"'Reference Data'!A48","v":"Medium:"}]
[null,null,"End of Life After Use Phase",null,null,null,"From RDC",null,null,null,"Waste from packaging process"]
[{"$f":"'Reference Data'!A50","v":"Material"},{"$f":"'Reference Data'!E50","v":"Total weight per tablet (mg)"},"Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
[{"$f":"'Reference Data'!A52","v":"PVC - blister"},{"$f":"'Reference Data'!E52","v":2351},{"$f":"IF(ISERROR(MATCH($A486,'Packaging EFs'!$A:$A,0)),\"\",$B486*(($B$463*VLOOKUP($A486,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A486,'Packaging EFs'!$A:$E,5,FALSE))))","v":2522.5665759999997},{"$f":"C486/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E486*D486,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A486,'Packaging EFs'!$A:$A,0)),\"\",$B486*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A486,'Packaging EFs'!$A:$E,3,FALSE))","v":36.464489795918368},{"$f":"G486/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I486*H486,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A486,'Packaging EFs'!$A:$A,0)),\"\",$B486*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP($A486,'Packaging EFs'!$A:$E,3,FALSE))","v":46.749345892203038},{"$f":"K486/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M486*L486,\"\")","v":""}]
[{"$f":"'Reference Data'!A53","v":"PVdC - blister"},{"$f":"'Reference Data'!E53","v":282},{"$f":"IF(ISERROR(MATCH($A487,'Packaging EFs'!$A:$A,0)),\"\",$B487*(($B$463*VLOOKUP($A487,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A487,'Packaging EFs'!$A:$E,5,FALSE))))","v":584.57923200000005},{"$f":"C487/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E487*D487,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A487,'Packaging EFs'!$A:$A,0)),\"\",$B487*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A487,'Packaging EFs'!$A:$E,3,FALSE))","v":10.128979591836737},{"$f":"G487/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I487*H487,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A487,'Packaging EFs'!$A:$A,0)),\"\",$B487*(($B$463*VLOOKUP($A487,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A487,'Packaging EFs'!$A:$E,4,FALSE))))","v":1373.1888480000002},{"$f":"K487/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M487*L487,\"\")","v":""}]
[{"$f":"'Reference Data'!A54","v":"Aluminium"},{"$f":"'Reference Data'!E54","v":377},{"$f":"IF(ISERROR(MATCH($A488,'Packaging EFs'!$A:$A,0)),\"\",$B488*(($B$463*VLOOKUP($A488,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A488,'Packaging EFs'!$A:$E,5,FALSE))))","v":0},{"$f":"C488/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E488*D488,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A488,'Packaging EFs'!$A:$A,0)),\"\",$B488*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A488,'Packaging EFs'!$A:$E,3,FALSE))","v":39.361877551020413},{"$f":"G488/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I488*H488,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A488,'Packaging EFs'!$A:$A,0)),\"\",$B488*(($B$463*VLOOKUP($A488,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A488,'Packaging EFs'!$A:$E,4,FALSE))))","v":1928.732},{"$f":"K488/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M488*L488,\"\")","v":""}]
[{"$f":"'Reference Data'!A55","v":"Paper"},{"$f":"'Reference Data'!E55","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($A489,'Packaging EFs'!$A:$A,0)),\"\",$B489*(($B$463*VLOOKUP($A489,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A489,'Packaging EFs'!$A:$E,5,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"C489/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E489*D489,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A489,'Packaging EFs'!$A:$A,0)),\"\",$B489*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A489,'Packaging EFs'!$A:$E,3,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"G489/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I489*H489,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A489,'Packaging EFs'!$A:$A,0)),\"\",$B489*(($B$463*VLOOKUP($A489,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A489,'Packaging EFs'!$A:$E,4,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"K489/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M489*L489,\"\")","v":""}]
[{"$f":"'Reference Data'!A56","v":"Cardboard"},{"$f":"'Reference Data'!E56","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($A490,'Packaging EFs'!$A:$A,0)),\"\",$B490*(($B$463*VLOOKUP($A490,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A490,'Packaging EFs'!$A:$E,5,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"C490/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E490*D490,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A490,'Packaging EFs'!$A:$A,0)),\"\",$B490*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A490,'Packaging EFs'!$A:$E,3,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"G490/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I490*H490,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A490,'Packaging EFs'!$A:$A,0)),\"\",$B490*(($B$463*VLOOKUP($A490,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A490,'Packaging EFs'!$A:$E,4,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"K490/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M490*L490,\"\")","v":""}]
[]
[{"$f":"'Reference Data'!A58","v":"Large:"}]
[null,null,"End of Life After Use Phase",null,null,null,"From RDC",null,null,null,"Waste from packaging process"]
[{"$f":"'Reference Data'!A60","v":"Material"},{"$f":"'Reference Data'!E60","v":"Total weight per tablet (mg)"},"Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
[{"$f":"'Reference Data'!A62","v":"PVC - blister"},{"$f":"'Reference Data'!E62","v":3634},{"$f":"IF(ISERROR(MATCH($A495,'Packaging EFs'!$A:$A,0)),\"\",$B495*(($B$463*VLOOKUP($A495,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A495,'Packaging EFs'!$A:$E,5,FALSE))))","v":3899.1947839999998},{"$f":"C495/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E495*D495,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A495,'Packaging EFs'!$A:$A,0)),\"\",$B495*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A495,'Packaging EFs'!$A:$E,3,FALSE))","v":56.364081632653068},{"$f":"G495/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I495*H495,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A495,'Packaging EFs'!$A:$A,0)),\"\",$B495*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP($A495,'Packaging EFs'!$A:$E,3,FALSE))","v":72.261643118785983},{"$f":"K495/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M495*L495,\"\")","v":""}]
[{"$f":"'Reference Data'!A63","v":"PVdC - blister"},{"$f":"'Reference Data'!E63","v":436},{"$f":"IF(ISERROR(MATCH($A496,'Packaging EFs'!$A:$A,0)),\"\",$B496*(($B$463*VLOOKUP($A496,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A496,'Packaging EFs'!$A:$E,5,FALSE))))","v":903.81753600000002},{"$f":"C496/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E496*D496,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A496,'Packaging EFs'!$A:$A,0)),\"\",$B496*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A496,'Packaging EFs'!$A:$E,3,FALSE))","v":15.660408163265309},{"$f":"G496/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I496*H496,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A496,'Packaging EFs'!$A:$A,0)),\"\",$B496*(($B$463*VLOOKUP($A496,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A496,'Packaging EFs'!$A:$E,4,FALSE))))","v":2123.0863040000004},{"$f":"K496/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M496*L496,\"\")","v":""}]
[{"$f":"'Reference Data'!A64","v":"Aluminium"},{"$f":"'Reference Data'!E64","v":583},{"$f":"IF(ISERROR(MATCH($A497,'Packaging EFs'!$A:$A,0)),\"\",$B497*(($B$463*VLOOKUP($A497,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A497,'Packaging EFs'!$A:$E,5,FALSE))))","v":0},{"$f":"C497/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E497*D497,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A497,'Packaging EFs'!$A:$A,0)),\"\",$B497*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A497,'Packaging EFs'!$A:$E,3,FALSE))","v":60.86995918367348},{"$f":"G497/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I497*H497,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A497,'Packaging EFs'!$A:$A,0)),\"\",$B497*(($B$463*VLOOKUP($A497,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A497,'Packaging EFs'!$A:$E,4,FALSE))))","v":2982.6279999999997},{"$f":"K497/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M497*L497,\"\")","v":""}]
[{"$f":"'Reference Data'!A65","v":"Paper"},{"$f":"'Reference Data'!E65","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($A498,'Packaging EFs'!$A:$A,0)),\"\",$B498*(($B$463*VLOOKUP($A498,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A498,'Packaging EFs'!$A:$E,5,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"C498/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E498*D498,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A498,'Packaging EFs'!$A:$A,0)),\"\",$B498*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A498,'Packaging EFs'!$A:$E,3,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"G498/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I498*H498,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A498,'Packaging EFs'!$A:$A,0)),\"\",$B498*(($B$463*VLOOKUP($A498,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A498,'Packaging EFs'!$A:$E,4,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"K498/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M498*L498,\"\")","v":""}]
[{"$f":"'Reference Data'!A66","v":"Cardboard"},{"$f":"'Reference Data'!E66","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($A499,'Packaging EFs'!$A:$A,0)),\"\",$B499*(($B$463*VLOOKUP($A499,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP($A499,'Packaging EFs'!$A:$E,5,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"C499/$B$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2","v":0.27674229601275946},{"$f":"IFERROR(E499*D499,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A499,'Packaging EFs'!$A:$A,0)),\"\",$B499*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP($A499,'Packaging EFs'!$A:$E,3,FALSE))","v":{"$error":"#DIV/0!"}},{"$f":"G499/$C$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$31","v":0.52147154066316037},{"$f":"IFERROR(I499*H499,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($A499,'Packaging EFs'!$A:$A,0)),\"\",$B499*(($B$463*VLOOKUP($A499,'Packaging EFs'!$A:$E,3,FALSE))+($B$464*VLOOKUP($A499,'Packaging EFs'!$A:$E,4,FALSE))))","v":{"$error":"#DIV/0!"}},{"$f":"K499/$D$471","v":{"$error":"#DIV/0!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$43)^2+$D$30+$D$31","v":0.76620078531356128},{"$f":"IFERROR(M499*L499,\"\")","v":""}]
[]
["Specified packaging"]
[]
["Specified Summary:"]
[]
[null,"End of Life - After Use","At RDC stage","At Packaging Stage"]
["Emissions (mg CO2e per tablet):",{"$f":"SUM(D511:D514,D518:D520,D524:D525)","v":0},{"$f":"SUM(H511:H514,H518:H520,H524:H525)","v":0},{"$f":"SUM(L511:L514,L518:L520,L524:L525)","v":0}]
["Σ Si2 x (ln Ui)2",{"$f":"SUM(G511:G514,G518:G520,G524:G525)","v":0},{"$f":"SUM(K511:K514,K518:K520,K524:K525)","v":0},{"$f":"SUM(O511:O514,O518:O520,O524:O525)","v":0}]
[]
[null,null,null,"End of Life After Use Phase",null,null,null,"From RDC",null,null,null,"Waste from packaging process"]
[null,"Material","Weight (mg per tablet)","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
["Blister Strip",{"$f":"'Data Input'!G109","v":0},{"$f":"('Data Input'!H109*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B511,'Packaging EFs'!$A:$A,0)),\"\",$C511*(($B$463*VLOOKUP('Calculation sheet'!$B511,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B511,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D511/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F511*E511,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B511,'Packaging EFs'!$A:$A,0)),\"\",$C511*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B511,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H511/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J511*I511,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B511,'Packaging EFs'!$A:$A,0)),\"\",$C511*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B511,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L511/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N511*M511,\"\")","v":""}]
[null,{"$f":"'Data Input'!G110","v":0},{"$f":"('Data Input'!H110*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B512,'Packaging EFs'!$A:$A,0)),\"\",$C512*(($B$463*VLOOKUP('Calculation sheet'!$B512,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B512,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D512/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F512*E512,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B512,'Packaging EFs'!$A:$A,0)),\"\",$C512*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B512,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H512/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J512*I512,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B512,'Packaging EFs'!$A:$A,0)),\"\",$C512*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B512,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L512/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N512*M512,\"\")","v":""}]
[null,{"$f":"'Data Input'!G111","v":0},{"$f":"('Data Input'!H111*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B513,'Packaging EFs'!$A:$A,0)),\"\",$C513*(($B$463*VLOOKUP('Calculation sheet'!$B513,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B513,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D513/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F513*E513,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B513,'Packaging EFs'!$A:$A,0)),\"\",$C513*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B513,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H513/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J513*I513,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B513,'Packaging EFs'!$A:$A,0)),\"\",$C513*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B513,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L513/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N513*M513,\"\")","v":""}]
[null,{"$f":"'Data Input'!G112","v":0},{"$f":"('Data Input'!H112*1000)/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B514,'Packaging EFs'!$A:$A,0)),\"\",$C514*(($B$463*VLOOKUP('Calculation sheet'!$B514,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B514,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D514/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F514*E514,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B514,'Packaging EFs'!$A:$A,0)),\"\",$C514*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B514,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H514/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J514*I514,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B514,'Packaging EFs'!$A:$A,0)),\"\",$C514*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B514,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L514/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N514*M514,\"\")","v":""}]
[]
[null,null,null,"End of Life After Use Phase",null,null,null,"From RDC",null,null,null,"Waste from packaging process"]
[null,"Material","Weight (mg per tablet)","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
["Retail Pack",{"$f":"'Data Input'!G114","v":0},{"$f":"('Data Input'!H114*1000)/(TabletsPerPack*BlistersPerRetail)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B518,'Packaging EFs'!$A:$A,0)),\"\",$C518*(($B$463*VLOOKUP('Calculation sheet'!$B518,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B518,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D518/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F518*E518,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B518,'Packaging EFs'!$A:$A,0)),\"\",$C518*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B518,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H518/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J518*I518,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B518,'Packaging EFs'!$A:$A,0)),\"\",$C518*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B518,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L518/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N518*M518,\"\")","v":""}]
[null,{"$f":"'Data Input'!G115","v":0},{"$f":"('Data Input'!H115*1000)/(TabletsPerPack*BlistersPerRetail)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B519,'Packaging EFs'!$A:$A,0)),\"\",$C519*(($B$463*VLOOKUP('Calculation sheet'!$B519,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B519,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D519/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F519*E519,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B519,'Packaging EFs'!$A:$A,0)),\"\",$C519*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B519,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H519/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J519*I519,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B519,'Packaging EFs'!$A:$A,0)),\"\",$C519*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B519,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L519/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N519*M519,\"\")","v":""}]
[null,{"$f":"'Data Input'!G116","v":0},{"$f":"('Data Input'!H116*1000)/(TabletsPerPack*BlistersPerRetail)","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B520,'Packaging EFs'!$A:$A,0)),\"\",$C520*(($B$463*VLOOKUP('Calculation sheet'!$B520,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B520,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D520/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F520*E520,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B520,'Packaging EFs'!$A:$A,0)),\"\",$C520*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B520,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H520/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J520*I520,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B520,'Packaging EFs'!$A:$A,0)),\"\",$C520*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B520,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L520/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N520*M520,\"\")","v":""}]
[]
[null,null,null,"End of Life After Use Phase",null,null,null,"From RDC",null,null,null,"Waste from packaging process"]
[null,"Material","Weight (mg per tablet)","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2","Emissions per tablet (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
["Outer Box",{"$f":"'Data Input'!G118","v":0},{"$f":"('Data Input'!H118*1000)/(TabletsPerPack*BlistersPerRetail*RetailsPerOuter )","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B524,'Packaging EFs'!$A:$A,0)),\"\",$C524*(($B$463*VLOOKUP('Calculation sheet'!$B524,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B524,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D524/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F524*E524,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B524,'Packaging EFs'!$A:$A,0)),\"\",$C524*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B524,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H524/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J524*I524,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B524,'Packaging EFs'!$A:$A,0)),\"\",$C524*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B524,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L524/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N524*M524,\"\")","v":""}]
[null,{"$f":"'Data Input'!G119","v":0},{"$f":"('Data Input'!H119*1000)/(TabletsPerPack*BlistersPerRetail*RetailsPerOuter )","v":{"$error":"#DIV/0!"}},{"$f":"IF(ISERROR(MATCH($B525,'Packaging EFs'!$A:$A,0)),\"\",$C525*(($B$463*VLOOKUP('Calculation sheet'!$B525,'Packaging EFs'!$A:$E,4,FALSE))+($B$464*VLOOKUP('Calculation sheet'!$B525,'Packaging EFs'!$A:$E,5,FALSE))))","v":""},{"$f":"D525/$B$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2","v":5.8550651179477109E-2},{"$f":"IFERROR(F525*E525,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B525,'Packaging EFs'!$A:$A,0)),\"\",$C525*$B$463*('Data Input'!$G$138/(1-'Data Input'!$G$138))*VLOOKUP('Calculation sheet'!$B525,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"H525/$C$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31","v":0.30327989582987802},{"$f":"IFERROR(J525*I525,\"\")","v":""},{"$f":"IF(ISERROR(MATCH($B525,'Packaging EFs'!$A:$A,0)),\"\",$C525*$B$463*('Data Input'!$G$102/((1-'Data Input'!$G$102)*(1-'Data Input'!$G$138)))*VLOOKUP('Calculation sheet'!$B525,'Packaging EFs'!$A:$E,3,FALSE))","v":""},{"$f":"L525/$D$506","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$36)^2+LN('Data Quality Matrix'!$N$44)^2+$D$31+$D$30","v":0.54800914048027893},{"$f":"IFERROR(N525*M525,\"\")","v":""}]
[]
[]
[]
["WASTE TRANSPORT"]
[]
[null,"Waste Lorry Emission Factor (kg CO2e/kg waste)","Weight of waste (mg):","Emissions (mg CO2e)","S2","(ln U)2","S2 x (ln U)2"]
["After End Use",{"$f":"'FPX Reference Data'!$D$1239","v":2.340057152073733E-2},{"$f":"$B$19","v":""},{"$f":"C532*B532","v":{"$error":"#VALUE!"}},{"$f":"D532/SUM($D$532:$D$534)","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$42)^2","v":0.24234876453072074},{"$f":"F532*E532","v":{"$error":"#VALUE!"}}]
["From RDC",{"$f":"'FPX Reference Data'!$D$1239","v":2.340057152073733E-2},{"$f":"('Data Input'!$G$138/(1-'Data Input'!$G$138))*$B$19","v":{"$error":"#VALUE!"}},{"$f":"C533*B533","v":{"$error":"#VALUE!"}},{"$f":"D533/SUM($D$532:$D$534)","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$42)^2+$D$31","v":0.48707800918112165},{"$f":"F533*E533","v":{"$error":"#VALUE!"}}]
["From Packaging Process",{"$f":"'FPX Reference Data'!$D$1239","v":2.340057152073733E-2},{"$f":"('Data Input'!$G$102/((1-'Data Input'!$G$138)*(1-'Data Input'!$G$102)))*$B$19","v":{"$error":"#VALUE!"}},{"$f":"C534*B534","v":{"$error":"#VALUE!"}},{"$f":"D534/SUM($D$532:$D$534)","v":{"$error":"#VALUE!"}},{"$f":"LN('Data Quality Matrix'!$N$42)^2+$D$31+$D$30","v":0.73180725383152256},{"$f":"F534*E534","v":{"$error":"#VALUE!"}}]

{"sheet":"Sheet2","index":4,"n_rows":777,"n_cols":14,"rows_kept":777,"cut":false,"hidden":true,"merged":[]}
[]
["API",{"$f":"'Calculation sheet'!D48","v":0},{"$f":"B2*SQRT('Calculation sheet'!F48)-B2","v":{"$error":"#DIV/0!"}}]
["Excipients",{"$f":"'Calculation sheet'!D49","v":0},{"$f":"B3*SQRT('Calculation sheet'!F49)-B3","v":{"$error":"#VALUE!"}}]
["Packaging",{"$f":"'Calculation sheet'!D50","v":""},{"$f":"B4*SQRT('Calculation sheet'!F50)-B4","v":{"$error":"#VALUE!"}}]
["Energy",{"$f":"'Calculation sheet'!D52","v":{"$error":"#N/A"}},{"$f":"B5*SQRT('Calculation sheet'!F51)-B5","v":{"$error":"#N/A"}}]
["In-bound Transport",{"$f":"'Calculation sheet'!D53","v":0},{"$f":"B6*SQRT('Calculation sheet'!F53)-B6","v":{"$error":"#DIV/0!"}}]
["Energy",{"$f":"'Calculation sheet'!D56","v":{"$error":"#N/A"}},{"$f":"B7*SQRT('Calculation sheet'!F56)-B7","v":{"$error":"#N/A"}}]
["In-bound Transport",{"$f":"'Calculation sheet'!D57","v":0},{"$f":"B8*SQRT('Calculation sheet'!F57)-B8","v":{"$error":"#DIV/0!"}}]
["Waste",{"$f":"'Calculation sheet'!D58","v":{"$error":"#VALUE!"}},{"$f":"B9*SQRT('Calculation sheet'!F58)-B9","v":{"$error":"#VALUE!"}}]
["RDC",{"$f":"'Calculation sheet'!D60","v":""},{"$f":"B10*SQRT('Calculation sheet'!F60)-B10","v":{"$error":"#VALUE!"}}]
["Transport",{"$f":"'Calculation sheet'!D61","v":""},{"$f":"B11*SQRT('Calculation sheet'!F61)-B11","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"Average",{"$f":"AVERAGE(N16:N777)","v":{"$error":"#DIV/0!"}}]
["Waste",{"$f":"'Calculation sheet'!D62","v":{"$error":"#VALUE!"}},{"$f":"B12*SQRT('Calculation sheet'!F62)-B12","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"St Dev",{"$f":"STDEV(N16:N777)","v":{"$error":"#DIV/0!"}}]
["End of Life",{"$f":"'Calculation sheet'!D67","v":{"$error":"#VALUE!"}},{"$f":"B13*SQRT('Calculation sheet'!F67)-B13","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,"Approx. U",{"$f":"1+(2*N12/N11)","v":{"$error":"#DIV/0!"}}]
[]
[null,"API","Excipients","Packaging","Energy","In-bound Transport","Energy","In-bound Transport","Waste","RDC","Transport","Waste","End of Life","Total"]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B16:M16)","v":{"$error":"#DIV/0!"}}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B17:M17)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B81:M81)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B145:M145)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B209:M209)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B273:M273)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B337:M337)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B401:M401)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B465:M465)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B529:M529)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B593:M593)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B657:M657)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$f":"_xlfn.NORM.INV(RAND(),$B$2,$C$2)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$3,$C$3)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$4,$C$4)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$5,$C$5)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$6,$C$6)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$7,$C$7)","v":{"$error":"#N/A"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$8,$C$8)","v":{"$error":"#DIV/0!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$9,$C$9)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$10,$C$10)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$11,$C$11)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$12,$C$12)","v":{"$error":"#VALUE!"}},{"$f":"_xlfn.NORM.INV(RAND(),$B$13,$C$13)","v":{"$error":"#VALUE!"}},{"$f":"SUM(B721:M721)","v":{"$error":"#DIV/0!"}}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]
[null,{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#N/A"},{"$error":"#DIV/0!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#DIV/0!"}]

{"sheet":"Data Quality Matrix","index":5,"n_rows":55,"n_cols":14,"rows_kept":55,"cut":false,"hidden":true,"merged":[[24,1,24,6],[24,7,24,12],[1,1,1,4],[1,5,1,8]]}
["Pedigree Matrix"]
[null,"Data Quality Criteria",null,null,null,"API Data Quality Criteria"]
["Data Quality Indicators","Very Good","Good","Fair","Poor","Very Good","Good","Fair","Poor"]
["Precision",1,1.1000000000000001,1.2,1.5,1,1.5,2.2000000000000002,3.5]
["Completeness",1,1.05,1.1000000000000001,1.2,1,1.5,2,3]
["Temporal Representativeness",1,1.1000000000000001,1.2,1.5,1,1.1000000000000001,1.2,1.5]
["Geographical Representativeness",1,1.02,1.05,1.1000000000000001,1,1.02,1.05,1.1000000000000001]
["Technological Representativenss",1,1.2,1.5,2,1,1.5,2,3]
[]
[]
["Basic Uncertainty Factors by Process Type"]
["Combustion Process",1.05]
["Thermal Energy",1.05]
["Electricity",1.05]
["Industrial Products",1.05]
["Agricultural Products",2]
["Transport Services",2]
["Infrastructure",3]
["Direct emissions, CO2",1.05]
["Direct emissions, Other GHGs",1.5]
["API",1.5]
["Activity Data",1]
[]
[]
[null,"Pedigree",null,null,null,null,null,"(ln(U))2",null,null,null,null,null,"U Total"]
[null,"Precision","Completeness","Temporal representativeness","Geographical representativeness","Technological representativeness","Basic","Precision","Completeness","Temporal representativeness","Geographical representativeness","Technological representativeness","Basic"]
["Average API EF","Poor","Fair","Fair","Poor","Poor","API",{"$f":"LN(HLOOKUP(B27,$F$3:$I$8,2,FALSE))^2","v":1.5694150552333266},{"$f":"LN(HLOOKUP(C27,$F$3:$I$8,3,FALSE))^2","v":0.48045301391820139},{"$f":"LN(HLOOKUP(D27,$F$3:$I$8,4,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(E27,$F$3:$I$8,5,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(F27,$F$3:$I$8,6,FALSE))^2","v":1.2069489608125821},{"$f":"LN(VLOOKUP(G27,$A$12:$B$22,2,FALSE))^2","v":0.16440195389316542},{"$f":"EXP(SQRT(SUM(H27:M27)))","v":6.430549267327593}]
["H,M,L API EF","Poor","Fair","Fair","Poor","Fair","API",{"$f":"LN(HLOOKUP(B28,$F$3:$I$8,2,FALSE))^2","v":1.5694150552333266},{"$f":"LN(HLOOKUP(C28,$F$3:$I$8,3,FALSE))^2","v":0.48045301391820139},{"$f":"LN(HLOOKUP(D28,$F$3:$I$8,4,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(E28,$F$3:$I$8,5,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(F28,$F$3:$I$8,6,FALSE))^2","v":0.48045301391820139},{"$f":"LN(VLOOKUP(G28,$A$12:$B$22,2,FALSE))^2","v":0.16440195389316542},5.2299550161573549]
["Default Excipient EF (not used)","Poor","Fair","Fair","Fair","Good","Industrial Products",{"$f":"LN(HLOOKUP(B29,$B$3:$E$8,2,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(C29,$B$3:$E$8,3,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(D29,$B$3:$E$8,4,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(E29,$B$3:$E$8,5,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(F29,$B$3:$E$8,6,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(VLOOKUP(G29,$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.6400080773205654]
["Packaging EF","Fair","Good","Good","Fair","Good","Industrial Products",3.3241150071771211E-2,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,2.3804801196801307E-3,1.3332100258556558]
["Electricity EF","Very Good","Very Good","Good","Very Good","Very Good","Electricity",0,0,9.0840303743327487E-3,0,0,2.3804801196801307E-3,1.1130148943987077]
["Gas EF","Good","Very Good","Good","Good","Very Good","Thermal Energy",9.0840303743327487E-3,0,9.0840303743327487E-3,3.921440478314025E-4,0,2.3804801196801307E-3,1.1557031727027498]
["Road Transport EF","Good","Good","Good","Good","Good","Transport Services",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,3.921440478314025E-4,3.3241150071771211E-2,0.48045301391820139,2.0775457873865859]
["Sea Transport EF","Good","Good","Good","Good","Good","Transport Services",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,3.921440478314025E-4,3.3241150071771211E-2,0.48045301391820139,2.0775457873865859]
["Air Transport EF","Good","Good","Good","Good","Good","Transport Services",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,3.921440478314025E-4,3.3241150071771211E-2,0.48045301391820139,2.0775457873865859]
["Packaging Material EF","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,2.3804801196801307E-3,1.2737590597901596]
["Use Phasre Material EF","Fair","Good","Good","Fair","Fair","Industrial Products",{"$f":"LN(HLOOKUP(B37,$B$3:$E$8,2,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(C37,$B$3:$E$8,3,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(D37,$B$3:$E$8,4,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(E37,$B$3:$E$8,5,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(F37,$B$3:$E$8,6,FALSE))^2","v":0.16440195389316542},{"$f":"LN(VLOOKUP(G37,$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},{"$f":"EXP(SQRT(SUM(H37:M37)))","v":1.587974441862682}]
[]
["Transport Distance","Poor","Fair","Very Good","Fair","Good","Activity Data",{"$f":"LN(HLOOKUP(B39,$B$3:$E$8,2,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(C39,$B$3:$E$8,3,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(D39,$B$3:$E$8,4,FALSE))^2","v":0},{"$f":"LN(HLOOKUP(E39,$B$3:$E$8,5,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(F39,$B$3:$E$8,6,FALSE))^2","v":3.3241150071771211E-2},0,{"$f":"EXP(SQRT(SUM(H39:M39)))","v":1.579775677111255}]
["Electricity Process","Fair","Good","Good","Fair","Good","Activity Data",3.3241150071771211E-2,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,0,1.3276635867218565]
["Gas Process","Fair","Good","Good","Fair","Good","Activity Data",3.3241150071771211E-2,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,0,1.3276635867218565]
["Waste Transport","Fair","Fair","Fair","Fair","Fair","Activity Data",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.16440195389316542,0,1.6360573781545753]
["Default Packaging - mass","Fair","Fair","Good","Fair","Fair","Activity Data",3.3241150071771211E-2,9.0840303743327487E-3,9.0840303743327487E-3,2.3804801196801307E-3,0.16440195389316542,0,1.5953767020422347]
["User defined packaging - mass","Very Good","Very Good","Very Good","Very Good","Very Good","Activity Data",0,0,0,0,0,0,1]
["Chemical input (API and excipient) - mass","Very Good","Very Good","Very Good","Very Good","Very Good","Activity Data",0,0,0,0,0,0,1]
["Formulation process","Fair","Good","Good","Good","Good","Activity Data",3.3241150071771211E-2,2.3804801196801307E-3,9.0840303743327487E-3,3.921440478314025E-4,3.3241150071771211E-2,0,1.3229855584076429]
["Packaging process","Fair","Good","Good","Good","Good","Activity Data",3.3241150071771211E-2,2.3804801196801307E-3,9.0840303743327487E-3,3.921440478314025E-4,3.3241150071771211E-2,0,1.3229855584076429]
["Distribution","Fair","Good","Good","Very Good","Good","Activity Data",3.3241150071771211E-2,2.3804801196801307E-3,9.0840303743327487E-3,0,3.3241150071771211E-2,0,1.3220579299510793]
["Retail","Poor","Fair","Good","Very Good","Good","Activity Data",0.16440195389316542,9.0840303743327487E-3,9.0840303743327487E-3,0,3.3241150071771211E-2,0,1.5913055862177166]
[]
["Wastage Rates - User Defined","Good","Good","Good","Good","Good","Industrial Products",{"$f":"LN(HLOOKUP(B51,$B$3:$E$8,2,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(C51,$B$3:$E$8,3,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(D51,$B$3:$E$8,4,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(E51,$B$3:$E$8,5,FALSE))^2","v":3.921440478314025E-4},{"$f":"LN(HLOOKUP(F51,$B$3:$E$8,6,FALSE))^2","v":3.3241150071771211E-2},2.3804801196801307E-3,{"$f":"EXP(SQRT(SUM(H51:M51)))","v":1.2684914136970371}]
["Wastage Rates - Default","Poor","Fair","Fair","Fair","Good","Industrial Products",{"$f":"LN(HLOOKUP(B52,$B$3:$E$8,2,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(C52,$B$3:$E$8,3,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(D52,$B$3:$E$8,4,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(E52,$B$3:$E$8,5,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(F52,$B$3:$E$8,6,FALSE))^2","v":3.3241150071771211E-2},2.3804801196801307E-3,{"$f":"EXP(SQRT(SUM(H52:M52)))","v":1.6400080773205654}]
[]
["Use ","Poor","Fair","Fair","Fair","Fair","Activity Data",{"$f":"LN(HLOOKUP(B54,$B$3:$E$8,2,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(C54,$B$3:$E$8,3,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(D54,$B$3:$E$8,4,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(E54,$B$3:$E$8,5,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(F54,$B$3:$E$8,6,FALSE))^2","v":0.16440195389316542},0,{"$f":"EXP(SQRT(SUM(H54:M54)))","v":1.842557020160978}]
["End of life","Poor","Poor","Poor","Poor","Poor","Activity Data",{"$f":"LN(HLOOKUP(B55,$B$3:$E$8,2,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(C55,$B$3:$E$8,3,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(D55,$B$3:$E$8,4,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(E55,$B$3:$E$8,5,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(F55,$B$3:$E$8,6,FALSE))^2","v":0.48045301391820139},0,{"$f":"EXP(SQRT(SUM(H55:M55)))","v":2.5163566012590954}]

{"sheet":"DATA ------------>","index":6,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[[1,1,24,11]]}
[]
[null,"DATA"]

{"sheet":"User Defined Excipient EFs","index":7,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
[]
[]
["Excipient Name","Default Uncertainty","User Defined Emission Factor (kg CO2e/kg)","Precision","Completeness","Temporal representativeness","Geographical representativeness","Technological representativeness","Basic","(ln(UEF))2","PLEASE SPECIFY THE DATA QUALITY INDICATORS FOR THIS EXCIPIENT"]
["Dicalcium phosphate",{"$f":"'Original Excipient EFs'!R2","v":2.2975193001530365},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D4,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E4,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F4,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G4,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H4,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I4,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},{"$f":"IF(C4<>\"\",IF(COUNTBLANK(D4:I4)>0,$K$3,\"\"),\"\")","v":""}]
["Microcrystalline cellulose",{"$f":"'Original Excipient EFs'!R3","v":1.6288573719223725},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D5,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E5,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F5,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G5,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H5,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I5,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},{"$f":"IF(C5<>\"\",IF(COUNTBLANK(D5:I5)>0,$K$3,\"\"),\"\")","v":""}]
["Lactose",{"$f":"'Original Excipient EFs'!R4","v":1.5994360002076888},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D6,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E6,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F6,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G6,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H6,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I6,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Mannitol",{"$f":"'Original Excipient EFs'!R5","v":2.2975193001530365},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D7,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E7,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F7,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G7,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H7,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I7,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Hydroxyypropylmethylcellulose",{"$f":"'Original Excipient EFs'!R6","v":1.6400080773205654},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D8,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E8,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F8,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G8,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H8,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I8,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Croscarmellose sodium",{"$f":"'Original Excipient EFs'!R7","v":2.1145724882592707},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D9,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E9,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F9,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G9,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H9,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I9,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Sodium starch glycolate",{"$f":"'Original Excipient EFs'!R8","v":2.2975193001530365},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D10,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E10,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F10,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G10,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H10,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I10,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Polyvinylpyrollidone",{"$f":"'Original Excipient EFs'!R9","v":2.2975193001530365},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D11,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E11,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F11,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G11,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H11,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I11,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Silicon dioxide",{"$f":"'Original Excipient EFs'!R10","v":1.6400080773205654},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D12,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E12,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F12,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G12,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H12,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I12,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Magnesium stearate",{"$f":"'Original Excipient EFs'!R11","v":2.1145724882592707},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D13,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E13,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F13,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G13,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H13,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I13,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Polyethyleneglycol",{"$f":"'Original Excipient EFs'!R12","v":2.3067731951631236},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D14,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E14,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F14,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G14,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H14,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I14,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Isopropyl alcohol",{"$f":"'Original Excipient EFs'!R13","v":1.1724429938968242},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D15,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E15,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F15,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G15,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H15,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I15,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Ethanol",{"$f":"'Original Excipient EFs'!R14","v":1.2737590597901596},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D16,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E16,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F16,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G16,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H16,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I16,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Purified water",{"$f":"'Original Excipient EFs'!R15","v":1.2737590597901596},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D17,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E17,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F17,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G17,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H17,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I17,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Gelatin",{"$f":"'Original Excipient EFs'!R16","v":2.3067731951631236},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D18,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E18,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F18,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G18,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H18,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I18,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Talc",{"$f":"'Original Excipient EFs'!R17","v":1.651081863442978},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D19,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E19,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F19,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G19,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H19,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I19,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Avicel",{"$f":"'Original Excipient EFs'!R18","v":1.651081863442978},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D20,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E20,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F20,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G20,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H20,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I20,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Colloidal anhydrous silica (collodial silicon dioxide, Cab-o-sil-M-5P)",{"$f":"'Original Excipient EFs'!R19","v":1.651081863442978},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D21,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E21,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F21,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G21,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H21,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I21,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Low substituted Hydroxypropylcellulose (L-HPC)",{"$f":"'Original Excipient EFs'!R20","v":1.856218788774791},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D22,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E22,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F22,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G22,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H22,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I22,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Opaglos 2 blue 97W90646",{"$f":"'Original Excipient EFs'!R21","v":2.3067731951631236},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D23,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E23,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F23,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G23,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H23,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I23,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Paraffin / Wax",{"$f":"'Original Excipient EFs'!R22","v":1.2737590597901596},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D24,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E24,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F24,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G24,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H24,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I24,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Potato starch",{"$f":"'Original Excipient EFs'!R23","v":1.2737590597901596},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D25,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E25,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F25,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G25,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H25,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I25,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Pregelatinised starch (Starch 1500)",{"$f":"'Original Excipient EFs'!R24","v":1.5458266020425071},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D26,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E26,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F26,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G26,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H26,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I26,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Red Ferric Oxide",{"$f":"'Original Excipient EFs'!R25","v":1.5458266020425071},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D27,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E27,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F27,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G27,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H27,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I27,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Sugar from sugar Cane",{"$f":"'Original Excipient EFs'!R26","v":1.2089750740786649},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D28,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E28,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F28,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G28,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H28,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I28,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Sugar from sugarbeet",{"$f":"'Original Excipient EFs'!R27","v":1.2737590597901596},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D29,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E29,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F29,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G29,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H29,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I29,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Yellow Ferric Oxide",{"$f":"'Original Excipient EFs'!R28","v":1.5458266020425071},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D30,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E30,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F30,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G30,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H30,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I30,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
["Zinc Oxide",{"$f":"'Original Excipient EFs'!R29","v":1.2737590597901596},null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D31,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E31,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F31,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G31,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H31,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I31,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D32,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E32,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F32,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G32,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H32,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I32,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D33,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E33,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F33,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G33,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H33,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I33,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D34,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E34,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F34,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G34,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H34,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I34,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D35,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E35,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F35,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G35,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H35,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I35,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D36,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E36,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F36,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G36,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H36,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I36,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D37,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E37,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F37,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G37,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H37,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I37,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D38,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E38,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F38,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G38,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H38,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I38,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D39,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E39,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F39,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G39,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H39,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I39,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D40,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E40,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F40,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G40,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H40,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I40,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D41,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E41,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F41,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G41,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H41,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I41,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D42,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E42,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F42,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G42,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H42,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I42,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D43,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E43,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F43,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G43,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H43,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I43,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D44,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E44,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F44,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G44,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H44,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I44,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D45,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E45,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F45,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G45,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H45,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I45,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D46,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E46,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F46,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G46,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H46,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I46,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D47,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E47,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F47,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G47,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H47,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I47,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D48,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E48,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F48,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G48,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H48,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I48,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(LN(HLOOKUP(D49,'Data Quality Matrix'!$B$3:$E$8,2,0))^2+LN(HLOOKUP(E49,'Data Quality Matrix'!$B$3:$E$8,3,0))^2+LN(HLOOKUP(F49,'Data Quality Matrix'!$B$3:$E$8,4,0))^2+LN(HLOOKUP(G49,'Data Quality Matrix'!$B$3:$E$8,5,0))^2+LN(HLOOKUP(H49,'Data Quality Matrix'!$B$3:$E$8,6,0))^2+LN(VLOOKUP(I49,'Data Quality Matrix'!$A$12:$B$20,2,0))^2,\"\")","v":""},""]

{"sheet":"Original Excipient EFs","index":8,"n_rows":47,"n_cols":18,"rows_kept":47,"cut":false,"hidden":true,"merged":[]}
["Excipient Name","Original Emission Factor (PUT UNIT HERE)","User Defined Emission Factor (PUT UNIT HERE)","Source","Note","Precision","Completeness","Temporal representativeness","Geographical representativeness","Technological representativeness","Basic","Precision","Completeness","Temporal representativeness","Geographical representativeness","Technological representativeness","Basic","U Total"]
["Dicalcium phosphate",1.86,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C4),FALSE,'User Defined Excipient EFs'!C4)","v":false},"Ecoinvent 2.2","inorganic chemichal","Poor","Fair","Fair","Fair","Poor","Industrial Products",{"$f":"LN(HLOOKUP(F2,DQM,2,FALSE))^2","v":0.16440195389316542},{"$f":"LN(HLOOKUP(G2,DQM,3,FALSE))^2","v":9.0840303743327487E-3},{"$f":"LN(HLOOKUP(H2,DQM,4,FALSE))^2","v":3.3241150071771211E-2},{"$f":"LN(HLOOKUP(I2,DQM,5,FALSE))^2","v":2.3804801196801307E-3},{"$f":"LN(HLOOKUP(J2,DQM,6,FALSE))^2","v":0.48045301391820139},{"$f":"LN(VLOOKUP(K2,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},{"$f":"EXP(SQRT(SUM(L2:Q2)))","v":2.2975193001530365}]
["Microcrystalline cellulose",4.2119999999999997,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C5),FALSE,'User Defined Excipient EFs'!C5)","v":false},"Ecoinvent 2.2","carboxymethyl cellulose, powder, at plant","Fair","Good","Fair","Fair","Fair","Industrial Products",3.3241150071771211E-2,2.3804801196801307E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K3,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},{"$f":"EXP(SQRT(SUM(L3:Q3)))","v":1.6288573719223725}]
["Lactose",9,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C6),FALSE,'User Defined Excipient EFs'!C6)","v":false},"CT",null,"Poor","Good","Good","Poor","Good","Industrial Products",0.16440195389316542,2.3804801196801307E-3,9.0840303743327487E-3,9.0840303743327487E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K4,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.5994360002076888]
["Mannitol",1.899,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C7),FALSE,'User Defined Excipient EFs'!C7)","v":false},"Ecoinvent 2.2","chemicals organic, at plant","Poor","Fair","Fair","Fair","Poor","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K5,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.2975193001530365]
["Hydroxyypropylmethylcellulose",2.8,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C8),FALSE,'User Defined Excipient EFs'!C8)","v":false},"FPX 3.3","Methyl Ethyl HydroxyEthyl Cellulose (MEHEC)","Fair","Fair","Fair","Fair","Fair","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K6,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.6400080773205654]
["Croscarmellose sodium",4.2119999999999997,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C9),FALSE,'User Defined Excipient EFs'!C9)","v":false},"Ecoinvent 2.2","carboxymethyl cellulose, powder, at plant","Fair","Fair","Fair","Fair","Poor","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K7,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.1145724882592707]
["Sodium starch glycolate",1.8985000000000001,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C10),FALSE,'User Defined Excipient EFs'!C10)","v":false},"Ecoinvent 2.2","chemicals organic, at plant","Poor","Fair","Fair","Fair","Poor","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K8,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.2975193001530365]
["Polyvinylpyrollidone",1.8985000000000001,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C11),FALSE,'User Defined Excipient EFs'!C11)","v":false},"Ecoinvent 2.2","chemicals organic, at plant","Poor","Fair","Fair","Fair","Poor","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K9,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.2975193001530365]
["Silicon dioxide",2.1000000000000001E-2,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C12),FALSE,'User Defined Excipient EFs'!C12)","v":false},"Ecoinvent 2.2","silica sand, at plant","Fair","Fair","Fair","Fair","Fair","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K10,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.6400080773205654]
["Magnesium stearate",0.74679896834074577,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C13),FALSE,'User Defined Excipient EFs'!C13)","v":false},"Ecoinvent 2.2","Nearest neighbor - tallow","Fair","Fair","Fair","Fair","Poor","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,2.3804801196801307E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K11,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.1145724882592707]
["Polyethyleneglycol",2.1,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C14),FALSE,'User Defined Excipient EFs'!C14)","v":false},"CT derivation from Ecoinvent data",null,"Poor","Fair","Fair","Poor","Poor","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K12,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.3067731951631236]
["Isopropyl alcohol",1.8487,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C15),FALSE,'User Defined Excipient EFs'!C15)","v":false},"Ecoinvent 2.2","isopropanol, at plant","Good","Good","Good","Fair","Very Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,0,{"$f":"LN(VLOOKUP(K13,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.1724429938968242]
["Ethanol",1.248,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C16),FALSE,'User Defined Excipient EFs'!C16)","v":false},"Ecoinvent 2.2","ethanol from ethylene","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K14,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2737590597901596]
["Purified water",6.8000000000000005E-4,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C17),FALSE,'User Defined Excipient EFs'!C17)","v":false},"Ecoinvent 2.2","water, ultrapure, at plant","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K15,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2737590597901596]
["Gelatin",1.8985000000000001,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C18),FALSE,'User Defined Excipient EFs'!C18)","v":false},"Ecoinvent 2.2","very poor proxy","Poor","Fair","Fair","Poor","Poor","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K16,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.3067731951631236]
["Talc",1.5980000000000001,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C19),FALSE,'User Defined Excipient EFs'!C19)","v":false},"Ecoinvent","colloidal anhydrous silica","Fair","Fair","Fair","Poor","Fair","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K17,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.651081863442978]
["Avicel",4.2122000000000002,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C20),FALSE,'User Defined Excipient EFs'!C20)","v":false},"Ecoinvent","carboxymethyl cellulose, powder, at plant","Fair","Fair","Fair","Poor","Fair","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K18,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.651081863442978]
["Colloidal anhydrous silica (collodial silicon dioxide, Cab-o-sil-M-5P)",1.5984651599723501,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C21),FALSE,'User Defined Excipient EFs'!C21)","v":false},"Ecoinvent","sodium silicate","Fair","Fair","Fair","Poor","Fair","Industrial Products",3.3241150071771211E-2,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K19,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.651081863442978]
["Low substituted Hydroxypropylcellulose (L-HPC)",4.2119999999999997,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C22),FALSE,'User Defined Excipient EFs'!C22)","v":false},"Ecoinvent","carboxymethyl cellulose, powder, at plant","Poor","Fair","Fair","Poor","Fair","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K20,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.856218788774791]
["Opaglos 2 blue 97W90646",0.82913999999999999,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C23),FALSE,'User Defined Excipient EFs'!C23)","v":false},"Ecoinvent","Paraffin used.  Opaglos contains ethanol, shellac, wax","Poor","Fair","Fair","Poor","Poor","Industrial Products",0.16440195389316542,9.0840303743327487E-3,3.3241150071771211E-2,9.0840303743327487E-3,0.48045301391820139,{"$f":"LN(VLOOKUP(K21,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},2.3067731951631236]
["Paraffin / Wax",0.82913999999999999,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C24),FALSE,'User Defined Excipient EFs'!C24)","v":false},"Ecoinvent","paraffin, at plant","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K22,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2737590597901596]
["Potato starch",0.71760000000000002,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C25),FALSE,'User Defined Excipient EFs'!C25)","v":false},"Ecoinvent","potato starch, at plant","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K23,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2737590597901596]
["Pregelatinised starch (Starch 1500)",2.016,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C26),FALSE,'User Defined Excipient EFs'!C26)","v":false},"Ecoinvent","modified starch, at plant","Good","Good","Good","Fair","Fair","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K24,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.5458266020425071]
["Red Ferric Oxide",3.1189000000000001E-2,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C27),FALSE,'User Defined Excipient EFs'!C27)","v":false},"Ecoinvent","portafer, at plant","Good","Good","Good","Fair","Fair","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K25,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.5458266020425071]
["Sugar from sugar Cane",0.3,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C28),FALSE,'User Defined Excipient EFs'!C28)","v":false},"FPX 3.3","sugar, from sugarcane, at sugar refinery","Very Good","Very Good","Very Good","Good","Good","Industrial Products",0,0,0,3.921440478314025E-4,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K26,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2089750740786649]
["Sugar from sugarbeet",0.50700000000000001,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C29),FALSE,'User Defined Excipient EFs'!C29)","v":false},"Ecoinvent","sugar, from sugar beet, at sugar refinery","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K27,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2737590597901596]
["Yellow Ferric Oxide",3.1189000000000001E-2,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C30),FALSE,'User Defined Excipient EFs'!C30)","v":false},"Ecoinvent","portafer, at plant","Good","Good","Good","Fair","Fair","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,0.16440195389316542,{"$f":"LN(VLOOKUP(K28,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.5458266020425071]
["Zinc Oxide",2.8889,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C31),FALSE,'User Defined Excipient EFs'!C31)","v":false},"Ecoinvent","zinc oxide, at plant","Good","Good","Good","Fair","Good","Industrial Products",9.0840303743327487E-3,2.3804801196801307E-3,9.0840303743327487E-3,2.3804801196801307E-3,3.3241150071771211E-2,{"$f":"LN(VLOOKUP(K29,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":2.3804801196801307E-3},1.2737590597901596]
[{"$f":"'User Defined Excipient EFs'!A32","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C32),FALSE,'User Defined Excipient EFs'!C32)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K30,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A33","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C33),FALSE,'User Defined Excipient EFs'!C33)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K31,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A34","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C34),FALSE,'User Defined Excipient EFs'!C34)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K32,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A35","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C35),FALSE,'User Defined Excipient EFs'!C35)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K33,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A36","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C36),FALSE,'User Defined Excipient EFs'!C36)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K34,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A37","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C37),FALSE,'User Defined Excipient EFs'!C37)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K35,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A38","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C38),FALSE,'User Defined Excipient EFs'!C38)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K36,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A39","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C39),FALSE,'User Defined Excipient EFs'!C39)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K37,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A40","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C40),FALSE,'User Defined Excipient EFs'!C40)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K38,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A41","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C41),FALSE,'User Defined Excipient EFs'!C41)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K39,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A42","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C42),FALSE,'User Defined Excipient EFs'!C42)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K40,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A43","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C43),FALSE,'User Defined Excipient EFs'!C43)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K41,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A44","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C44),FALSE,'User Defined Excipient EFs'!C44)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K42,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A45","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C45),FALSE,'User Defined Excipient EFs'!C45)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K43,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A46","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C46),FALSE,'User Defined Excipient EFs'!C46)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K44,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A47","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C47),FALSE,'User Defined Excipient EFs'!C47)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K45,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A48","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C48),FALSE,'User Defined Excipient EFs'!C48)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K46,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[{"$f":"'User Defined Excipient EFs'!A49","v":0},false,{"$f":"IF(ISBLANK('User Defined Excipient EFs'!C49),FALSE,'User Defined Excipient EFs'!C49)","v":false},null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"LN(VLOOKUP(K47,'Data Quality Matrix'!$A$12:$B$22,2,FALSE))^2","v":{"$error":"#N/A"}},{"$error":"#N/A"}]

{"sheet":"Reference Data","index":9,"n_rows":101,"n_cols":5,"rows_kept":101,"cut":false,"hidden":true,"merged":[[59,0,60,0],[59,1,59,3],[59,4,60,4],[39,1,39,3],[39,4,40,4],[39,0,40,0],[49,0,50,0],[49,1,49,3],[49,4,50,4]]}
["APIs"]
[]
["Type of API Emission Factors (for dropdown)"]
[" ","<----This row intentionally blank"]
["Specific"]
["Calculated"]
["High/Medium/Low"]
["Average"]
[]
["High/Medium/Low API Emission Factors"]
[]
["Low",600,"kg CO2e/kg"]
["Medium",1500,"kg CO2e/kg"]
["High",7000,"kg CO2e/kg"]
[]
["Average API Emission Factors"]
[]
["Average Factor",1500,"kg CO2e/kg"]
[]
["FORMULATION"]
[]
["Electricity requirement (kWh per kg of tablet):",14.31]
["Gas requirement (kWh per kg of tablet):",14.4]
[]
["PACKAGING"]
[]
["Electricity requirement (kWh per kg of tablet):",11.45]
["Gas requirement (kWh per kg of tablet):",11.52]
[]
[]
["DEFAULT PACKAGING"]
[]
["Summary:"]
[]
["Total Weight per tablet (mg):",{"$f":"IF(WasteDefault=\"Small\",SUM('Reference Data'!E42:E46),IF(WasteDefault=\"Medium\",SUM(E52:E56),IF(WasteDefault=\"Large\",SUM(E62:E66),\"\")))","v":{"$error":"#DIV/0!"}}]
[]
[]
["Small:"]
[]
["Material","Quantites per tablet (g)",null,null,"Total weight per tablet (mg)"]
[null,"Blister","Retail","Outer"]
["PVC - blister",1.486,null,null,{"$f":"SUM(B42:D42)*1000","v":1486}]
["PVdC - blister",0.17799999999999999,null,null,{"$f":"SUM(B43:D43)*1000","v":178}]
["Aluminium",0.23899999999999999,null,null,{"$f":"SUM(B44:D44)*1000","v":239}]
["Paper",null,{"$f":"4/TabletsPerPack","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(B45:D45)*1000","v":{"$error":"#DIV/0!"}}]
["Cardboard",null,{"$f":"10.56/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"195/(TabletsPerPack*30)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B46:D46)*1000","v":{"$error":"#DIV/0!"}}]
[]
["Medium:"]
[]
["Material","Quantites per tablet (g)",null,null,"Total weight per tablet (mg)"]
[null,"Blister","Retail","Outer"]
["PVC - blister",2.351,null,null,{"$f":"SUM(B52:D52)*1000","v":2351}]
["PVdC - blister",0.28199999999999997,null,null,{"$f":"SUM(B53:D53)*1000","v":282}]
["Aluminium",0.377,null,null,{"$f":"SUM(B54:D54)*1000","v":377}]
["Paper",null,{"$f":"6/TabletsPerPack","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(B55:D55)*1000","v":{"$error":"#DIV/0!"}}]
["Cardboard",null,{"$f":"13.56/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"195/(TabletsPerPack*30)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B56:D56)*1000","v":{"$error":"#DIV/0!"}}]
[]
["Large:"]
[]
["Material","Quantites per tablet (g)",null,null,"Total weight per tablet (mg)"]
[null,"Blister","Retail","Outer"]
["PVC - blister",3.6339999999999999,null,null,{"$f":"SUM(B62:D62)*1000","v":3634}]
["PVdC - blister",0.436,null,null,{"$f":"SUM(B63:D63)*1000","v":436}]
["Aluminium",0.58299999999999996,null,null,{"$f":"SUM(B64:D64)*1000","v":583}]
["Paper",null,{"$f":"12/TabletsPerPack","v":{"$error":"#DIV/0!"}},null,{"$f":"SUM(B65:D65)*1000","v":{"$error":"#DIV/0!"}}]
["Cardboard",null,{"$f":"24.8/TabletsPerPack","v":{"$error":"#DIV/0!"}},{"$f":"195/(TabletsPerPack*30)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(B66:D66)*1000","v":{"$error":"#DIV/0!"}}]
[]
[]
["USE (PLASTIC CUP FOR NHS, PAPER BAG + LABEL FOR PHARMACY)"]
[]
["NHS:"]
[]
["Material","PP - bottle"]
["Mass per cup",4.0000000000000001E-3,"kg"]
["Avg. tablets per cup",2]
[]
["Pharmacy:"]
[]
["Paper bag weight",1.2E-2,"kg"]
["Paper label weight",{"$f":"0.05*0.08*0.1*2","v":8.0000000000000004E-4},"kg"]
[]
["DEFAULT SALES SPLIT"]
[]
["NHS hospital",0.3]
["Other hospital",0.1]
["Pharmacy (NHS prescription)",0.5]
["Pharmacy (non-NHS)/retail",0.1]
[]
["DEFAULT WASTAGE RATES"]
[]
["Formulation Site 1 - Process Wastage",0.02]
["Formulation Site 2 - Process Wastage",0.02]
["% Product lost during packaging",5.0000000000000001E-3]
["% Packaging lost during packaging",2.5000000000000001E-2]
["RDC Wastage",0.02]
[]
["DEFAULT PACKAGING SPLIT"]
[]
["Default Blisters Per Retail Pack:",4]
["Default retail packs per outer box:",50]
["Default outer boxes per pallet:",200]

{"sheet":"FPX Reference Data","index":10,"n_rows":1384,"n_cols":28,"rows_kept":1384,"cut":false,"hidden":true,"merged":[]}
["Core Data Details","Footprint Expert Reference Database 3.3",null,null,null,null,null,"Intrinsic Data Quality ","Data Application Information",null,null,null,"Data Intrinsic  Information",null,null,null,null,null,null,"PAS 2050 Compliancy Information"]
["Data Group","Unique Name",null,"Number","Units","Technical scope","Data type","Intrinsic data quality grade","Geographical Area","Data Source Date","Date Collection End Period ","Technology/method/notes","Accuracy","Representativeness","Consistency","Reproducibility","Data source organisation","Data source publication","Source Author","Boundaries criteria ","Cut off ","Allocation principle","Allocation type","Offsetting included","GHGs included and GWP","Biogenic carbon treatment","Biogenic carbon storage","Land use change"]
["Biodegradability Rates","Degradability rate  -Card packaging",null,0.64,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Composted Organic Material",null,0.56999999999999995,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Incinerator Ash",null,0.56999999999999995,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Liquid Cartons",null,0.64,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Non-degradable (e.g. plastics)",null,0,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Other Card",null,0.64,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Other misc. combustibles",null,0.5,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Other Paper",null,0.98,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Textiles",null,0.5,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Biodegradability Rates","Degradability rate  -Wood",null,0.75,"%","N/A","Activity Data","B","EU",2002,2001,"Calculated using existing literature","Calculated","Medium","High","Medium","Golders Associates, Environment Agency and Land Quality Management Ltd","Development of a landfill gas risk assessment model: GasSim","Golders Associates, Environment Agency and Land Quality Management Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Absorbent hygiene",null,0.14799999999999999,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - aggregates/minerals",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Biogenic Carbon Content - WEEE",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Combustion residues",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - ELVs",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Fines",null,6.9000000000000006E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Glass",null,3.0000000000000001E-3,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Green/Plant Waste",null,0.17199999999999999,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Inorganic Chemicals",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Inorganic Sludges",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Kitchen/Food Waste",null,0.13500000000000001,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Mixed Chemicals",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Oils/Fuels",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Organic Chemicals",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Organic Sludges",null,0.309,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - other non combustibles",null,3.5000000000000003E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Other organic waste",null,0.13500000000000001,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Paper and Card",null,0.31900000000000001,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Plastic (dense)",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Plastics (film)",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Silt/soil",null,7.0000000000000007E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Textiles",null,0.19899999999999998,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Tyres",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Biogenic Carbon Content - Wood",null,0.43799999999999994,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Absorbent hygiene",null,3.6999999999999998E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - aggregates/minerals",null,7.0000000000000007E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Combustion residues",null,7.0000000000000007E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - ELVs",null,0.158,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Fines",null,6.9000000000000006E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Glass",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Green/Plant Waste",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Inorganic Chemicals",null,0.38400000000000001,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Inorganic Sludges",null,0.309,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Kitchen/Food Waste",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Mixed Chemicals",null,0.38400000000000001,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Oils/Fuels",null,0.80400000000000005,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Organic Chemicals",null,0.38400000000000001,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - other non combustibles",null,3.5000000000000003E-2,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Other organic waste",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Paper and Card",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Plastic (dense)",null,0.54799999999999993,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Plastics (film)",null,0.47799999999999998,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Silt/soil",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Textiles",null,0.19899999999999998,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Tyres",null,0.74,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - WEEE",null,0.158,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Content - Wood",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Carbon Contents","Fossil Carbon Contents - Organic Sludges",null,0,"%","N/A","Activity Data","B","EU",2006,2005,"Study using surveys/sampling","Calculated","Medium","High","Medium","ERM, Golders Associates ","Carbon Balances and Energy impacts of the Management of UK wastes","ERM and Golders Associates","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Chemicals","Acetic acid - from conventional petrochemicals ",null,1.8,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Acetone ",null,2.2000000000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Acetone cyanohydrin ",null,3.8,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Acrylic acid - from conventional petrochemicals ",null,1.7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Acrylonitrile ",null,3.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Adipic acid - from conventional petrochemicals ",null,4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Alamine",null,1.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Ammonia",null,2.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Ammonium Bicarbonate",null,0.69,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"Based on case study","Calculated","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Chemicals","Benzene ",null,1.8,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Butadiene",null,1.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Butanol  - from conventional petrochemicals ",null,1.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Butenes - mixed",null,1.5,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Calcium oxide - CaO (from calcium carbonate)",null,1.0900000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Caprolactam - from conventional petrochemicals ",null,5.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Chlorine",null,0.79,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Concrete Release Agent - mineral Oil-Based ",null,0.45200000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Environmental Assessment Tool for Biomaterials ","National Non-Food Crops Centre and North Energy","Custom definition","Unknown","Organisational specific","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Concrete Release Agent - spent Biolubricant ",null,8.7999999999999995E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Environmental Assessment Tool for Biomaterials ","National Non-Food Crops Centre and North Energy","Custom definition","Unknown","Organisational specific","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Concrete Release Agent - vegetable Oil-Based ",null,1.952,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Environmental Assessment Tool for Biomaterials ","National Non-Food Crops Centre and North Energy","Custom definition","Unknown","Organisational specific","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Dextrose",null,0.43,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"Based on case study","Calculated","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Chemicals","Di (2-ethylhexyl) phthalate (DEHP) ",null,1.99,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2001,2000,"8 industrial companies manufacturing intermediates and/or high commodity phthalate esters in Europe","Calculated","High","High","Medium","The European Council for Plasticisers and Intermediates (ECPI)","Eco-profile of high volume commodity phthalate esters (DEHP/DINP/DIDP)","ECPI","ISO 14000 series","PAS 2050","PAS 2050","System expansion","No","PAS 2050","Unknown","Unknown","PAS 2050"]
["Chemicals","Diammonium phosphate - 21% conc.",null,6.0600000000000001E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","National Non-Food Crops Centre and North Energy","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Diphenylmethane diisocyanate (MDI)",null,3.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 series","PAS 2050","No","None","No","PAS 2050","Unknown","No","No"]
["Chemicals","Enzyme Alpha Amylase ",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Enzyme AMG",null,2.25,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Ethanol - from conventional petrochemicals ",null,2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Ethyl benzene ",null,1.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Ethylene dichloride ",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Glycerine",null,2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"Based on case study","Calculated","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Chemicals","High-fructose corn syrup (HFCS) ",null,2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"Based on case study","Calculated","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Chemicals","Hydrogen - cracker",null,1.7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Hydrogen - electrolytic ",null,0.95,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Hydrogen - from natural gas",null,1.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Hydrogen - reformer",null,7.5,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Hydrogen chloride",null,1.5,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Hydrogen cyanide",null,7.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Methyl Ethyl HydroxyEthyl Cellulose (MEHEC)",null,2.8,"kg CO2(e)/kg","Cradle to RDC","Emission Factor","A","SWE",2005,2005,"Company specific processes and technologies","Calculated","Medium","High","Medium","International Environment Product Declaration System","Certified Environmental Product Declaration (EPD) MEHEC","Cellulosic Specialties","ISO 14000 series","PAS 2050","Organisational specific","economic","No","Kyoto gases only","Unknown","No","Unknown"]
["Chemicals","Methyl methacrylate (MMA) ",null,6.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Nitrogen ",null,8.8319763035372839E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Nitrogen; via cryogenic air separation; production mix, at plant; gaseous  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Octanol ",null,1.2992300000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Oxygen ",null,0.14719960505895505,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Oxygen; via cryogenic air separation; production mix, at plant; gaseous  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Pentane",null,1.1000000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Phenol",null,2.2000000000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Phenol-resorinol-formaldehyde",null,4.09,"kg CO2/kg","Cradle to Gate","Emission Factor","A","USA",2004,2003,"Survey/study of existing technologies and production processes at time","Calculated","Medium","High","Medium","National Renewable Energy Laboratory ","U.S. Life-Cycle Inventory (LCI) Database ","Maureen E. Puettman","Custom definition","PAS 2050","No","None","No","Kyoto gases only","Unknown","No","Unknown"]
["Chemicals","Polylactic acid - from conventional petrochemicals  ",null,2.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Polyols",null,3.5,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Propanediol - from conventional petrochemicals3 ",null,4.4000000000000004,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Sodium chlorate",null,8.5999999999999993E-2,"kg CO2(e)/kg","Cradle to RDC","Emission Factor","A","SWE",2007,2007,"Company specific processes and technologies","Calculated","Medium","High","Medium","International Environment Product Declaration System","Certified Environmental Product Declaration (EPD) for Sodium chlorate (NaClO3)","AkzoNobel","ISO 14000 series","PAS 2050","Organisational specific","economic","No","Kyoto gases only","Unknown","No","Unknown"]
["Chemicals","Sodium hydroxide",null,1.4,"kg CO2/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 series","PAS 2050","No","None","No","PAS 2050","Unknown","No","No"]
["Chemicals","Styrene",null,3.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Succinic acid - from conventional petrochemicals2 ",null,7.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2006,2004,"Survey/study of average technologies and production processes at time","Calculated","Medium","Medium","Low","European Commission, Utrecht University","Medium and Long-term Opportunities and Risks of the Biotechnological Production of Bulk Chemicals from Renewable Resources","Dr. Martin Patel et al.","Custom definition","PAS 2050","Unknown","unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Sulphur ",null,0.55027728528584607,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Sulphur; from crude oil; consumption mix, at refinery; elemental sulphur  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Sulphuric acid (93% conc.) ",null,0.1368096,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Chemicals","Terephthalic acid",null,2.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Titanium dioxide (TiO2)",null,4.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2004,"ILCD Database","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Chemicals","Tolylene diisocyanate (TDI)",null,6.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Chemicals","Vinyl chloride",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Distribution","Average Buildings Emissions - high rise offices, almost always  air-conditioned - UK",null,0.15365949119373778,"kg CO2(e)/m2 floor space/day","Gate to Gate","Emission Factor","B","GBR",2007,2006,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from UK Green Building Council","Calculated","Medium","Medium","High","UK Green Building Council","Report on Carbon Reductions in New Non-Domestic Buildings","UK Green Building Council","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","Unknown","Unknown","Unknown"]
["Distribution","Average Buildings Emissions - low rise offices, hospitals, education and numerous uses - UK",null,8.9178082191780833E-2,"kg CO2(e)/m2 floor space/day","Gate to Gate","Emission Factor","B","GBR",2007,2006,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from UK Green Building Council","Calculated","Medium","Medium","High","UK Green Building Council","Report on Carbon Reductions in New Non-Domestic Buildings","UK Green Building Council","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","Unknown","Unknown","Unknown"]
["Distribution","Average Buildings Emissions - Warehouses,  factories,  various large and out of town retail - UK",null,3.4794520547945205E-2,"kg CO2(e)/m2 floor space/day","Gate to Gate","Emission Factor","B","GBR",2007,2006,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from UK Green Building Council","Calculated","Medium","Medium","High","UK Green Building Council","Report on Carbon Reductions in New Non-Domestic Buildings","UK Green Building Council","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","Unknown","Unknown","Unknown"]
["Distribution","Average Number of containers per create (for 1 pint glass bottle) - UK",null,20,"containers","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average Number of containers per pallet (for 1 litre carton gable-top) - UK",null,160,"containers","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average Number of containers per pallet (for 1 litre carton screw-cap) - UK",null,160,"containers","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average Number of containers per pallet (for 1 litre PET bottle) - UK",null,160,"containers","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average Number of containers per pallet (for 2 pint HDPE container) - UK",null,140,"containers","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average Number of times crate is reused - UK",null,120,"times","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average Number of times pallet is reused - UK",null,500,"times","N/A","activity data","A","GBR",2010,2009,"Estimation based on official waste data","Estimation","Medium","High","Medium","Waste & Resources Action Programme (WRAP)","WRAP (2009): Household Food and Drink Waste in the UK, WRAP (2010): Lifecycle assessment of example packaging systems for milk","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Distribution","Average RDC Emissions - apples - UK",null,8.412468444069076E-3,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO411","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - bread - UK",null,2.8041561480230254E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO414","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - cheese - UK",null,8.2184521749324863E-3,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO408","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - fresh meat - UK",null,1.3741252036487118E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO405","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - frozen chips - UK",null,8.0567681358611115E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO410","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - frozen peas - UK",null,8.951964595401235E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO409","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - milk - UK ",null,1.1451043363739264E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO407","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - potatoes - UK",null,6.3093513330518079E-3,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO412","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - ready meals - UK",null,8.2501305711217776E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO406","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Distribution","Average RDC Emissions - strawberries - UK",null,6.6063711713880369E-2,"kg CO2(e)/kg","Gate to Gate","Emission Factor","A","GBR",2008,2007,"Footprint Expert calculated emission factor using the RDC Calculator and average activity data from DEFRA","Calculated","High","High","High","DEFRA, Carbon Trust","Greenhouse Gas Impacts of Food Retailing, DEFRA Project Code FO413","Brunel University","PAS 2050","PAS 2050","N/A","N/A","No","PAS 2050","PAS 2050","N/A","N/A"]
["Electricity Factor","Electricity: Africa","Africa",0.80316686436332407,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AFR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Argentina ","Argentina ",0.45526411620061424,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ARG",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Asia subcontinent","Asia subcontinent",1.0297607981662982,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ASIA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Australia - Average","Australia",0.94311468112538599,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Austria","Austria",0.21546417949117885,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUT",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Bangladesh ","Bangladesh ",0.50245518334683592,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","BGD",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Belgium ","Belgium ",0.24912392964076877,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","BEL",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Brazil ","Brazil ",0.12122377676853034,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","BRA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Bulgaria ","Bulgaria ",0.67600000000000005,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","BGR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Canada ","Canada ",0.25293451262011962,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","CAN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Central/Eastern Europe","Central/Eastern Europe",0.60017180636069722,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EUR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Chile","Chile",0.61560489613670322,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","CHL",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: China ","China ",0.92572252578387915,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","CHN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Colombia ","Colombia ",0.13807841612635435,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","COL",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Costa Rica ","Costa Rica ",8.435468932578899E-2,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","CRI",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Cyprus","Cyprus",1.1379999999999999,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","CYP",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Czech Republic","Czech Republic",0.72158436407381588,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","CZE",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Denmark","Denmark",0.68575466673151053,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","DNK",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Ecuador ","Ecuador ",0.43753044941883518,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ECU",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Egypt","Egypt",0.585874632768563,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EGY",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: EU 27","EU 27",0.47902347686759716,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EUR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Finland ","Finland ",0.29174875259980648,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","FIN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: France ","France ",9.2389878208380238E-2,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","FRA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Germany ","Germany ",0.61081842333831415,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","DEU",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Greece ","Greece ",0.9162561150586952,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","GRC",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Guatemala ","Guatemala ",0.53521611652778678,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","GTM",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Hungary ","Hungary ",0.4310860312396308,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","HUN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: India ","India ",1.1062718177411439,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","IND",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Indonesia ","Indonesia ",0.94085938380060197,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","IDN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Ireland (Republic of) ","Ireland (Republic of) ",0.65083090694758816,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","IRL",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Israel ","Israel ",0.89110193595501563,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ISR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Italy ","Italy ",0.55194023109067192,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ITA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Japan ","Japan ",0.58291522464933065,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","JPN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Kenya ","Kenya ",0.36098801329356012,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","KEN",2009,2007,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Latin America","Latin America",0.30186278848713055,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","LA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Latvia","Latvia",0.39667696699999999,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","LVA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies.  Also remodelled to take into account the carbon intensity of electricity imported from neighbouring countries.","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Malaysia ","Malaysia ",0.61724873200984254,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","MYS",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Malta ","Malta ",1.3720000000000001,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","MLT",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Mexico ","Mexico ",0.63361143769442574,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","MEX",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Middle East","Middle East",0.81586297974212252,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","MIDDLE EAST",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Netherlands ","Netherlands ",0.58638920712314091,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","NLD",2009,2007,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: New Zealand ","New Zealand ",0.25194960630069796,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","NZL",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Non-OECD total","Non-OECD total",0.74062349345945278,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","NON-OECD",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: North America","North America",0.63040830522007596,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","NORTH AMERICA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Norway ","Norway ",1.049451093610587E-2,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","NOR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: OECD total","OECD total",0.59932853585096402,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","OECD",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Pakistan","Pakistan",0.67652328975166598,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","PAK",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Panama","Panama",0.46600000000000003,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","PAN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Peru","Peru",0.27300000000000002,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","PER",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Philippines","Philippines",0.58473205046650367,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","PHI",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Poland ","Poland ",1.1265149884162933,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","POL",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Portugal ","Portugal ",0.56127091783235894,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","PRT",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Romania ","Romania ",0.496,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ROM",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Russia ","Russia ",0.49537408766333174,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","RUS",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Saudi Arabia","Saudi Arabia",0.90863183112411028,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","KSA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Serbia ","Serbia ",0.9373146364651771,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","YUG",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2005, EcoInvent 2.0 and Dukes Digest 2008","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Singapore ","Singapore ",0.60870432695669041,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","SGP",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: South Africa ","South Africa ",1.1259417633769284,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ZAF",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: South East Asia","South East Asia",0.66763138680063705,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","SOUTH EAST ASIA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: South Korea ","South Korea ",0.62192540439278265,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","SKR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Spain ","Spain ",0.43454882554236196,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","ESP",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Sweden ","Sweden ",3.2146854099155187E-2,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","SWE",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Taiwan","Taiwan",0.76048098389302987,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","TWN",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Thailand","Thailand",0.59687316554555847,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","THA",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Turkey ","Turkey ",0.67771558519933239,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","TUR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Ukraine ","Ukraine ",0.51780516144323641,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","UKR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: United Arab Emirates (UAE)","United Arab Emirates (UAE)",0.53203149151847406,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","UAE",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: United Kingdom","United Kingdom",0.62832096455817366,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","GBR",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: US Average","US Average",0.6864438958828134,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2010,2008,"Calculated using US EPA grid mix data","Calculated","Medium","High","High","Carbon Trust, Digest of United Kingdom energy statistics (DUKES), US Environmental Protection Agency, EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007, EcoInvent 2.0 and Dukes Digest 2009","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: Vietnam ","Vietnam ",0.48502679726960557,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","VNM",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Electricity Factor","Electricity: World average","World average",0.65610773089884389,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","VNM",2010,2008,"Calculated using IEA fuel mixes, average fuel emissions (combustion and upstream), and accounting for transmission losses and average power plant efficiencies","Calculated","Medium","High","High","Carbon Trust, International Energy Agency, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["End of Life Fate","Average Municipal Compost Rate:  Austria",null,0.4,"%","N/A","Activity Data","A","AUT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Belgium",null,0.24,"%","N/A","Activity Data","A","BEL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Bulgaria",null,0,"%","N/A","Activity Data","A","BUL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Cyprus",null,0,"%","N/A","Activity Data","A","CYP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Czech Republic",null,0.02,"%","N/A","Activity Data","A","CZE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Denmark",null,0.18,"%","N/A","Activity Data","A","DNK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Estonia",null,0.08,"%","N/A","Activity Data","A","EST",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  EU 27",null,0.17,"%","N/A","Activity Data","A","EU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Finland",null,0.08,"%","N/A","Activity Data","A","FIN ",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  France",null,0.15,"%","N/A","Activity Data","A","FRA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Germany",null,0.17,"%","N/A","Activity Data","A","DEU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Greece",null,0.02,"%","N/A","Activity Data","A","GRC",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Hungary",null,0.02,"%","N/A","Activity Data","A","HUN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Ireland",null,0.03,"%","N/A","Activity Data","A","IRL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Italy",null,0.34,"%","N/A","Activity Data","A","ITA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Latvia",null,0.01,"%","N/A","Activity Data","A","LVA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Lithuania",null,0.01,"%","N/A","Activity Data","A","LIT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Luxembourg",null,0.2,"%","N/A","Activity Data","A","LUX",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Malta",null,0,"%","N/A","Activity Data","A","MLT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Netherlands",null,0.27,"%","N/A","Activity Data","A","NLD",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Poland",null,0.04,"%","N/A","Activity Data","A","POL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Portugal",null,0.08,"%","N/A","Activity Data","A","PRT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Romania",null,0,"%","N/A","Activity Data","A","ROM",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Slovakia",null,0.05,"%","N/A","Activity Data","A","SVK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Slovenia",null,0.02,"%","N/A","Activity Data","A","SVN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Spain",null,0.2,"%","N/A","Activity Data","A","ESP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  Sweden",null,0.13,"%","N/A","Activity Data","A","SWE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Compost Rate:  United Kingdom",null,0.12,"%","N/A","Activity Data","A","GBR",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Austria",null,0.27,"%","N/A","Activity Data","A","AUT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Belgium",null,0.36,"%","N/A","Activity Data","A","BEL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Bulgaria",null,0,"%","N/A","Activity Data","A","BUL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Cyprus",null,0,"%","N/A","Activity Data","A","CYP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Czech Republic",null,0.13,"%","N/A","Activity Data","A","CZE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Denmark",null,0.54,"%","N/A","Activity Data","A","DNK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Estonia",null,0,"%","N/A","Activity Data","A","EST",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  EU 27",null,0.2,"%","N/A","Activity Data","A","EU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Finland",null,0.17,"%","N/A","Activity Data","A","FIN ",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  France",null,0.32,"%","N/A","Activity Data","A","FRA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Germany",null,0.35,"%","N/A","Activity Data","A","DEU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Greece",null,0,"%","N/A","Activity Data","A","GRC",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Hungary",null,0.09,"%","N/A","Activity Data","A","HUN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Ireland",null,0.03,"%","N/A","Activity Data","A","IRL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Italy",null,0.11,"%","N/A","Activity Data","A","ITA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Latvia",null,0,"%","N/A","Activity Data","A","LVA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Lithuania",null,0,"%","N/A","Activity Data","A","LIT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Luxembourg",null,0.36,"%","N/A","Activity Data","A","LUX",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Malta",null,0,"%","N/A","Activity Data","A","MLT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Netherlands",null,0.39,"%","N/A","Activity Data","A","NLD",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Poland",null,0.01,"%","N/A","Activity Data","A","POL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Portugal",null,0.19,"%","N/A","Activity Data","A","PRT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Romania",null,0,"%","N/A","Activity Data","A","ROM",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Slovakia",null,0.1,"%","N/A","Activity Data","A","SVK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Slovenia",null,0.01,"%","N/A","Activity Data","A","SVN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Spain",null,0.09,"%","N/A","Activity Data","A","ESP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  Sweden",null,0.49,"%","N/A","Activity Data","A","SWE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Incineration Rate:  United Kingdom",null,0.1,"%","N/A","Activity Data","A","GBR",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Combined Landfill Rate: Australia",null,0.48,"%","N/A","Activity Data","A","AUS",2010,2007,"National survey of waste activity and treatment","Calculated","Medium","High","High","Australian Bureau of Statistics","Australia’s Environment Issues and Trends 2010","Brian Pink","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Commercial Landfill Rate: Australia",null,0.44,"%","N/A","Activity Data","A","AUS",2010,2007,"National survey of waste activity and treatment","Calculated","Medium","High","High","Australian Bureau of Statistics","Australia’s Environment Issues and Trends 2010","Brian Pink","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Construction and Demolition Landfill Rate: Australia",null,0.43,"%","N/A","Activity Data","A","AUS",2010,2007,"National survey of waste activity and treatment","Calculated","Medium","High","High","Australian Bureau of Statistics","Australia’s Environment Issues and Trends 2010","Brian Pink","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate: Australia",null,0.6,"%","N/A","Activity Data","A","AUS",2010,2007,"National survey of waste activity and treatment","Calculated","Medium","High","High","Australian Bureau of Statistics","Australia’s Environment Issues and Trends 2010","Brian Pink","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Austria",null,0.03,"%","N/A","Activity Data","A","AUT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Belgium",null,0.05,"%","N/A","Activity Data","A","BEL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Bulgaria",null,1,"%","N/A","Activity Data","A","BUL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Cyprus",null,0.87,"%","N/A","Activity Data","A","CYP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Czech Republic",null,0.83,"%","N/A","Activity Data","A","CZE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Denmark",null,0.04,"%","N/A","Activity Data","A","DNK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Estonia",null,0.75,"%","N/A","Activity Data","A","EST",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  EU 27",null,0.4,"%","N/A","Activity Data","A","EU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Finland",null,0.5,"%","N/A","Activity Data","A","FIN ",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  France",null,0.36,"%","N/A","Activity Data","A","FRA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Germany",null,0.01,"%","N/A","Activity Data","A","DEU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Greece",null,0.77,"%","N/A","Activity Data","A","GRC",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Hungary",null,0.74,"%","N/A","Activity Data","A","HUN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Ireland",null,0.62,"%","N/A","Activity Data","A","IRL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Italy",null,0.44,"%","N/A","Activity Data","A","ITA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Latvia",null,0.93,"%","N/A","Activity Data","A","LVA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Lithuania",null,0.96,"%","N/A","Activity Data","A","LIT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Luxembourg",null,0.19,"%","N/A","Activity Data","A","LUX",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Malta",null,0.97,"%","N/A","Activity Data","A","MLT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Netherlands",null,0.01,"%","N/A","Activity Data","A","NLD",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Poland",null,0.87,"%","N/A","Activity Data","A","POL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Portugal",null,0.65,"%","N/A","Activity Data","A","PRT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Romania",null,0.99,"%","N/A","Activity Data","A","ROM",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Slovakia",null,0.83,"%","N/A","Activity Data","A","SVK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Slovenia",null,0.66,"%","N/A","Activity Data","A","SVN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Spain",null,0.56999999999999995,"%","N/A","Activity Data","A","ESP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  Sweden",null,0.03,"%","N/A","Activity Data","A","SWE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Landfill Rate:  United Kingdom",null,0.55000000000000004,"%","N/A","Activity Data","A","GBR",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Combined Recycling Rate: Australia",null,0.52,"%","N/A","Activity Data","A","AUS",2010,2007,"National survey of waste activity and treatment","Calculated","Medium","High","High","Australian Bureau of Statistics","Australia’s Environment Issues and Trends 2010","Brian Pink","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Austria",null,0.28999999999999998,"%","N/A","Activity Data","A","AUT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Belgium",null,0.35,"%","N/A","Activity Data","A","BEL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Bulgaria",null,0,"%","N/A","Activity Data","A","BUL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Cyprus",null,0.13,"%","N/A","Activity Data","A","CYP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Czech Republic",null,0.02,"%","N/A","Activity Data","A","CZE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Denmark",null,0.24,"%","N/A","Activity Data","A","DNK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Estonia",null,0.18,"%","N/A","Activity Data","A","EST",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  EU 27",null,0.23,"%","N/A","Activity Data","A","EU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Finland",null,0.25,"%","N/A","Activity Data","A","FIN ",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  France",null,0.18,"%","N/A","Activity Data","A","FRA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Germany",null,0.48,"%","N/A","Activity Data","A","DEU",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Greece",null,0.21,"%","N/A","Activity Data","A","GRC",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Hungary",null,0.15,"%","N/A","Activity Data","A","HUN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Ireland",null,0.32,"%","N/A","Activity Data","A","IRL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Italy",null,0.11,"%","N/A","Activity Data","A","ITA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Latvia",null,0.06,"%","N/A","Activity Data","A","LVA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Lithuania",null,0.03,"%","N/A","Activity Data","A","LIT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Luxembourg",null,0.25,"%","N/A","Activity Data","A","LUX",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Malta",null,0.03,"%","N/A","Activity Data","A","MLT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Netherlands",null,0.32,"%","N/A","Activity Data","A","NLD",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Poland",null,0.09,"%","N/A","Activity Data","A","POL",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Portugal",null,0.09,"%","N/A","Activity Data","A","PRT",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Romania",null,0.01,"%","N/A","Activity Data","A","ROM",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Slovakia",null,0.03,"%","N/A","Activity Data","A","SVK",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Slovenia",null,0.31,"%","N/A","Activity Data","A","SVN",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Spain",null,0.14000000000000001,"%","N/A","Activity Data","A","ESP",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  Sweden",null,0.35,"%","N/A","Activity Data","A","SWE",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Average Municipal Recycling Rate:  United Kingdom",null,0.23,"%","N/A","Activity Data","A","GBR",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","Eurostat","http://epp.eurostat.ec.europa.eu/portal/page/portal/waste/data/sectors/municipal_waste","Eurostat","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Aluminium Recycling Rate (combined): Germany",null,0.77800000000000002,"%","N/A","Activity Data","A","DEU",2007,"Unknown","Study using surveys/sampling","Calculated","Medium","High","Medium","BMU","Gesellschaft für Verpackungsmarktforschung mbH (GVM), Recyclingbilanz","BMU","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Beverage Cartons Recycling Rate (combined): Germany",null,0.624,"%","N/A","Activity Data","A","DEU",2007,"Unknown","Study using surveys/sampling","Calculated","Medium","High","Medium","BMU","Gesellschaft für Verpackungsmarktforschung mbH (GVM), Recyclingbilanz","BMU","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Fibre Recycling Rate (combined): Finland ",null,0.86,"%","N/A","Activity Data","A","FIN",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","PYR Ltd","The Environmental Register of Packaging PYR Ltd","PYR Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined):  Austria ",null,0.84,"%","N/A","Activity Data","A","AUT",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined):  Belgium ",null,0.96,"%","N/A","Activity Data","A","BEL",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined):  Bulgaria  ",null,0.23,"%","N/A","Activity Data","A","BUL",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Czech Republic   ",null,0.62,"%","N/A","Activity Data","A","CZE",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Denmark ",null,0.88,"%","N/A","Activity Data","A","DNK",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Estonia ",null,0.32,"%","N/A","Activity Data","A","EST",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): EU 27 ",null,0.65,"%","N/A","Activity Data","A","EU",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Finland ",null,0.92,"%","N/A","Activity Data","A","FIN ",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): France",null,0.61,"%","N/A","Activity Data","A","FRA",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Germany",null,0.82,"%","N/A","Activity Data","A","DEU",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Greece",null,0.12,"%","N/A","Activity Data","A","GRC",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Hungary",null,0.24,"%","N/A","Activity Data","A","HUN",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Ireland",null,0.8,"%","N/A","Activity Data","A","IRL",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Italy",null,0.72,"%","N/A","Activity Data","A","ITA",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Latvia",null,0.35,"%","N/A","Activity Data","A","LVA",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Lithuania",null,0.36,"%","N/A","Activity Data","A","LIT",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Luxembourg",null,0.75,"%","N/A","Activity Data","A","LUX",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Netherlands",null,0.81,"%","N/A","Activity Data","A","NLD",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Norway",null,0.92,"%","N/A","Activity Data","A","CYP",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Poland",null,0.36,"%","N/A","Activity Data","A","POL",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Portugal",null,0.52,"%","N/A","Activity Data","A","PRT",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Romania",null,0.11,"%","N/A","Activity Data","A","ROM",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Slovakia",null,0.38,"%","N/A","Activity Data","A","SVK",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Spain",null,0.6,"%","N/A","Activity Data","A","ESP",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Sweden",null,0.94,"%","N/A","Activity Data","A","SWE",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Switzerland",null,0.95,"%","N/A","Activity Data","A","CHE",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): Turkey",null,0.19,"%","N/A","Activity Data","A","TUR",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Glass Recycling Rate (combined): UK",null,0.61,"%","N/A","Activity Data","A","GBR",2009,2008,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Container Glass Federation","http://www.feve.org/index.php?option=com_content&view=article&id=10&Itemid=11","European Container Glass Federation","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Metal Recycling Rate (combined): EU 15 ",null,0.56999999999999995,"%","N/A","Activity Data","A","EU15",2006,2004,"Study using surveys/sampling","Estimation","Medium","High","High","Commission of the European Communities","Report from the commission to the council and the European Parliament on implementation of the community waste legislation for the period 2001-2006","Commission of the European Communities","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Metal Recycling Rate (combined): Finland ",null,0.59,"%","N/A","Activity Data","A","FIN",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","PYR Ltd","The Environmental Register of Packaging PYR Ltd","PYR Ltd","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Metal Recycling Rate (combined): France",null,0.65200000000000002,"%","N/A","Activity Data","A","FRA",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","IFEN","Indicateurs de suivi des engagements européens","ADEME","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Paper Recycling Rate (combined): EU 15 ",null,0.68,"%","N/A","Activity Data","A","EU15",2006,2004,"Study using surveys/sampling","Estimation","Medium","High","High","Commission of the European Communities","Report from the commission to the council and the European Parliament on implementation of the community waste legislation for the period 2001-2004","Commission of the European Communities","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Paper Recycling Rate (combined): EU 27 ",null,0.66,"%","N/A","Activity Data","A","EU",2010,2009,"Study using surveys/sampling","Estimation","Medium","High","Medium","European Recovered Paper Council (ERPC)","http://www.paperrecovery.org/facts/erpc_facts_figures.asp?folderid=527","European Recovered Paper Council (ERPC)","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Paper Recycling Rate (combined): France",null,0.84599999999999997,"%","N/A","Activity Data","A","FRA",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","IFEN","Indicateurs de suivi des engagements européens","ADEME","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Paper Recycling Rate (combined): Germany",null,0.82099999999999995,"%","N/A","Activity Data","A","DEU",2007,"Unknown","Study using surveys/sampling","Calculated","Medium","High","Medium","BMU","Gesellschaft für Verpackungsmarktforschung mbH (GVM), Recyclingbilanz","BMU","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Paper Recycling Rate (combined): UK",null,0.71099999999999997,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastic Recycling Rate (combined): Denmark ",null,0.17566016073478799,"%","N/A","Activity Data","A","DNK",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastic Recycling Rate (combined): EU 15 ",null,0.24,"%","N/A","Activity Data","A","EU15",2006,2004,"Study using surveys/sampling","Estimation","Medium","High","High","Commission of the European Communities","Report from the commission to the council and the European Parliament on implementation of the community waste legislation for the period 2001-2005","Commission of the European Communities","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastic Recycling Rate (combined): Germany",null,0.338691159586682,"%","N/A","Activity Data","A","DEU",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastic Recycling Rate (combined): Switzerland",null,0.24110218140068887,"%","N/A","Activity Data","A","CHE",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Austria",null,0.27210103329506302,"%","N/A","Activity Data","A","AUT",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Belgium",null,0.29506314580941401,"%","N/A","Activity Data","A","BEL",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Bulgaria",null,0.1079219288174512,"%","N/A","Activity Data","A","BUL",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Cyprus",null,8.6107921928817457E-2,"%","N/A","Activity Data","A","CYP",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Czech Republic",null,0.27324913892078073,"%","N/A","Activity Data","A","CZE",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Estonia",null,0.27210103329506313,"%","N/A","Activity Data","A","EST",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Finland",null,0.16417910447761194,"%","N/A","Activity Data","A","FIN",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): France",null,0.16762342135476463,"%","N/A","Activity Data","A","FRA",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Greece",null,7.5774971297359356E-2,"%","N/A","Activity Data","A","GRC",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Hungary",null,0.16073478760045926,"%","N/A","Activity Data","A","HUN",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Ireland",null,0.21699196326062001,"%","N/A","Activity Data","A","IRL",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Italy",null,0.218140068886338,"%","N/A","Activity Data","A","ITA",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Latvia",null,0.19058553386911595,"%","N/A","Activity Data","A","LVA",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Lithuania",null,7.5774971297359356E-2,"%","N/A","Activity Data","A","LIT",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Luxembourg",null,0.1618828932261768,"%","N/A","Activity Data","A","LUX",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Malta",null,9.4144661308840416E-2,"%","N/A","Activity Data","A","MLT",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Netherlands",null,0.23306544202066601,"%","N/A","Activity Data","A","NLD",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Norway",null,0.27324913892078101,"%","N/A","Activity Data","A","NOR",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Poland",null,0.14810562571756603,"%","N/A","Activity Data","A","POL",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Portugal",null,0.142365097588978,"%","N/A","Activity Data","A","PRT",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Romania",null,0.1079219288174512,"%","N/A","Activity Data","A","ROM",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Slovakia",null,0.18140068886337543,"%","N/A","Activity Data","A","SVK",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Slovenia",null,0.20665901262916189,"%","N/A","Activity Data","A","SVK",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Spain",null,0.19288174512055101,"%","N/A","Activity Data","A","ESP",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): Sweden",null,0.27784156142365102,"%","N/A","Activity Data","A","SWE",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Plastics Recycling Rate (combined): UK",null,0.18599311136624599,"%","N/A","Activity Data","A","GBR",2009,2008,"Survey of European Plants","Estimation","Medium","High","Medium","Plastics Europe","The compelling facts about plastics 2009","Plastics Europe","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Tinplate Recycling Rate (combined): Germany",null,0.90700000000000003,"%","N/A","Activity Data","A","DEU",2007,"Unknown","Study using surveys/sampling","Calculated","Medium","High","Medium","BMU","Gesellschaft für Verpackungsmarktforschung mbH (GVM), Recyclingbilanz","BMU","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","Wood Recycling Rate (combined): France",null,0.20100000000000001,"%","N/A","Activity Data","A","FRA",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","IFEN","Indicateurs de suivi des engagements européens","ADEME","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates -  combustion wastes",null,0.266349803458092,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates -  Industrial Sludges",null,0.12869317505799377,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates -  Other animal by-products",null,9.8530217801789971E-2,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates -  Paints & Varnishes",null,0.20447023871059744,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - C&D",null,0.18431947924313302,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - common sludges",null,9.3908410203766765E-2,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Discarded equipment",null,0.54085039030029891,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Food",null,0.24084971252737566,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Metallic Wastes",null,0.86655750753661176,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Oils and Solvents",null,0.32799194873826548,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Other Chemical Wastes",null,0.11479788388002315,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Other mineral wastes",null,0.10703555552523682,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - other mixed general waste",null,4.0177219428447077E-2,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Other non-metallic, non-mineral wastes",null,0.71580638817820941,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Commercial Recycling Rates - Paper and Card",null,0.85860534843461866,"%","N/A","Activity Data","A","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","E-Digest of Environmental Statistics http://www.defra.gov.uk/evidence/statistics/environment/waste/wrpaper.htm","Defra","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Cans",null,0.10406360168121565,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Compost",null,0.30358791789655803,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Glass",null,0.46541398032423437,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Paper & card",null,0.33085400021554051,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: HDPE/PET bottles ",null,0.27,"%","N/A","Activity Data","B","GBR",2007,2006,"Estimation based on official waste data","Estimation","Medium","High","High","WRAP","Annual Local Plastics Authorities Plastics Collections Survey 2007","WRAP","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Plastics ",null,2.7325164472772619E-2,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Scrap metals & white goods",null,0.46659403530552868,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","UK Household Recycling: Textiles",null,0.1332887772389266,"%","N/A","Activity Data","A","GBR",2007,2006,"Study using surveys/sampling","Estimation","Medium","High","Medium","Department for Environment, Food and Rural Affairs (DEFRA), WRAP","Municipal Waste Statistics 2006/7' and 'Analysis of household waste composition and factors driving waste increases' ","J.Parfitt ","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Aluminium",null,0.218,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Aluminium beer and drinks cans",null,0.48599999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Aluminium foil and other packaging",null,9.8000000000000004E-2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Aluminium food and other cans",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Beer and soft drinks bottles",null,0.34499999999999997,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Books",null,0.26100000000000001,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Commercial printing",null,0.57299999999999995,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Corrugated boxes",null,0.73599999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Ferrous",null,0.33799999999999997,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Folding cartons",null,0.27300000000000002,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Food and other bottles and jars",null,0.14800000000000002,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Glass general",null,0.23699999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Magazines",null,0.39600000000000002,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - metal general",null,0.34799999999999998,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - metals in containers and packaging",null,0.54100000000000004,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - metals in durable goods",null,0.29799999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Milk and water bottles (HDPE)",null,0.28000000000000003,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - milk cartons",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Newsprint",null,0.78599999999999992,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Non packaging paper",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Office paper",null,0.71799999999999997,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Other  plastic containers",null,0.13900000000000001,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Other Nonferrous",null,0.69299999999999995,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Other paper packaging",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Other paperboard packaging",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Other plastic packaging",null,2.3E-2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - other steel packaging",null,0.66700000000000004,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Paper bags and sacks",null,0.36799999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Paper plates and cups",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Plastic bags sacks and wraps",null,9.0999999999999998E-2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Plastic general",null,6.8000000000000005E-2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Plastic in durable goods",null,4.8000000000000001E-2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Rubber and Leather",null,0.14699999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Rubber in tires",null,0.34799999999999998,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Soft drinks bottles (PET)",null,0.36599999999999999,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Standard Mail",null,0.40299999999999997,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Steel cans",null,0.64300000000000002,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Telephone directories",null,0.2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Textiles",null,0.159,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Tissue paper and towels",null,5.0000000000000001E-4,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - wine and liquor bottles",null,0.15,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["End of Life Fate","US Combined Recycling Rates - Wood",null,9.3000000000000013E-2,"%","N/A","Activity Data","A","USA",2008,2007,"Study using surveys/sampling","Estimation","Medium","High","Medium","US Environmental Protection Authority (EPA)","Municipal solid waste in the United States: 2007 Facts and Figures","US EPA","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Natural gas - NSW and ACT - AUS",null,0.23885239078321899,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Natural gas - QLD - AUS",null,0.21581239078323752,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Natural gas - SA - AUS",null,0.22229239078323232,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Natural gas - VIC- AUS",null,0.19925239078325077,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Natural gas - WA - AUS",null,0.19925239078325077,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Natural Gas (Low Pressure, high upstream emission countries) (net kWh)",null,0.29525867,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Austria, Czech Republic, Finland, Greece, Hungary and Slovakia","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, low upstream emission countries) (net kWh)",null,0.22913296,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Belgium, Denmark, Ireland, Netherlands, Sweden","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)",null,0.25608379999999997,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Switzerland, Germany, Spain, France and Italy","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, UK) (Emissions per net kWh)",null,0.22197609999999998,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Emissions per net kWh) - USA",null,0.21377031420274889,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Aviation Spirit (Emissions by volume) ",null,2.6589760675883256,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Burning Oil (Emissions by volume)",null,3.0130614746543776,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Compressed Natural Gas (CNG) (Emissions by volume)",null,0.54374801158474562,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel (Emissions by volume)",null,3.1756163133640554,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Gas Oil (Emissions by volume)",null,3.5758533640553001,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Emissions by volume)",null,3.0160685714285709,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Liquefied Petroleum Gas (LPG) (Emissions by volume)",null,1.6786014439324117,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: LNG (Emissions by volume)",null,1.6573635076528652,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol (Emissions by volume)",null,2.723096006144393,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel (Emissions by volume) - USA",null,3.0335192926947085,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Kerosene (Emissions by volume) - USA",null,2.9183069830751447,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Petrol (Emissions by volume) - USA",null,2.7800473561616021,"kg CO2(e)/litre","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Aviation gasoline - AUS",null,0.259309271889193,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Aviation Spirit (Emissions by mass)",null,3.7597142857142862,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Aviation Spirit (Emissions per gross kWh)",null,0.28529379416282641,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Aviation Spirit (Emissions per net kWh)",null,0.30033352380952383,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Aviation turbine fuel (jet kerosene) - AUS",null,0.267854986174901,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Black coal for electricity - AUS",null,0.35279999999971778,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Black coal—uses other than for electricity and coking - AUS",null,0.33622711520710402,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Brown coal briquettes - AUS",null,0.37569533640522901,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Burning Oil  (Emissions by mass)",null,3.751243287250384,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Burning Oil (Emissions per gross kWh)",null,0.29252311213517668,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Burning Oil (Emissions per net kWh) ",null,0.3079172780337941,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Charcoal - AUS",null,1.8719999999985026E-2,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Coal - Brown coal - AUS",null,0.33659999999973078,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Coal (Anthracite) (Emissions by mass) - USA",null,2405,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal (Bituminous) (Emissions by mass) - USA",null,2308.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal (domestic) (Emissions by mass) ",null,3.3857367741935485,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (domestic) (Emissions per gross kWh)",null,0.39962068817204305,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (domestic) (Emissions per net kWh)",null,0.42064996927803378,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (Electric power) (Emissions per net kWh) - USA",null,0.33807873680770223,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal (electricity generation) (Emissions by mass)",null,2.6268213517665129,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (electricity generation) (Emissions per gross kWh)",null,0.37826304147465434,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (electricity generation) (Emissions per net kWh)",null,0.39817723502304098,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (Emissions by mass)",null,2.76291376344086,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (Emissions per gross kWh)",null,0.38497548079877109,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (Emissions per net kWh)",null,0.40524499846390172,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coal (Gross kWh by mass)",null,7472.3553851070628,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Coal (Industrial Coking) (Emissions per net kWh) - USA",null,0.35962078433542488,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal (Lignite) (Emissions by mass) - USA",null,1408.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal (Net kWh by mass)",null,7098.7035856331786,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Coal (Residential/Commercial) (Emissions per net kWh) - USA",null,0.36847550711496013,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal (Sub-bituminous) (Emissions by mass) - USA",null,1792.7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Coal mine waste gas - AUS",null,0.20411999999983674,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Coking Coal - AUS",null,0.45251999999963805,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Coking Coal (Emissions by mass)",null,3.5411537019969277,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coking Coal (Emissions per gross kWh)",null,0.39103577265745004,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coking Coal (Emissions per net kWh)",null,0.41162418740399387,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Coking coal (metallurgical coal) - AUS",null,0.399297843317653,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Compressed Natural Gas (CNG)  (Emissions by mass)",null,3.1070743519128321,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Compressed Natural Gas (CNG) (Emissions per gross kWh)",null,0.21068717050691246,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Compressed Natural Gas (CNG) (Emissions per net kWh)",null,0.23436249769585252,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Crude oil - AUS",null,0.268069271889187,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Diesel - retail station biofuel blend (Emissions by mass)",null,3.7041418433179722,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel - retail station biofuel blend (Emissions by mass)",null,3.7041418433179722,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel - retail station biofuel blend (Emissions per gross kWh)",null,0.29375324116743473,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel - retail station biofuel blend (Emissions per net kWh)",null,0.3126493701996928,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel (Automotive Diesel Oil) - AUS",null,0.26932070046061402,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Diesel (Emissions by mass)",null,3.7948341013824884,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel (Emissions per gross kWh)",null,0.29967588940092171,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel (Emissions per net kWh)",null,0.31881353609831026,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Diesel (Emissions per net kWh) - USA",null,0.31158268567656011,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Diesel (Gross kWh by mass)",null,12651.593011305242,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Diesel (Gross kWh by volume)",null,10.551822278440984,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Diesel (Net kWh by mass)",null,12018.77581674803,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Diesel (Net kWh by volume)",null,10.024033045437477,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Fuel oil - AUS",null,0.282340700460604,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Fuel Oil (Emissions by mass)",null,3.7734301075268819,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Fuel Oil (Emissions per gross kWh)",null,0.31260200307219654,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Fuel Oil (Emissions per net kWh)",null,0.33255119815668199,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Fuel Oil (Gross kWh by mass)",null,12121.382727170363,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Fuel Oil (Net kWh by mass)",null,11515.421643786773,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Gas Oil (Emissions by mass)",null,4.1229337634408605,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Gas Oil (Emissions per gross kWh)",null,0.32557988018433187,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Gas Oil (Emissions per net kWh)",null,0.34636865745007683,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Gas Oil (Gross kWh by mass)",null,12651.526110227109,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Gas Oil (Gross kWh by volume)",null,10.95363807319543,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Gas Oil (Net kWh by mass)",null,12018.689020200633,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Gas Oil (Net kWh by volume)",null,10.405730383399753,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Kerosene - AUS",null,0.26531999999978778,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Kerosene (Emissions per net kWh) - USA",null,0.28139438477940421,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Emissions by mass)",null,3.7669857142857146,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Emissions per gross kWh)",null,0.29352917972350229,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Emissions per net kWh)",null,0.30896453456221207,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Gross kWh by mass)",null,12832.372273075529,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Gross kWh by volume)",null,10.298802371063349,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Net kWh by mass)",null,12190.851976708551,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Kerosene / Burning Oil / Aviation Turbine Fuel (Net kWh by volume)",null,9.7839411584431506,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Landfill gas - AUS",null,1.7279999999986178E-2,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Liquefied Petroleum Gas - AUS ",null,0.2336807004606426,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Liquid Petroleum Gas (LPG) (Emissions by mass)",null,2.2730000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2009,2007,"Calculated from reports","Calculated","Medium","High","High","Arup, CONCAWE, EUCAR and JRC of the EU Commission","Imported from CT Model (using data from Arup, CONCAWE, EUCAR and JRC of the EU Commission)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Liquid Petroleum Gas (LPG) (Emissions per net kWh) - USA",null,0.26027585079842652,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Liquefied Natural Gas (LNG) (Emissions by mass)",null,3.662774351912832,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Liquefied Natural Gas (LNG) (Emissions per gross kWh)",null,0.24837717050691244,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Liquefied Natural Gas (LNG) (Emissions per net kWh)",null,0.2762824976958525,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Liquefied Petroleum Gas (LPG) (Emissions per gross kWh)",null,0.24837717050691244,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Liquefied Petroleum Gas (LPG) (Emissions per net kWh)",null,0.25875654070660525,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Lubricants (Emissions by mass)",null,3.5677328725038397,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Lubricants (Emissions per gross kWh)",null,0.29556337941628263,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Lubricants (Emissions per net kWh) ",null,0.31443334869431644,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Lubricants and greases - AUS",null,0.11951999999990438,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2009,2008,"Official Australian government data","Calculated","Medium","High","High","Carbon Trust, Department of Climate Change, Australia","National Greenhouse Accounts (NGA) Factors, 2009","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Naphtha - AUS",null,0.26817214446061499,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Naphtha (Emissions by mass)",null,3.5839046082949308,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Naphtha (Emissions per gross kWh)",null,0.27146638709677418,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Naphtha (Emissions per net kWh)",null,0.28574713056835643,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Naphtha (Gross kWh by mass)",null,13190.328267987574,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Naphtha (Net kWh by mass)",null,12530.706651778593,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Natural Gas (Emissions by volume) - USA",null,2.4401160627745737,"kg CO2(e)/Nm3","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Natural Gas (Low Pressure,  with high upstream emission countries) (Emissions by volume)",null,2.5323297999999999,"kg CO2(e)/m3","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Austria, Czech Republic, Finland, Greece, Hungary and Slovakia","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, high upstream emission countries) (gross kWh)",null,0.26534623276699032,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Austria, Czech Republic, Finland, Greece, Hungary and Slovakia","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, low upstream emission countries) (Emissions by volume)",null,2.0708766666666669,"kg CO2(e)/m3","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Belgium, Denmark, Ireland, Netherlands, Sweden","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, low upstream emission countries) (gross kWh)",null,0.20596149320388349,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Belgium, Denmark, Ireland, Netherlands, Sweden","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (Emissions by volume)",null,2.265815937777778,"kg CO2(e)/m3","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Switzerland, Germany, Spain, France and Italy","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (gross kWh)",null,0.23016491747572815,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from Ecoinvent reports.  Applies to Switzerland, Germany, Spain, France and Italy","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, UK) (Emissions by volume)",null,2.1950425444444446,"kg CO2(e)/m3","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, UK) (Emissions per gross kWh)",null,0.20942,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Natural Gas (Low Pressure, UK) (Gross kWh by volume)",null,11,"kWh/Nm3","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Natural Gas (Low Pressure, UK) (Net kWh by volume)",null,9.8888888888888893,"kWh/Nm3","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Other Petroleum Gas (Emissions by mass)",null,3.0112459907834106,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Other Petroleum Gas (Emissions per gross kWh)",null,0.21401487557603685,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Other Petroleum Gas (Emissions per net kWh)",null,0.23263203993855608,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol - AUS",null,0.26973091244218056,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Petrol - retail station biofuel blend (Emissions by mass)",null,3.6244164976958522,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol - retail station biofuels blend (Emissions per gross kWh)",null,0.2804300460829493,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol (Emissions by mass)",null,3.7088316743471577,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol (Emissions per gross kWh)",null,0.28349034408602153,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol (Emissions per net kWh)",null,0.29841260522273427,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petrol (Emissions per net kWh) - USA",null,0.30992615106406529,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Petrol (Gross kWh by mass)",null,13075.432811211871,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Petrol (Gross kWh by volume)",null,9.6071723000824409,"kWh/litre","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Petrol (Net kWh by mass)",null,12421.584367780084,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Petrol (Net kWh by volume)",null,9.1267572541802107,"kWh/litre","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petroleum Coke - AUS",null,0.34690927188912302,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","AUS",2010,2008,"Official Australian government data","Calculated","Medium","High","Medium","Carbon Trust, Department of Climate Change, Australia","Modelled using National Greenhouse Accounts (NGA) Factors, 2010","Department of Climate Change, Australia","PAS 2050","PAS 2050","No","Unknown","No","PAS 2050","N/A","N/A","No"]
["Fuels","Fuel: Petroleum Coke (Emissions by mass)",null,3.5366168049155147,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petroleum Coke (Emissions per gross kWh)",null,0.35602974500768048,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petroleum Coke (Emissions per net kWh)",null,0.37475732718894006,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Petroleum Coke (Emissions per net kWh) - USA",null,0.43620162056430545,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Fuels","Fuel: Petroleum Coke (Gross kWh by mass)",null,9925.129746745697,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Petroleum Coke (Net kWh by mass)",null,9428.8331492308098,"kWh/tonne","N/A","Conversion Factor","A","EU",2009,2007,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2009, Dukes Digest 2006, & EcoInvent data v2.0)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Fuels","Fuel: Propane (Emissions by mass)",null,3.528,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Refinery Miscellaneous (Emissions per gross kWh)",null,0.2758978740399386,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Refinery Miscellaneous (Emissions per net kWh)",null,0.29041823041474657,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","EU",2011,2009,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Fuels","Fuel: Residual Fuel Oil (Emissions per net kWh) - USA",null,0.31382436571227934,"kg CO2(e)/kWh","Cradle to Gate","Emission Factor","A","USA",2008,2007,"Calculated based on US EPA government data","Calculated","Medium","High","High","US EPA, Carbon Trust","Modelled by Carbon Trust with reference to Inventory of U.S. Greenhouse Gas Emissions and Sinks 1990-2007","US EPA, Carbon Trust","PAS 2050","PAS 2050","No","None","No","PAS 2050","No","No","No"]
["Global Constant","Atmospheric Pressure",null,101325,"Pa","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Atomic Mass of C",null,12,null,"N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Atomic Mass of H",null,1,null,"N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Atomic Mass of N",null,14,null,"N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Atomic Mass of O",null,16,null,"N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Days per Week",null,7,"days/week","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Days per Year",null,365.25,"days/year","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","feet to metres",null,0.30480000000000002,"m/ft","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","feet3 to metres3",null,2.8316846592000004E-2,"m3/ft3","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Hours per Day",null,24,"hours/day","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Hours per week",null,168,"hours/week","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Hours per year",null,8766,"hours/year","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Kcal to Kilojoules",null,4.1840000000000002,"Kj/kcal","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg C to kg CH4",null,1.3333333333333333,null,"N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg C to kg CO",null,2.3333333333333335,null,"N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg C to kg CO2",null,3.666666666666667,null,"N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg CH4 to kg C",null,0.75,null,"N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg CO to kg C",null,0.42857142857142855,null,"N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg CO2 to kg C",null,0.27272727272727271,null,"N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg to lb",null,2.2046000000000001,"lb/kg","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","kg to tonnes",null,1E-3,"tonnes/kg","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Kilojoules to Kilowatt-hour",null,2.7777777777777778E-4,"kWh/kJ","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Kilowatt-hour to Kilojoules",null,3600,"kJ/kWh","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","km to miles",null,0.62137119223733395,"mile/km","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","km/litre to MPG (UK)",null,2.8250000000000002,"mile/gallon (UK) / km/litre","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","km/litre to MPG (US)",null,2.3530000000000002,"mile/gallon (US) / km/litre","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Knots to Km per hour",null,1.8520000000000001,"km/h/Knots","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","lb to kg",null,0.4535970244035199,"kg/lb","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","m3 to litres",null,1000,"L/m3","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","miles to km",null,1.6093440000000001,"km/mile","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Months per year",null,12,"months/year","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","MPG (UK) to km/litre",null,0.35399999999999998,"km/litre / mile/gallon (UK)","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","MPG (US) to km/litre",null,0.42499999999999999,"km/litre / mile/gallon (US)","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Nautical Miles to Km",null,1.8520000000000001,"Km/Nm","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","tonnes to kg",null,1000,"kg/tonne","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","UK gallon to US gallon",null,1.2010000000000001,"US gallon/UK gallon","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Universal gas constant",null,8.3145000000000007,"J/mol K","N/A","Conversion Factor","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Weeks per month",null,4.333333333333333,"weeks/month","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Global Constant","Weeks per year",null,52,"weeks/year","N/A","Global Parameter","N/A","GLO","N/A","N/A","N/A","Measurement","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["GWP","GWP: Biogenic Methane (CH4)",null,22.25,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Carbon Dioxide (CO2)",null,1,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Carbon Tetrachloride",null,1400,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: CFC-11",null,4750,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: CFC-113",null,6130,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: CFC-114",null,10000,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: CFC-115",null,7370,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: CFC-12",null,10900,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: CFC-13",null,14400,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Dimethylether (CH3OCH3)",null,1,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Fossil Methane (CH4)",null,25,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Halon-1211",null,1890,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Halon-1301",null,7140,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Halon-2402",null,1640,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-123",null,77,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-124",null,609,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-141b",null,725,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-142b",null,2310,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-22",null,1810,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-225ca",null,122,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFC-225cb",null,595,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HCFE- 235da2",null,350,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-125",null,3500,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-134a",null,1430,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-143a",null,4470,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-152a",null,124,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-227ea",null,3220,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-23",null,14800,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-236fa",null,9810,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-245fa",null,1030,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-32",null,675,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-365mfc",null,794,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFC-43-10mee",null,1640,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE- 236ca12 (HG-10)",null,2800,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE- 356pcc3",null,110,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE- 43-10pccc124 (H-Galden 1040x)",null,1870,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-125",null,14900,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-134",null,6320,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-143a",null,756,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-245cb2",null,708,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-245fa2",null,659,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2009,2007,"Calculated based on existing literature","Measurement","Medium","High","High","Intergovernmental Panel on Climate Change","Imported from Carbon Trust Refrigerant Emissions Calculator 2010","CTFC","PAS 2050","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-254cb2",null,259,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-338pcc13 (HG-01)",null,1500,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-347mcc3",null,575,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-347pcf2",null,580,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-449sl (HFE-7100)",null,297,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: HFE-569sf2 (HFE-7200)",null,59,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Methyl Bromide",null,5,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Methyl Chloride (CH3CL)",null,13,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Methylene Chloride (CH2Cl2)",null,8.6999999999999993,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Nitrogen trifluoride (NF3)",null,17200,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Nitrous Oxide (N2O)",null,298,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Perfluoroethane (C2F6) PFC-116",null,12200,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Perfluoromethane (CF4) PFC-14",null,7390,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFC-218",null,8830,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFC-3-1-10",null,8860,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFC-318",null,10300,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFC-4-1-12",null,9160,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFC-5-1-14",null,9300,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFC-9-1-18",null,7500,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: PFPMIE",null,10300,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: R404a",null,3921.6,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2009,2007,"Calculated based on existing literature","Measurement","Medium","High","High","Intergovernmental Panel on Climate Change","Imported from Carbon Trust Refrigerant Emissions Calculator 2010","CTFC","PAS 2050","PAS 2050","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: R405a",null,5327.73,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2009,2007,"Calculated based on existing literature","Measurement","Medium","High","High","Intergovernmental Panel on Climate Change","Imported from Carbon Trust Refrigerant Emissions Calculator 2010","CTFC","PAS 2050","PAS 2050","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: R407c",null,1773.85,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2009,2007,"Calculated based on existing literature","Measurement","Medium","High","High","Intergovernmental Panel on Climate Change","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: R410a",null,2087.5,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2009,2007,"Calculated based on existing literature","Measurement","Medium","High","High","Intergovernmental Panel on Climate Change","Imported from Carbon Trust Refrigerant Emissions Calculator 2010","CTFC","PAS 2050","PAS 2050","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: R417a",null,2064.6622000000002,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2009,2007,"Calculated based on existing literature","Measurement","Medium","High","High","Intergovernmental Panel on Climate Change","Imported from Carbon Trust Electricity Emission Factor Generator using IEA data 2007","CTFC","PAS 2050","PAS 2050","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP: Sulphur hexafluoride (SF6)",null,22800,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP:Methyl chloroform",null,146,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["GWP","GWP:Trifluoromethyl sulphur pentafluoride (SF5CF3)",null,17700,"kg CO2(e)/kg","N/A","Emission Factor","A","GLO",2007,2007,"Calculated based on existing literature","Measurement","High","High","High","Intergovernmental Panel on Climate Change","IPCC 2007, Fourth Assessment Report, \"2007_4AR_Changes in atmospheric constituents and in radiative forcing_IPCC.pdf\" P212-213","Coordinating lead authors: Piers Forster (UK), Venkatachalam Ramaswamy (USA) ","IPCC","N/A","N/A","None","No","PAS 2050","N/A","N/A","N/A"]
["Materials","AUS - Virgin Aluminium ",null,22.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and using Bayer/Hall-Heroult process","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Copper (Hydromet)",null,6.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Copper (Pyromet)",null,3.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Lead (BF)",null,2.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Lead (ISF)",null,3.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Nickel  (Pyromet)",null,11.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Nickel (Hydromet)",null,16.100000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Steel  ",null,2.2999999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Zinc (Electrolytic)",null,4.5999999999999996,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Virgin Zinc (ISF)",null,3.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","EU - Virgin Aluminium (Cast)",null,13.1,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","High","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Aluminium (Extruded)",null,12.5,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","High","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Aluminium (General Use)",null,12.79,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","High","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Aluminium (Rolled)",null,12.8,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","High","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Carton Board Box",null,1.92,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2007,2007,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","High","Carbon Trust, EcoInvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","N/A","PAS 2050"]
["Materials","EU - Virgin Copper - roofing sheets ",null,11.1,"kg CO2(e)/m2","Cradle to Gate","Emission Factor","C","EU",2005,2004,"0.66 mm","Calculated","Unknown","High","Low","European Copper Institute","http://www.kupfer-institut.de/lifecycle/","Unknown","Custom definition","Unknown","Unknown","unknown","No","Unknown","Unknown","No","Unknown"]
["Materials","EU - Virgin Copper - tube ",null,0.81599999999999995,"kg CO2(e)/m2","Cradle to Gate","Emission Factor","C","EU",2005,2004," 1mm2 section, 1m length","Calculated","Unknown","High","Low","European Copper Institute","http://www.kupfer-institut.de/lifecycle/","Unknown","Custom definition","Unknown","Unknown","unknown","No","Unknown","Unknown","No","Unknown"]
["Materials","EU - Virgin Copper - wire, high grade ",null,27.638000000000002,"kg CO2(e)/m","Cradle to Gate","Emission Factor","C","EU",2005,2004,"15 mm diameter, 1 mm thickness","Calculated","Unknown","High","Low","European Copper Institute","http://www.kupfer-institut.de/lifecycle/","Unknown","Custom definition","Unknown","Unknown","unknown","No","Unknown","Unknown","No","Unknown"]
["Materials","EU - Virgin Corrugate Box (single wall)",null,1.1399999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2007,2007,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","High","Carbon Trust, EcoInvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","N/A","PAS 2050"]
["Materials","EU - Virgin Epoxy liquid resins ",null,8.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Ethylene pipeline ",null,1.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin HDPE bottles",null,2.83,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin HDPE pipe",null,2.4569999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin HDPE Resin",null,1.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin High impact polystyrene (HIPS) ",null,3.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin LDPE Film",null,2.16,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin LDPE Resin",null,2.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Nylon 6 ",null,9.1,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Nylon 6 (glass filled)",null,7.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Nylon 66 (glass filled)",null,7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Virgin OPP Film",null,2.96,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Paper - packaging paper, unbleached",null,0.77800000000000002,"kg CO2/kg","Cradle to Gate","Emission Factor","A","EU",2003,2001,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","Medium","Carbon Trust, EcoInvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","EU - Virgin Paper label - without glue ",null,1.55,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU","Unknown","Unknown","Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","Medium","Carbon Trust, EcoInvent","EcoInvent 2.0, Carbon Trust","EcoInvent","Custom definition","Unknown","Unknown","unknown","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Virgin PET Bottle Grade",null,3.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin PET Bottles",null,4.7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin PET Film",null,5.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polycarbonate",null,7.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polypropylene (injection moulded)",null,4.4059114856022896,"kg CO2/kg","Cradle to Gate","Emission Factor","A","EU",2006,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 series","PAS 2050","No","None","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polystyrene (Expandable)",null,3.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polystyrene (General Purpose)",null,3.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polyurethane flexible foam",null,4.7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polyurethane rigid foam",null,4.2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polyvinylchloride (PVC) - bulk polymerisation",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polyvinylchloride (PVC) (emulsion polymerisation)",null,2.5,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polyvinylchloride (PVC) (suspension polymerisation)",null,1.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Polyvinylidene chloride (PVdC)",null,4.4000000000000004,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin PP Resin",null,2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Propylene",null,1.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Propylene - pipeline",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin PVC Film",null,3.0840000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","Yes","Unknown"]
["Materials","EU - Virgin Steel ",null,2.89,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Steel (Bar and Rod)",null,2.77,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Steel (Pipe)",null,2.87,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Steel (Plate)",null,3.27,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Steel (Section)",null,3.03,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Steel (Sheet - Galvanised)",null,3.01,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Steel (Sheet)",null,2.74,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Titanium ",null,31.55,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Generally limited and poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Virgin Zinc (high grade)",null,3.1957984456913628,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Special high grade zinc; primary production; production mix, at plant;  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","IZA","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","UK - Virgin Brass ",null,4.8,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Virgin Coarse aggregate - basalt ",null,2.0061575725305932E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2007,"Data from two coarse aggregate quarries, modelled to UK fuel and electricity grid mix","Calculated","Medium","High","Medium","Carbon Trust, Department of Civil Engineering, Monash University","Green House Gas Emissions due to Concrete Manufacture","David J. M. Flower and Jay G. Sanjayan","PAS 2050","PAS 2050","Unknown","Unknown","No","PAS 2050","Unknown","No","Unknown"]
["Materials","UK - Virgin Copper ",null,3.83,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Virgin Copper (Tube and Sheet)",null,3.81,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Virgin Glass",null,0.91,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Virgin Iron",null,2.0299999999999998,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Data quality not sufficient to estimate coefficients for a broad range of iron products","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Virgin Lead ",null,3.37,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Mass allocation between lead and zinc applied","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Virgin Zinc ",null,4.18,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","US - Virgin ABS Resin",null,3.7490000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin Flexible Foam Polyurethane",null,3.8530000000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin GPPS Resin",null,3.1749999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin HDPE Resin",null,1.89,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin HIPS Resin",null,3.194,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin LDPE Resin",null,2.21,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin LLDPE Resin",null,1.9239999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin MDI Resin",null,2.2890000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin PET Resin",null,2.7890000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin PP Resin",null,1.8680000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin PVC Resin",null,2.2549999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin Rigid Foam Polyurethane",null,3.5379999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","US - Virgin TDI Resin",null,2.2120000000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2003,"Based on data collected specifically for this project from 17 resin/precursor manufacturers, representing more than 80 plants in North America","Calculated","High","High","Medium","American Chemistry Council: The Plastics Division ","CRADLE-TO-GATE LIFE CYCLE INVENTORY OF NINE PLASTIC RESINS AND FOUR POLYURETHANE PRECURSORS","FRANKLIN ASSOCIATES","ISO 14000 Series","PAS 2050","ISO 14000 Series","mass and enthalpy allocation","No","PAS 2050","Unknown","Unknown","No"]
["Materials","EU - Recycled Aluminium (cast)",null,1.45,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Aluminium (extruded)",null,2.12,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Aluminium (general Use)",null,1.81,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Aluminium (rolled)",null,1.79,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","EU",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Corrugated box (double wall)",null,1.1299999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2008,2008,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","High","Carbon Trust, EcoInvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","N/A","PAS 2050"]
["Materials","EU - Recycled Corrugated box (single wall)",null,1.1200000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2008,2008,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","High","Carbon Trust, EcoInvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","N/A","PAS 2050"]
["Materials","EU - Recycled PET Bottle Grade",null,1.1599999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","Unknown","Yes","PAS 2050"]
["Materials","EU - Recycled PET Bottles",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2008,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Modelled by CT using data from Plastics Europe","CTFC","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","Unknown","Yes","PAS 2050"]
["Materials","EU - Recycled Steel (bar and rod)",null,0.45,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Steel (engineering)",null,0.72,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Steel (general use)",null,0.47,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Steel (section)",null,0.47,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Recycled Titanium",null,14.7,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Generally limited and poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Recycled Brass",null,1.2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","Unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Recycled Copper (from high grade scrap)",null,0.96,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Recycled Copper (from low grade scrap)",null,2.75,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Recycled Copper (Tube and Sheet)",null,0.84,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Recycled Glass container ",null,0.52900000000000003,"kg CO2/kg","Cradle to Gate","Emission Factor","B","GBR",2003,2002,"Survey of glass manufacturing facilities in UK","Calculated","High","High","Medium","British Glass Manufacturers Confederation","GLASS RECYCLING – LIFE CYCLE CARBON DIOXIDE EMISSIONS","Enviros","Custom definition","PAS 2050","Unknown","Unknown","No","CO2 only","Unknown","Unknown","No"]
["Materials","UK - Recycled Glass wool",null,0.60299999999999998,"kg CO2/kg","Cradle to Gate","Emission Factor","B","GBR",2003,2002,"Survey of glass manufacturing facilities in UK","Calculated","High","High","Medium","British Glass Manufacturers Confederation","GLASS RECYCLING – LIFE CYCLE CARBON DIOXIDE EMISSIONS","Enviros","Custom definition","PAS 2050","Unknown","Unknown","No","CO2 only","Unknown","Unknown","No"]
["Materials","UK - Recycled Lead ",null,0.57999999999999996,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Recycled Zinc ",null,0.52,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Mass allocation between lead and zinc applied","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","ARG - Feed crops for livestock - Soy (Average - no land use change)    ",null,0.24773921925360204,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","ARG",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","ARG - Feed crops for livestock - Soy (Land use change included)  ",null,6.9406526050803734,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","ARG",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","ARG - Feed crops for livestock - Soy meal (Average - no land use change)    ",null,0.21395746818127923,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","ARG",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","ARG - Feed crops for livestock - Soy meal (Land use change included)  ",null,5.4657466467078759,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","ARG",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","AUS - Average Aluminium ",null,11.8,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and using Bayer/Hall-Heroult process","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Copper (hydromet)",null,1.69,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Copper (pyromet)",null,0.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Glass (37% recycled) ",null,1.0569999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","AUS",2005,2001,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","High","Carbon Trust, Ecoinvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","N/A","PAS 2050"]
["Materials","AUS - Average Lead (BF)",null,0.56999999999999995,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Lead (ISF)",null,0.87,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Nickel  (Pyromet)",null,3.11,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Nickel (Hydromet)",null,4.3899999999999997,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Steel ",null,0.63,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Zinc  (ISF)",null,0.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","AUS - Average Zinc (electrolytic)",null,1.25,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","AUS",2003,1999,"Process data derived from literature and general industry technologies","Calculated","Medium","High","High","Australian Commonwealth Scientific and Research Organization (CSIRO)","Norgate, T E and Rankin, W J, 2000. Life cycle assessment of copper and nickel production, MINPREX 2000 (The AusIMM), Melbourne, pp. 133-138; Norgate, T E and Rankin, W J, 2001. Greenhouse gas emissions from aluminium production – a life cycle approach. G","Terry Norgate and John Rankin","PAS 2050","PAS 2050","Unknown","unknown","No","PAS 2050","No","No","No"]
["Materials","BRA - Feed crops for livestock - Soy (Average - no land use change)    ",null,0.26737019666285133,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","BRA - Feed crops for livestock - Soy (Land use change included)  ",null,14.834299330521118,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","BRA - Feed crops for livestock - Soy meal (Average - no land use change)    ",null,0.22122155581991867,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","BRA - Feed crops for livestock - Soy meal (Land use change included)  ",null,11.651586238495453,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","EU - Acrylonitrile-Butadiene-Styrene Copolymer (ABS)",null,3.8,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Aerated concrete block ",null,0.46675420957800806,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2004,"Aerated concrete block; mix of P2 04 and P4 05; production mix, at plant; average density 433 kg/m3  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Aerated concrete block - reinforced ",null,0.51920036228533506,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2004,"Aerated concrete block; type P4 05 reinforced; production mix, at plant; average density 485 kg/m3  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Aluminium extrusion (process) ",null,2.4520765719273472,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Aluminium extrusion profile; primary production; production mix, at plant; aluminium semi-finished extrusion product, including primary production, transformation and recycling","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EAA","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Aluminium sheet (process) ",null,3.2297186324828586,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Aluminium sheet; primary production; production mix, at plant; aluminium semi-finished sheet product, including primary production, transformation and recycling (en","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EAA","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Brine - purified ",null,0.17,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","Unknown","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Calcium anhydrite ",null,9.9553964306409351E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2002,"ILCD Database","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Calcium silicate ",null,0.1468527758024008,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Calcium silicate; blocks and elements; production mix, at plant; density 1400 to 2000 kg/m3  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROGYPSUM ","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Concrete - pre cast ",null,0.12089114960515897,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Pre-cast concrete; minimum reinforcement; production mix, at plant; concrete type C20/25, without consideration of casings  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Concrete block - lightweight ",null,0.25940572672351347,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2004,"Lightweight concrete block; expanded clay as base material; production mix, at plant;  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Copper (From High Grade Scrap)",null,1.1000000000000001,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Copper (From Low Grade Scrap)",null,3.1,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Copper (Tube and Sheet)",null,2.71,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","EU",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","EU - Ethylene ",null,1.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Glass wool ",null,2.8051829571860445,"kg CO2/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Glass wool; fleece; production mix, at plant; density between 10 to 100 kg/m3  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Gravel ",null,3.3947730596963275E-3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Gravel 2/32; wet and dry quarry; production mix, at plant; undried  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Gypsum ",null,4.7E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","EU",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","ISO 14000 Series","PAS 2050","Unknown","Unknown","No","Kyoto gases only","Unknown","No","No"]
["Materials","EU - Gypsum plaster - alpha hemihydrates ",null,0.24339488348453148,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2002,"Gypsum plaster (CaSO4 alpha hemihydrates); via calcination of calcium sulphate dihydrate; production mix, at plant; grinded and purified product  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROGYPSUM ","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Gypsum plaster - beta hemihydrates ",null,0.10762469443154557,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2002,"Gypsum plaster (CaSO4 beta hemihydrates); technology mix of natural gypsum (45%) and gypsum from flue gas desulphurisation (55%); production mix, at plant; grinded and purified product  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROGYPSUM ","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Lead ",null,1.7826943587558841,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2002,"Lead; primary; consumption mix, at plant;  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Oriented strand board ",null,0.67419666591920757,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Oriented Strand Board; OSB III; production mix, at plant; 4,8% water content  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Particle board ",null,0.91139923521008426,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Particle board; P5 (V100); production mix, at plant; 7,8% water content  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Plasticisers, 30-45% solids",null,0.22037999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2006,2005,"This environmental declaration is based on the figures from eight of Europe’s largest admixture producers and is an average of the normal plasticisers types detailed above.","Calculated","High","High","Medium","European Federation of Concrete Admixture Associations","EFCA ENVIRONMENTAL DECLARATION PLASTICISING ADMIXTURES – March 2006","European Federation of Concrete Admixture Associations","ISO 14000 series","Unknown","Unknown","Unknown","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","EU - Polyacrylonitrile (PAN)  fibres ",null,5.7024226970665932,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Polyacrylonitrile fibres (PAN); from acrylonitrile and methacrylate; production mix, at plant; PAN without additives  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Polybutadiene ",null,3.9,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Polymethyl methacrylate (PMMA)",null,7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Portland cement ",null,0.90040826247850758,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Portland cement (CEM I); CEMBUREAU technology mix, EN 197-1; CEMBUREAU production mix, at plant;  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","CEMBUREAU ","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Pyrolysis gasoline",null,1.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","Unknown","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","Unknown"]
["Materials","EU - Retarders, 17-46% solids",null,0.13403500000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2006,2005,"This environmental declaration is based on the figures from eight of Europe’s largest admixture producers and is an average of the normal plasticisers types detailed above.","Calculated","High","High","Medium","European Federation of Concrete Admixture Associations","EFCA ENVIRONMENTAL DECLARATION PLASTICISING ADMIXTURES – March 2006","European Federation of Concrete Admixture Associations","ISO 14000 series","Unknown","Unknown","Unknown","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","EU - Rock wool ",null,1.1359315110387875,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Rock wool; fleece; production mix, at plant; density between 30 to 180 kg/m3  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Sand 0/2 ",null,2.447840699038268E-3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Sand 0/2; wet and dry quarry; production mix, at plant; undried  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Silica sand  ",null,0.31132674637721403,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2005,"Calcium silicate; blocks and elements; production mix, at plant; density 1400 to 2000 kg/m3 ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Stainless steel - hot rolled coil",null,3.2297186324828586,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2000,"Stainless Steel Hot Rolled Coil; annealed and pickled, grade 304, Austenitic, electric arc furnace route; production mix, at plant; 18% chromium, 10% nickel  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROFER","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Steel - hot rolled coil (process)",null,0.93136606799999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2000,"Steel hot rolled coil; blast furnace route; production mix, at plant; thickness 2 to 7 mm, width 600 to 2100 mm  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROFER","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Steel - hot rolled section (process)",null,1.1320102491999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2000,"Steel hot rolled section; blast furnace and electric arc furnace route; production mix, at plant;  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROFER","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Steel rebar (process)",null,1.02847909,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2000,"Steel rebar; blast furnace and electric arc furnace route; production mix, at plant;  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","EUROFER","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Stone - crushed ",null,1.3959741780223214E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2010,2006,"Crushed stone 16/32; open pit mining; production mix, at plant; undried  ","Calculated","Medium","High","Medium","European Commission - Joint Research Centre ","ELCD Database","European Commission  - Joint Research Centre ELCD Database","ISO 14000 Series","PAS 2050","ISO 14000 Series","Unknown","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Styrene-Acrylonitrile Copolymer (SAN)",null,3.4,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Superplasticisers, 30-45% solids",null,0.72126699999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2006,2005,"This environmental declaration is based on the figures from eight of Europe’s largest admixture producers and is an average of the normal plasticisers types detailed above.","Calculated","High","High","Medium","European Federation of Concrete Admixture Associations","EFCA ENVIRONMENTAL DECLARATION PLASTICISING ADMIXTURES – March 2006","European Federation of Concrete Admixture Associations","ISO 14000 series","PAS 2050","Unknown","Unknown","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","EU - Toluene",null,1.5,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Xylenes - mixed",null,1.6,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","EU",2005,2001,"PlasticsEurope Eco-profiles and EPDs represent European industry averages within\nthe scope of PlasticsEurope as the issuing trade federation.  As a general rule, Eco-profiles represent a minimum of three (3)\nproducers.","Calculated","High","High","Medium","Plastics Europe, Carbon Trust","Eco-profiles of the European Plastics Industry","I Boustead","ISO 14000 Series","PAS 2050","ISO 14000 Series","Mass","No","PAS 2050","Unknown","No","No"]
["Materials","EU - Zirconium",null,97.2,"kg CO2/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Cardboards ",null,0.58225000000000005,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1283","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Composites ",null,12.3,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1273","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Ferrous Ni < 5% (20-60% recycled material)  ",null,1.50475,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1271","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Ferrous Ni = 0% (20-60% recycled material)  ",null,1.3274999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1272","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Ferrous Ni > 5% (20-60% recycled material)  ",null,4.1054999999999993,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1270","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Glass (55-99% recycled material)  ",null,0.77975000000000005,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1274","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Non-ferrous 5 (15-45% recycled material)  ",null,10.2425,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1269","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Non-ferrous 8 (15-45% recycled material)  ",null,20.035,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1268","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Papers ",null,0.69,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1284","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Porous Ceramics ",null,0.42049999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1275","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Rubbers   ",null,1.825,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1279","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (Bar and Rod, 39% recycled)",null,1.86,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (coil sheet galvanised, 39% recycled)",null,2.0299999999999998,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (coil sheet, 39% recycled)",null,1.85,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (general, 39% recycled)",null,1.95,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (pipe, 39% recycled)",null,1.94,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (plate, 39% recycled)",null,2.21,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (section, 39% recycled)",null,2.0299999999999998,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (stainless, 39% recycled)",null,6.15,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Steel (wire, 39% recycled)",null,3.02,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GLO",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","GLO - Average Thermoplastics   ",null,3.625,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1277","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Thermosets epoxy  ",null,4.4249999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1276","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Thermosets PUR ",null,4.6775000000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1278","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Woods' HI ",null,0.88624999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1280","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Woods' LI ",null,0.65700000000000003,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1282","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","GLO - Average Woods' MI ",null,1.0069999999999999,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GLO",2005,2001,"Broad average of sector - only use for hotspots and low materiality products","Calculated","Low","High","Medium","Department of Technology, University of Kalmar","Life cycle inventory data for materials grouped according to environmental and material properties - Journal of Cleaner Production 13 (2005) 1258e1281","Carl Johan Rydh, Mingbo Sun ","Custom definition","Unknown","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","ITA - Average Clothing fabric (28% Elastan (Lycra) and 72% Polyamide)",null,2.21,"kg CO2(e)/m2","Cradle to RDC","Emission Factor","A","ITA",2009,2009,"Company specific processes and technologies","Calculated","Medium","High","Medium","International Environment Product Declaration System","Sensitive® Products Classic - Plus - Ultralight","EUROJERSEY Spa","ISO 14000 series","PAS 2050","Unknown","Unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","NZL - Average Glass (60% recycled) - NZL",null,0.57599999999999996,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","AUS",2005,2001,"Calculated using Ecoinvent report and modelled by CT","Calculated","Medium","High","High","Carbon Trust, Ecoinvent","EcoInvent 2.0, Carbon Trust","EcoInvent","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","N/A","PAS 2050"]
["Materials","South America - Feed crops for livestock - Soy  (Average -  land use change included)  ",null,9.4999175505148852,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA, ARG, BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","South America - Feed crops for livestock - Soy  (Average - no land use change)  ",null,0.31365891714230626,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA, ARG, BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","South America - Feed crops for livestock - Soy meal  (Average - no land use change)  ",null,0.26078369669040424,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA, ARG, BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","South America - Feed crops for livestock - Soy meal (Average - land use change included)  ",null,7.469048752690834,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA, ARG, BRA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Average Aggregate (gravel or crushed rock)",null,5.1999999999999998E-3,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimated from UK industrial fuel consumption data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Aggregates - fine aggregate",null,1.0135404682553542E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2007,"Data from two coarse aggregate quarries, modelled to UK fuel and electricity grid mix","Calculated","Medium","High","Medium","Carbon Trust, Department of Civil Engineering, Monash University","Green House Gas Emissions due to Concrete Manufacture","David J. M. Flower and Jay G. Sanjayan","PAS 2050","PAS 2050","Unknown","Unknown","No","PAS 2050","Unknown","No","Unknown"]
["Materials","UK - Average Aluminium (Cast, 33% recycled) ",null,9.2200000000000006,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","GBR",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Aluminium (Extruded, 33% recycled) ",null,9.08,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","GBR",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Aluminium (General, 33% recycled) ",null,9.16,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","GBR",2011,"Various","Large sample size, with many high quality data sources. ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Aluminium (Rolled, 33% recycled) ",null,9.18,"kg CO2e/kg","Cradle to Gate","Emission Factor","A","GBR",2011,"Various","Large sample size, with many high quality data sources. General aluminium assumed a UK ratio of 25.6% extrusions, 55.7% rolled & 18.7% castings and a worldwide average recycled content of 33% ","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Asphalt - road & pavement",null,0.14000000000000001,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Asphalt (4% Bitumen Binder Content)",null,6.6000000000000003E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Large data range, high standard deviation of values","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Asphalt (5% Binder Content)",null,7.0999999999999994E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Large data range, high standard deviation of values","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Asphalt (6% Binder Content)",null,7.5999999999999998E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Large data range, high standard deviation of values","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Asphalt (7% Binder Content)",null,8.1000000000000003E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Large data range, high standard deviation of values","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Asphalt (8% Binder Content)",null,8.5999999999999993E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Poor data availability and very large data range","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Bitumen",null,0.48,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Poor data quality, estimate based on the mix of fuels in the UK brass indsutry","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Brass (60% recycled)",null,2.64,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Bricks - (general)",null,0.24,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Bronze",null,4,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Calcium chloride - CaCl",null,0.60499999999999998,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","No"]
["Materials","UK - Average Calcium silicate sheet",null,0.13,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - felt (hair and jute) underlay",null,0.97,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Geoff Hammond and Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - general",null,3.9,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), carpet tiles, weight 1100 g/m2",null,19.7,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), carpet tiles, weight 300 g/m2",null,7.75,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), carpet tiles, weight 500 g/m2",null,10.7,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), carpet tiles, weight 700 g/m2",null,13.7,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), carpet tiles, weight 900 g/m2",null,16.7,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), pile weight 1100 g/m2",null,18.399999999999999,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), pile weight 300 g/m2",null,6.7,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), pile weight 500 g/m2",null,9.6999999999999993,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), pile weight 700 g/m2",null,12.7,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Nylon (Polyamide), pile weight 900 g/m2",null,15.6,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Polyethylterepthalate (PET)",null,5.56,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Polyprolylene",null,4.9800000000000004,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Polyurethane",null,3.76,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - Rubber",null,5.5449999999999999,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - saturated felt underlay (impregnated with asphalt or tar)",null,1.65,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Carpet - wool",null,5.53,"kg CO2/m2","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","General shortage of quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Cement - fibre",null,2.11,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - mortar (1:0.5:4.5 cement:Lime:sand mix)",null,0.21299999999999999,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - mortar (1:1:6 cement:Lime:sand mix)",null,0.17399999999999999,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement  -mortar (1:2:9 cement:Lime:sand mix)",null,0.155,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - mortar (1:3 cement:san mix)",null,0.221,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - mortar (1:4 cement:sand mix)",null,0.182,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - mortar (1:5 cement:sand mix)",null,0.156,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - mortar (1:6 cement:sand mix)",null,0.13600000000000001,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - Ordinary Portland Cement",null,0.93,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2006,"Calculated based on industry data","Calculated","Medium","Medium","Low","Sustainable Concrete","Sheet P1 - Embodied CO2 of UK cement, additions and cementitious material","Sustainable Concrete","Custom definition","PAS 2050","Unknown","unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","UK - Average Cement - Portland limestone cement (20% limestone)",null,0.75,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2006,"Calculated based on industry data","Calculated","Medium","Medium","Low","Sustainable Concrete","Sheet P2 - Embodied CO2 of factory made cements and combinations","Sustainable Concrete","Custom definition","PAS 2050","Unknown","unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","UK - Average Cement - Portland limestone cement (6% limestone)",null,0.88,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2006,"Calculated based on industry data","Calculated","Medium","Medium","Low","Sustainable Concrete","Sheet P2 - Embodied CO2 of factory made cements and combinations","Sustainable Concrete","Custom definition","PAS 2050","Unknown","unknown","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","UK - Average Cement - stabilised soil at 5%",null,6.0999999999999999E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cement - stabilised soil at 8%",null,8.4000000000000005E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Ceramic (fittings)",null,1.1399999999999999,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Ceramic (general)",null,0.7,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Ceramic (sanitary products)",null,1.61,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Ceramic (tiles and cladding panels)",null,0.78,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Chromium",null,5.39,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Calculated","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Clay pipe (vitrified DN 100 & DN 150)",null,0.46,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Clay pipe (vitrified DN 200 & DN 300)",null,0.5,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Clay pipe (vitrified DN 500)",null,0.55000000000000004,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Clay Products",null,0.24,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Clay tile",null,0.48,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on large amount of relatively modern data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (16/20 Mpa)",null,0.1,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (20/25 Mpa)",null,0.107,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (25/30 Mpa)",null,0.113,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (28/35 Mpa)",null,0.12,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (32/40 Mpa)",null,0.13200000000000001,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (40/50 Mpa)",null,0.151,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Concrete (general)",null,0.107,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Cotton - fabric",null,6.78,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Cotton - padding",null,1.28,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Damp proof course/membrane",null,4.2,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Flat glass",null,0.628,"kg CO2/kg","Cradle to Gate","Emission Factor","B","GBR",2006,2002,"Survey of the 3 flat glass manufacturing companies in the UK","Calculated","High","High","Medium","British Glass Manufacturers Confederation","UK GLASS MANUFACTURE - A MASS BALANCE STUDY","Envirowise","Custom definition","PAS 2050","Unknown","Unknown","No","CO2 only","Unknown","Unknown","No"]
["Materials","UK - Average Glass - fibreglass",null,1.54,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Glass - toughened",null,1.35,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Glass (38% recycled)",null,0.85,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Glass container",null,0.84299999999999997,"kg CO2/kg","Cradle to Gate","Emission Factor","B","GBR",2003,2002,"Survey of glass manufacturing facilities in UK","Calculated","High","High","Medium","British Glass Manufacturers Confederation","GLASS RECYCLING – LIFE CYCLE CARBON DIOXIDE EMISSIONS","Enviros","Custom definition","PAS 2050","Unknown","Unknown","No","CO2 only","Unknown","Unknown","No"]
["Materials","UK - Average Glass reinforced plastic - GRP fibreglass",null,8.1,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Grit",null,0.01,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Ground granulated blastfurnace slag (GGBS)",null,8.3000000000000004E-2,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Igneous rock - Granite/hornfels",null,2.5040566753351291E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2007,2007,"Data from two coarse aggregate quarries, modelled to UK fuel and electricity grid mix","Calculated","Medium","High","Medium","Carbon Trust, Department of Civil Engineering, Monash University","Green House Gas Emissions due to Concrete Manufacture","David J. M. Flower and Jay G. Sanjayan","PAS 2050","PAS 2050","Unknown","Unknown","No","PAS 2050","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - board",null,0.98,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - cork",null,0.19,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - fibreglass (glasswool)",null,1.35,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - flax",null,1.7,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - general",null,1.86,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - mineral wool",null,1.28,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - paperwool",null,0.63,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Insulation - rockwool (stonewool)",null,1.1200000000000001,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied energy and carbon data for insulation materials was relatively poor","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Lead (61.5% recycled)",null,1.67,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Mass allocation between lead and zinc applied","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","mass","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Lime",null,0.78,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Limestone (quarried and crushed)",null,1.7000000000000001E-2,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Linoleum",null,1.21,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Lithium",null,5.3,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Mandolite",null,1.4,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Manganese",null,3.5,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Marble",null,0.112,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Marble tile",null,0.187,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Mercury",null,4.9400000000000004,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Mineral fibre tile - roofing",null,2.7,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Molybedenum",null,30.3,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Nickel",null,12.4,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paint - double coat",null,0.87,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied carbon of paint within the literature had a particulatly high range, this made the selection of embodied carbon coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paint - general",null,2.91,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied carbon of paint within the literature had a particulatly high range, this made the selection of embodied carbon coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paint - single coat",null,0.44,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied carbon of paint within the literature had a particulatly high range, this made the selection of embodied carbon coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paint - solventborne",null,3.76,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied carbon of paint within the literature had a particulatly high range, this made the selection of embodied carbon coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paint - triple coat",null,1.31,"kg CO2e/m2","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied carbon of paint within the literature had a particulatly high range, this made the selection of embodied carbon coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paint - waterborne",null,2.54,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Embodied carbon of paint within the literature had a particulatly high range, this made the selection of embodied carbon coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Paper - fine paper",null,1.49,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Paper - paper label",null,2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GBR",2009,2007,"Based on case study","Calculated","Medium","Low","Low","Department for Environment, Food and Rural Affairs (DEFRA)","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Average Paper - paperboard (general for construction use)",null,1.29,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Paper - wallpaper",null,1.93,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Paperboard - general for construction use",null,1.32,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Perlite - expanded",null,0.52,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Perlite - natural",null,0.03,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Plaster - general",null,0.13,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Large variation in values, poor background data on carbon","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Plaster - plasterboard",null,0.39,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Large variation in values, poor background data on carbon","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Polythene bags ",null,1.39,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","C","GBR",2009,2007,"Based on case study","Calculated","Medium","Medium","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Average Quartz powder",null,0.02,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Rubber  - natural latex",null,1.63,"kg CO2e/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Limited data availability","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Rubber - general",null,2.85,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Limited data availability","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Rubber - synthetic",null,4.0199999999999996,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Sand and Gravel ",null,5.1000000000000004E-3,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Transport is a significant contributor to the cradle to gate embodied energy of sand.","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Sandstone",null,0.01,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2010,2009,"Case study of sandstone production in Scotland","Calculated","Low","High","Medium","Herriot Watt University","Embodied Carbon in Natural Building Stone in Scotland","Naeeda Crishna, Dr. Suzy Goodsir, Professor Phil Banfill, Dr. Keith Baker","Custom definition","PAS 2050","Unknown","Unknown","No","PAS 2050","Unknown","No","Unknown"]
["Materials","UK - Average Sealants & Adhesives (epoxide resin)",null,5.7,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Limited data from quality resources make selection of coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Sealants & Adhesives (melamine resin)",null,4.1900000000000004,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Limited data from quality resources make selection of coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Sealants & Adhesives (phenol formaldehyde)",null,2.98,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Limited data from quality resources make selection of coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Sealants & Adhesives (urea formaldehyde)",null,2.76,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Limited data from quality resources make selection of coefficients difficult","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Shale",null,2E-3,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Shingle",null,0.3,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Silver",null,6.31,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Single baked clay products",null,0.22,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Slate",null,5.6000000000000001E-2,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Soil (cement stabilised at 5%)",null,6.0999999999999999E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Soil (cement stabilised at 8%)",null,8.4000000000000005E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Soil (fly ash stabilised)",null,4.1000000000000002E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Soil (general rammed)",null,2.4E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Soil (GGBS stabilised)",null,4.7E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (Bar and Rod, 59% recycled)",null,1.4,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (Coil Sheet Galvanised, 59% recycled)",null,1.54,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (Coil Sheet, 59% recycled)",null,1.38,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (General, 59% recycled)",null,1.46,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (Pipe, 59% recycled)",null,1.45,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (Plate, 59% recycled)",null,1.66,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Steel (Section, 59% recycled)",null,1.53,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (general)",null,7.9000000000000001E-2,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (granite)",null,0.7,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (limestone)",null,0.09,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (marble tile)",null,0.21,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (marble)",null,0.13,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (sandstone)",null,0.06,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone (shale)",null,2E-3,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Stone gravel/chippings",null,1.7000000000000001E-2,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Terrazzo tiles",null,0.12,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Tin",null,14.47,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Generally poor quality data","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Vanadium",null,228,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Vermiculite - expanded",null,0.52,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Vermiculite - natural",null,0.03,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Vinasses ",null,0.63700000000000001,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2005,"Calculated based on case study","Calculated","Medium","High","High","National Non-Food Crops Centre and North Energy","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter (2009) Life cycle assessment workbooks for selection of major renewable chemicals, NNFCC and North Energy.","Mortimer, N., A. Evans, A. Ashley, C. Hatto, V. Shaw, C. Whittaker and A. Hunter ","Custom definition","PAS 2050","PAS 2050","economic","No","Kyoto gases only","Unknown","No","Unknown"]
["Materials","UK - Average Vinyl Flooring (general) ",null,3.19,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Wallpaper",null,1.93,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Wood stain/varnish",null,5.35,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Wool ",null,5.53,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Yttrium",null,84,"kg CO2/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Average Zinc (16% recycled) ",null,3.31,"kg CO2/kg","Cradle to Gate","Emission Factor","C","GBR",2008,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 1.6a","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","CO2 only","Unknown","No","Unknown"]
["Materials","UK - Average Zinc (30% recycled) ",null,3.09,"kg CO2e/kg","Cradle to Gate","Emission Factor","B","GBR",2011,"Various","Estimation based on existing literature and applying the UK electricity and fuel mix","Estimation","Medium","Low","Low","University of Bath","Inventory of Carbon Energy (ICE) version 2.0","Prof. Geoff Hammond & Craig Jones","Custom definition","PAS 2050","Unknown","unknown","No","PAS2050","Unknown","No","Unknown"]
["Materials","UK - Feed crops for livestock - Beet Molasses  ",null,0.11,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2009,2008,"Carbon Trust Certified Model.  For key assumptions see the Footprint Expert Guide.","Calculated","High","High","High","Carbon Trust, project partners","N/A","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Brewers Grain  ",null,0.03,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2008,2007,"Carbon Trust Certified Model.  For key assumptions see the Footprint Expert Guide.","Calculated","High","High","High","Carbon Trust, project partners","N/A","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Cane Molasses  ",null,0.15,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","BRA",2009,2008,"Carbon Trust Certified Model.  For key assumptions see the Footprint Expert Guide.","Calculated","High","High","High","Carbon Trust, project partners","N/A","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Citrus Pulp (wet)",null,1.4999999999999999E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","Brazil",2008,2007,"Carbon Trust Certified Model.  For key assumptions see the Footprint Expert Guide.","Calculated","High","High","High","Carbon Trust, project partners","N/A","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Distillers Grains (wet) ",null,0.03,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2008,2007,"Carbon Trust Certified Model.  For key assumptions see the Footprint Expert Guide.","Calculated","High","High","High","Carbon Trust, project partners","N/A","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Fodder Beet  ",null,3.047492927922078E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Forage Maize  ",null,4.7465439712425249E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Forage Rape  ",null,4.3628335800902251E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Kale (Direct Drilled)  ",null,3.8149391828571425E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Maize Gluten  ",null,0.33800000000000002,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2008,2007,"Carbon Trust Certified Model.  For key assumptions see the Footprint Expert Guide.","Calculated","High","High","High","Carbon Trust, project partners","N/A","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Maize Silage  ",null,0.18,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"whole crop maize, cut and clamped for feeding dairy cattle.","Estimation","Medium","Medium","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - OSR Meal (Spring)  ",null,0.44779144442712387,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - OSR Meal (Winter)  ",null,0.40458306427637536,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Second Wheat  ",null,0.40536727046228566,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Second Wheat- (milled & 10% dried)  ",null,0.45794137322121531,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Second Wheat (milled & 6% dried)  ",null,0.45628161329720285,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Spring Barley   ",null,0.35381648356715789,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Spring Barley (milled & 6% dried)  ",null,0.40344911496596281,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Spring Oats  ",null,0.29870164386243397,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Spring Oats (milled & 10% dried)  ",null,0.34607341616201215,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Spring Oats (milled & 6% dried)  ",null,0.34361451257088238,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Spring Oilseed Rape  ",null,0.96506776816190498,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Stubble Turnips  ",null,5.8639920625000001E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Sugar Beet  ",null,3.1317869489051096E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Turnips  ",null,2.4693153877551017E-2,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - whole crop cereal  ",null,0.11484918368347825,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Barley  ",null,0.36742462230399997,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Barley (milled & 10% dried)  ",null,0.41766832492468692,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Barley (milled & 6% dried)  ",null,0.41577145644010122,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Field Beans  ",null,0.13334975180715791,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Field Beans   ",null,0.133191141544,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Oats  ",null,0.30749749361344542,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Oats (milled & 10% dried)  ",null,0.35214557867067348,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Oats (milled & 6% dried)  ",null,0.35019291993654106,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Oilseed Rape  ",null,0.8719462592163264,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Wheat  ",null,0.34417004150006097,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Wheat (milled & 10% dried)  ",null,0.38943876912456588,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Feed crops for livestock - Winter Wheat (milled & 6% dried)  ",null,0.38794685009174568,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","GBR",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Medium","High","High","Modelled by Carbon trust using the following sources: Agro Business Consultants, John Nix, Carbon Trust, ADAS Consultants, DEFRA, EcoInvent"," Agricultural Budgeting & Costing Book 70th Edition; John Nix Farm Management Pocketbook 40th edition\n"," Agricultural Budgeting & Costing Book 70th Edition - Richard King; ohn Nix Farm Management Pocketbook 40th edition - John Nix","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Oilseed rape - Conventional ",null,0.7,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"Conventional OSR was drilled after min-til cultivations, using heavy discs. Fertiliser\napplications were made as per BSFP, 2007. The oilseed rape crop was harvested\nand dried by 3%, then processed for oil. The OSR meal was produced as a coproduct\nwas then feed to livestock.","Calculated","Medium","Medium","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","UK - Oilseed rape - Organic ",null,0.64,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","B","GBR",2009,2007,"Organic OSR was drilled after discing, then rolled. Nutrition was supplied as a result\nof clover ley earlier in the rotation (50% of emissions allocated from clover ley). The\noilseed rape crop was harvested dried by 3% and then processed for oil. The meal\nwas produced as a co-product was then feed to livestock.","Calculated","Medium","Medium","Medium","Department for Environment, Food and Rural Affairs (DEFRA) ","Scenario building to test and inform the development of a BSI method for assessing greenhouse gas emissions from food. Report to Defra, Project Reference Number: FO0404. ADAS, London, 2009. ","Jeremy Wiltshire, Adrian Williams et al.","PAS 2050","PAS 2050","PAS 2050","multiple","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","USA - Feed crops for livestock - Soy (average - no land use change)    ",null,0.39337556067869256,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","USA - Feed crops for livestock - Soy (land use change included)  ",null,6.9318370991402318,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","USA - Feed crops for livestock - Soy meal (average - no land use change)    ",null,0.32271575293227611,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["Materials","USA - Feed crops for livestock - Soy meal (land use change included)  ",null,5.4533097965697985,"kg CO2(e)/kg","Cradle to Gate","Emission Factor","A","USA",2010,2009,"For key assumptions see the Footprint Expert Guide.","Calculated","Unknown","High","High","Modelled by Carbon trust using the following sources: Renewable Transport Fuels Obligation (RTFO), Carbon Trust, Omnitech International, DEFRA","http://www.renewablefuelsagency.gov.uk/aboutthertfo","Carbon Trust","PAS 2050","PAS 2050","PAS 2050","Economic","No","PAS 2050","PAS 2050","No","PAS 2050"]
["processing","thermoforming, with calendering",null,0.78244000000000002,"kg CO2(e)/kg"]
["processing","extrusion, plastic film",null,0.52405000000000002,"kg CO2(e)/kg"]
["Passenger Transport","Average Storage at port - Timber",null,30,"days","N/A","Activity Data","B","GBR",2009,2009,"Calculated using information from projects","Estimation","Medium","High","High","Carbon Trust","N/A","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Passenger Transport","Passenger - Air Short Haul Average",null,9.9239999999999995E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Air Short Haul Business Class",null,0.14186000000000001,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Air Short Haul Economy Class",null,9.4579999999999997E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Air Travel Business class",null,0.23988000000000001,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Air Travel Long Haul Average",null,0.11330999999999999,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Air Travel Long Haul First class",null,0.33087,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Air Travel Long Haul Premium economy class",null,0.13235000000000002,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Average bus",null,0.10462,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Average bus and coach",null,6.9120000000000001E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Average diesel car",null,0.19833999999999999,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Average LPG or CNG car",null,0.22452,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Black cab",null,0.17173999999999998,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Coach",null,3.0619999999999998E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Diesel van (Class I), up to 1.305 tonne",null,0.16197,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Diesel van (Class II), 1.305 to 1.74 tonne",null,0.22645000000000001,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Diesel van (Class III), 1.74 to 3.5 tonne",null,0.30135999999999996,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - International rail (Eurostar)",null,1.7779999999999997E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Large diesel cars, above 2.0 litres",null,0.25762000000000007,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Large LPG or CNG car",null,0.26068000000000002,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Large petrol cars, above 2.0 litres",null,0.29760999999999999,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Large petrol hybrid car",null,0.22600000000000001,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Large petrol motorbike (over 500cc)",null,0.13977000000000001,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Light rail and tram",null,8.3989999999999995E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - London Underground",null,7.8549999999999995E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Medium diesel car, from 1.4 - 2.0 litres",null,0.18938999999999998,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Medium LPG or CNG car",null,0.18834000000000001,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Medium petrol car, from 1.4 - 2.0 litres",null,0.21493999999999999,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Medium petrol hybrid car",null,0.12822000000000003,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Medium petrol motorbike (125-500cc)",null,0.10568,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - National rail",null,6.1129999999999997E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Passenger - Local bus",null,0.11152999999999999,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Passenger - London bus",null,8.3770000000000011E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Petrol van up to 1.25 tonne",null,0.22824000000000003,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Regular taxi",null,0.15964999999999999,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Small diesel car, up to 1.4 litre engine",null,0.15276999999999999,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger - Small petrol car, up to 1.4 litre engine",null,0.18200000000000002,"kg CO2(e)/km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Passenger Transport","Passenger -Air Long Haul Travel Economy class",null,8.2720000000000002E-2,"kg CO2(e)/passenger km","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Survey/study of existing transport modes and associated emissions ","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from DEFRA 2009 GHG conversion factors","DEFRA","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","No"]
["Transport","Air Domestic (UK) - UK",null,2.3454490937019972,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Air Long Haul",null,0.71750809989597286,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Air Short Haul",null,2.2472448409283112,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Rail (diesel)",null,2.4983557090330025E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","EU",2007,2006,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","Imported from CT Model (using data from Defra 2007, Dukes Digest 2006, & EcoInvent data v1.3)","CTFC","N/A","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Rail (electric) ",null,4.2700000000000002E-2,"kWh/tonne/km","N/A","Conversion Factor","A","EU",2008,2006,"Calculated from official government reports","Calculated","High","High","High","Carbon Trust, DEFRA, Digest of United Kingdom energy statistics (DUKES), EcoInvent","EcoTranIT: Environmental Methodology and Data update 2008","EcoTransIT","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Artic Lorry Over 33 tonne (5 / 6-axle)",null,1.0645215831188909E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Rigid Lorry 14 to 17 tonne (2-axle)",null,4.3849687346219947E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Rigid Lorry 17 to 25 tonne (3-axle)",null,2.4839491552498774E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Rigid Lorry 25 to 32 tonne (4-axle)",null,2.5727254100127044E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Rigid Lorry 3.5 to 7.5 tonne (2-axle)",null,6.4234912728520527E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Rigid Lorry 7.5 to 14 tonne (2-axle)",null,4.2503425015414951E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 2b Diesel Vehicles",null,9.9902212038455354E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 4 Diesel Vehicles",null,7.060659845888502E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 5 Diesel Vehicles",null,6.2601943821153805E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 6 Diesel Vehicles",null,5.370432112610795E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 7 Diesel Vehicles",null,4.9940078321725895E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 8a Diesel Vehicles",null,2.091332876423636E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US - Class 8b Diesel Vehicles",null,1.351492830004016E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US -Class 3 Diesel Vehicles",null,0.17499999999999999,"litres diesel / km / tonne capacity","N/A","Activity Data","A","GBR",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","US -Class 3 Diesel Vehicles",null,7.5993362204751794E-2,"litres diesel / km / tonne capacity","N/A","Activity Data","A","USA",2009,2008,"Calculated using existing literature","Calculated","Medium","High","High","PE Americas, Carbon Trust, DEFRA, Department of Transport (UK)","PE Americas, Carbon Trust 2009, DEFRA 2009, DfT 2008","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Bulk Carrier - Large",null,8.1887893502478014E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk Carrier - Small ",null,1.3086848849635615E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier 0–9999 dwt  - GLO",null,3.4403388632872504E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier 10,000–34,999 dwt  - GLO",null,9.3076774193548394E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier 100,000–199,999 dwt - GLO",null,3.5292258064516129E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier 200,000+ dwt  - GLO",null,2.9492258064516127E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier 35,000–59,999 dwt  - GLO",null,6.7084516129032263E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier 60,000–99,999 dwt  - GLO",null,4.8288387096774186E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Bulk carrier Average - GLO",null,4.1188387096774198E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general - average - GLO",null,1.5376129032258067E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general 0–4999 dwt  - GLO",null,1.637574193548387E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general 0–4999 dwt 100+ TEU  - GLO",null,2.3336098310291861E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general 10,000+ dwt  - GLO",null,1.401651612903226E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general 10,000+ dwt 100+ TEU  - GLO",null,1.295690322580645E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general 5000–9999 dwt  - GLO",null,1.862725960061444E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Cargo, general 5000–9999 dwt 100+ TEU  - GLO",null,2.0626872503840248E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container 0–999 TEU  - GLO",null,4.2771066052227344E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container 1000–1999 TEU  - GLO",null,3.7832227342549922E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container 2000–2999 TEU  - GLO",null,2.3566098310291859E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container 3000–4999 TEU  - GLO",null,1.9566872503840246E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container 5000–7999 TEU  - GLO",null,1.9566872503840246E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container 8000+ TEU  - GLO",null,1.4726129032258065E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container Average - GLO",null,1.8767259600614438E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container Vessel - Large ",null,1.5207751650460202E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Container Vessel - Small",null,1.7845702976775839E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Ferry, large RoPax - GLO",null,0.4528786635944701,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Ferry, Ro–Ro  - average - GLO",null,6.0038712749615974E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Ferry, Ro–Ro  0–1999 LM  - GLO",null,7.1056003072196616E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Ferry, Ro–Ro  2000+ LM  - GLO",null,5.8329099846390176E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker - Large ",null,5.8491352501770016E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker - Small ",null,2.379427063570112E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker - Very Large ",null,4.6793082001416013E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, chemical - average - GLO",null,1.1996903225806451E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, chemical 0–4999 dwt  - GLO",null,2.6165324116743473E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, chemical 10,000–19,999 dwt  - GLO",null,1.2716903225806452E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, chemical 20,000+ dwt  - GLO",null,9.88767741935484E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, chemical 5000–9999 dwt - GLO",null,1.7795354838709677E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) 0–9999 dwt - GLO",null,3.9241840245775726E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) 10,000–59,999 dwt - GLO",null,1.0717290322580645E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) 120,000–199,999 dwt - GLO",null,5.1788387096774191E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) 200,000+ dwt - GLO",null,3.4092258064516126E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) 60,000–79,999 dwt - GLO",null,8.8376774193548394E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) 80,000–119,999 dwt - GLO",null,6.9580645161290335E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, crude (oil) average - GLO",null,5.308838709677419E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, LNG 0–199,999 m3  - GLO",null,1.7075741935483869E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, LNG 200,000+ m3  - GLO",null,1.0957290322580646E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, LNG Average - GLO",null,1.341651612903226E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, LPG 0–49,999 m3  - GLO",null,5.1249130568356373E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, LPG 50,000+ m3  - GLO",null,1.0607290322580645E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, products  10,000–19,999 dwt - GLO",null,2.2036485407066049E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, products  20,000–59,999 dwt - GLO",null,1.2136903225806451E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, products  5000–9999 dwt - GLO",null,3.4403388632872504E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, products  60,000+ dwt - GLO",null,6.7084516129032263E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, products  Average - GLO",null,1.0497290322580646E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Tanker, products 0–4999 dwt - GLO",null,5.3028356374807982E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Waste Lorry",null,2.340057152073733E-2,"kg CO2(e)/kg of waste","Gate to Gate","Emission Factor","A","GBR",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009, Data Collection from Suppliers)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Additional fuel use for Chilled Products - Container Ship",null,4.0269805303974802E-2,"kg CO2/container/km","N/A","Emission Factor","B","GLO",2009,2007,"Calculated from projects/existing reports","Estimation","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","CO2 only","N/A","N/A","PAS 2050"]
["Transport","Additional fuel use for Frozen Products - Container Ship",null,1.6107922121589922E-2,"kg CO2/tonne/km","N/A","Emission Factor","B","GLO",2009,2007,"Calculated from projects/existing reports","Estimation","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","CO2 only","N/A","N/A","PAS 2050"]
["Transport","Refrigerant loss from sea freight",null,3.4843995730782736E-3,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2009,2007,"Calculated from government reports and literature","Calculated","Medium","High","High","Carbon Trust, DEFRA, EcoInvent","Imported from CT Model (using data from Defra 2009& EcoInvent data v2.0)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","LCF - Artic Lorry Over 33 tonne (5 / 6-axle)",null,0.66600000000000004,"number","N/A","Activity Data","A","GBR",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - Rigid Lorry 14 to 17 tonne (2-axle)",null,0.111,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - Rigid Lorry 17 to 25 tonne (3-axle)",null,0.438,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - Rigid Lorry 25 to 32 tonne (4-axle)",null,0.438,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - Rigid Lorry 3.5 to 7.5 tonne (2-axle)",null,0.17499999999999999,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - Rigid Lorry 7.5 to 14 tonne (2-axle)",null,0.111,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 2b Diesel Vehicles",null,0.17499999999999999,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 4 Diesel Vehicles",null,0.17499999999999999,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 5 Diesel Vehicles",null,0.111,"number","N/A","Activity Data","A","USA",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 6 Diesel Vehicles",null,0.111,"number","N/A","Activity Data","A","GBR",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 7 Diesel Vehicles",null,0.111,"number","N/A","Activity Data","A","GBR",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 8a Diesel Vehicles",null,0.27500000000000002,"number","N/A","Activity Data","A","GBR",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","LCF - US - Class 8b Diesel Vehicles",null,0.66600000000000004,"number","N/A","Activity Data","A","GBR",2008,2007,"Calculated using official DEFRA data","Calculated","Medium","High","High","Carbon Trust, DEFRA","Imported from CT Model (using data from Defra 2008, Continuing Survey of Road Goods Transport, & EcoInvent data v1.3)","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average Distance to between RDC and Store (UK)",null,60,"miles","N/A","Activity Data","B","GBR",2009,2009,"Calculated using information from projects","Estimation","Medium","High","High","Carbon Trust","N/A","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Agricultural products",null,114,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Beverages",null,131,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Building materials",null,62,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Chemicals",null,136,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Coal and coke",null,70,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Crude materials",null,114,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Crude minerals",null,42,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Fertiliser",null,62,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Iron and steel products",null,126,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Machinery and transport equipment",null,118,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Miscellaneous articles",null,82,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Miscellaneous manufactures",null,133,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Ores",null,74,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Other foodstuffs",null,117,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Other metal products",null,91,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Petrol and petroleum products",null,81,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by commodity - Wood, timber and cork",null,115,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Artic Lorry 3.5t to 33t",null,112,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Artic Lorry Over 33 tonne (5 / 6-axle)",null,121,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - average across all truck types",null,87,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Average all Artics",null,120,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Rigid Lorry 17 to 25 tonne (3-axle)",null,60.5,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Rigid Lorry 25 to 32 tonne (4-axle)",null,38,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Rigid Lorry 3.5 to 7.5 tonne (2-axle)",null,54,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average length of haul by truck type - Rigid Lorry 7.5 to 17 tonne (2-axle)",null,53,"km","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Agricultural, forestry and fishing",null,0.623,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Banking, finance and services",null,0.746,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Construction",null,0.57499999999999996,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Energy and water supply",null,0.57200000000000006,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Manufacture, mining and quarrying",null,0.69499999999999995,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Transport, storage and communication",null,0.76400000000000001,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by business type - Wholesale & retail trade, repairs and hotels",null,0.73699999999999999,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by truck type - Artic Lorry Over 33 tonne (5 / 6-axle)",null,0.70899999999999996,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by truck type - Rigid Lorry 17 to 25 tonne (3-axle)",null,0.74,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by truck type - Rigid Lorry 25 to 32 tonne (4-axle)",null,0.86799999999999999,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by truck type - Rigid Lorry 3.5 to 7.5 tonne (2-axle)",null,0.74,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average load of vehicle by truck type - Rigid Lorry 7.5 to 17 tonne (2-axle)",null,0.73499999999999999,"%","N/A","Activity Data","A","GBR",2009,2007,"Study using surveys/sampling","Calculated","Medium","High","Medium","Department for Transport, UK","Road Freight Statistics 2008","Department for Transport, UK","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average Storage at Port - Paper and other Packing materials",null,20,"days","N/A","Activity Data","B","GBR",2009,2009,"Calculated using information from projects","Estimation","Medium","High","High","Carbon Trust","N/A","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average Storage at Port - Perishables",null,1,"days","N/A","Activity Data","B","GBR",2009,2009,"Calculated using information from projects","Estimation","Medium","High","High","Carbon Trust","N/A","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Average Storage at port Newsprint",null,50,"days","N/A","Activity Data","B","GBR",2009,2009,"Calculated using information from projects","Estimation","Medium","High","High","Carbon Trust","N/A","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Fuel Use - Uplift for chilled / frozen",null,0.14000000000000001,"% uplift on base transport emissions","N/A","Activity Data","B","GBR",2006,2005,"Study using surveys/sampling","Estimation","Medium","High","High","Carbon Trust","N/A","CTFC","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A","N/A"]
["Transport","Lorry (all types, average) - UK",null,0.15054000000000001,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (articulated, >3.5-33t) - UK",null,0.18400000000000002,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (articulated, >33t) - UK",null,0.10461999999999999,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (articulated, average) - UK",null,0.10692000000000002,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (rigid, >17t) - UK",null,0.24130000000000001,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (rigid, >3.5-7.5t) - UK",null,0.79456000000000004,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (rigid, >7.5-17t) - UK",null,0.49692000000000003,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Lorry (rigid, average) - UK",null,0.30259999999999998,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GBR",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Refrigerated cargo  All dwt - GLO",null,1.5196129032258065E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Vehicle transport 0–3999 CEU  - GLO",null,6.7876777265745009E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Vehicle transport 4000+ CEU  - GLO",null,3.771222734254992E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Transport","Vehicle transport Average - GLO",null,4.4830678955453153E-2,"kg CO2(e)/tonne/km","Gate to Gate","Emission Factor","A","GLO",2010,2008,"Calculated from reports","Calculated","Medium","High","High","Carbon Trust, DEFRA, European Comission Joint Research Centre","Imported from CT Model (using data from 2010 Guidelines to Defra / DECC's GHG Conversion Factors for Company Reporting and Well-to-Wheels analysis of future automotive fuels and powertrains in the European context WELL-TO-TANK Report Version 3.0 November 2008)","CTFC","PAS 2050","PAS 2050","No","None","No","PAS 2050","N/A","N/A","PAS 2050"]
["Waste Treatment","Average End of Life Emissions - Bio waste - Austria",null,3.8431788727499995E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","AUT",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Bio waste - UK",null,0.16812363410276543,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Cardboard packaging - EU",null,0.17565231640797865,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Cardboard packaging - France",null,6.1539090091030604E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Cardboard packaging - Germany",null,3.8746834501760005E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Cardboard packaging - UK",null,0.1895018259709155,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Commercial Waste - Combustion Wastes - UK ",null,0.1164223085962348,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Commercial Waste - Metallic Wastes - UK ",null,2.6334362647294058E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Commercial Waste - Other animal by-products - UK ",null,0.19543387607709622,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Commercial Waste - Other mineral wastes - UK  ",null,3.5244619727692376E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Commercial Waste - Paper and Card - UK ",null,0.14196936505773083,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - Austria",null,9.3512475000000039E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","AUT",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - Denmark",null,1.2181701724137954E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DNK",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - Germany",null,3.4171034722222243E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - Ireland",null,2.4273576923076797E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","IRL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - Netherlands",null,4.7525887500000042E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","NLD",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - Spain",null,3.0226254545454554E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ESP",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Construction and Demolition - UK",null,1.389316923076925E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Austria",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","AUT",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Belgium",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","BEL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Denmark",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DNK",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - EU 25 + Norway",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Finland",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FIN",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - France",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Germany",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Ireland",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","IRL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Italy",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ITA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Netherlands",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","NLD",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Norway",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","NOR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Portugal",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","PRT",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Spain",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ESP",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - Sweden",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","SWE",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Glass - UK",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Liquid cartons - EU",null,0.17565231640797865,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Liquid cartons - France",null,6.1539090091030604E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Liquid cartons - Germany",null,8.0937832070343118E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Liquid cartons - UK",null,0.1895018259709155,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Magazines - EU",null,0.12625010241823464,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Magazines - France",null,4.4231221002928249E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Magazines - Germany",null,2.7849287298139999E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Magazines - UK",null,0.13620443741659549,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Newspapers - EU",null,9.6059860535613315E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Newspapers - France",null,3.3654189893532353E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Newspapers - Germany",null,2.1189675118150003E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Newspapers - UK",null,0.10363381107784438,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other cardboard - EU",null,0.17565231640797865,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other cardboard - France",null,6.1539090091030604E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other cardboard - Germany",null,3.8746834501760005E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other cardboard - UK",null,0.1895018259709155,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other paper - EU",null,0.26896760949971726,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other paper - France",null,9.4231731701890573E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other paper - Germany",null,5.9331090330819996E-3,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Other paper - UK",null,0.29017467101796435,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","High","Eurostat, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Belgium",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","BEL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Denmark",null,8.8359982090273625E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DNK",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - EU",null,0.13374972847282593,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - France",null,2.9904783088235281E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Germany",null,0.17007258491781246,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","IRL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Ireland",null,6.3310536430274678E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ITA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Italy",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","NLD",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Netherlands",null,0.29110675621890564,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ESP",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Spain",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","SWE",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - Sweden",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (dense)  - United Kingdom",null,2.1938988430627922E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Belgium",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","BEL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Denmark",null,7.7073123064143781E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DNK",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - EU",null,0.13374972847282593,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","EU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - France",null,2.6084829044117637E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","FRA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Germany",null,0.11104078445121952,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","DEU",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Ireland",null,6.3310536430274678E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","IRL",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Italy",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ITA",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Netherlands",null,0.29110675621890564,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","NLD",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Spain",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","ESP",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - Sweden",null,0,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","SWE",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]
["Waste Treatment","Average End of Life Emissions - Plastic (film) - United Kingdom",null,2.1938988430627922E-2,"kg CO2(e)/kg of waste","Gate to Grave","Emission Factor","A","GBR",2008,2007,"Modelled by CT using variety of activity data of waste scenarios","Calculated","Medium","High","Medium","Plastics Europe, European Environment Agency, Confederation of European Waste-to-Energy Plants and modelling by the Carbon Trust","Diverting waste from landfill Effectiveness of waste‑management policies in the European Union; Environment in the EU27\n40% of municipal waste recycled or composted in 2008; 2008 Country Reports on Waste Management (CEWEP)","Eurostat, European Environment Agency, and Confederation of European Waste-to-Energy Plants","PAS 2050","PAS 2050","No","None","No","PAS 2050","PAS 2050","No","Unknown"]

{"sheet":"Typical heat sources","index":11,"n_rows":72,"n_cols":4,"rows_kept":72,"cut":false,"hidden":true,"merged":[]}
["Country/Region","Predominant heat source","Source","Proxy"]
["Africa",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Argentina ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Asia subcontinent","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["Australia",null,null,"Fuel: Natural gas - VIC- AUS"]
["Austria","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Bangladesh ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Belgium ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Brazil ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Bulgaria ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Canada ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Central/Eastern Europe","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Chile",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["China ","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["Colombia ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Costa Rica ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Cyprus",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Czech Republic","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["Denmark","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Ecuador ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Egypt",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["EU 27","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Finland ","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["France ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Germany ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Greece ","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["Guatemala ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Hungary ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["India ","Coal","?","Fuel: Coal (Emissions per net kWh)"]
["Indonesia ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Ireland (Republic of) ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Israel ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Italy ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Japan ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Kenya ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Latin America",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Latvia","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Malaysia ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Malta ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Mexico ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Middle East",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Netherlands ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["New Zealand ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Non-OECD total","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["North America",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Norway ","Waste","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["OECD total","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Pakistan",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Panama",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Peru",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Philippines",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Poland ","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["Portugal ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Romania ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Russia ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Saudi Arabia",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Serbia ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Singapore ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["South Africa ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["South East Asia","Coal","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Coal (Emissions per net kWh)"]
["South Korea ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Spain ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Sweden ","Biofuels","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Taiwan",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Thailand",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Turkey ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["Ukraine ","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["United Arab Emirates (UAE)",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["United Kingdom","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, UK) (Emissions per net kWh)"]
["US Average","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Emissions per net kWh) - USA"]
["Vietnam ",null,null,"Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]
["World average","Gas","http://www.iea.org/stats/prodresult.asp?PRODUCT=Electricity/Heat","Fuel: Natural Gas (Low Pressure, medium upstream emission countries) (net kWh)"]

{"sheet":"Packaging EFs","index":12,"n_rows":12,"n_cols":10,"rows_kept":12,"cut":false,"hidden":true,"merged":[]}
["Material","Emission Factor Proxy","Material EF (kgCO2e/kg)","Commercial EF (kg CO2e/kg waste)","Domestic EF (kg CO2e/kg waste)","End of Life EFs ---->","Material","EF (kg CO2e/kg waste)","Source","Notes"]
["Paper","GLO - Average Papers ",{"$f":"VLOOKUP(B2,'FPX Reference Data'!B:D,3,FALSE)","v":0.69},{"$f":"H4","v":0.14365412167507999},{"$f":"H5","v":0.67983887514289199},null,"Card - Commercial",4.2197908641771899E-2,"FPX calculator","Figures here account for recycling rates"]
["Cardboard","GLO - Average Cardboards ",{"$f":"VLOOKUP(B3,'FPX Reference Data'!B:D,3,FALSE)","v":0.58225000000000005},{"$f":"H2","v":4.2197908641771899E-2},{"$f":"H3","v":0.19970035255439},null,"Card - Domestic",0.19970035255439,"FPX calculator","Figures here account for recycling rates"]
["Aluminium","EU - Virgin Aluminium (General Use)",{"$f":"VLOOKUP(B4,'FPX Reference Data'!B:D,3,FALSE)","v":12.79},0,0,null,"Paper - Commercial",0.14365412167507999,"FPX calculator","Figures here account for recycling rates"]
["HDPE - blister","EU - Virgin HDPE Resin",{"$f":"VLOOKUP(B5,'FPX Reference Data'!B:D,3,FALSE)","v":1.9},{"$f":"$H$6","v":2.1930000000000002E-2},{"$f":"$H$7","v":2.1930000000000002E-2},null,"Paper - Domestic",0.67983887514289199,"FPX calculator","Figures here account for recycling rates"]
["HDPE - film","EU - Virgin HDPE Resin",{"$f":"VLOOKUP(B6,'FPX Reference Data'!B:D,3,FALSE)","v":1.9},{"$f":"$H$6","v":2.1930000000000002E-2},{"$f":"$H$7","v":2.1930000000000002E-2},null,"Plastic - Commerical",2.1930000000000002E-2,"FPX 3.3 Database"]
["PET - blister","EU - Virgin PET Bottle Grade",{"$f":"VLOOKUP(B7,'FPX Reference Data'!B:D,3,FALSE)","v":3.4},2.1930000000000002E-2,2.1930000000000002E-2,null,"Plastic - Domestic",2.1930000000000002E-2,"FPX 3.3 Database"]
["PET - film","EU - Virgin PET Film",{"$f":"VLOOKUP(B8,'FPX Reference Data'!B:D,3,FALSE)","v":5.4},2.1930000000000002E-2,2.1930000000000002E-2]
["PVC - blister","EU - Virgin Polyvinylchloride (PVC) (suspension polymerisation)",{"$f":"VLOOKUP(B9,'FPX Reference Data'!B:D,3,FALSE)","v":1.9},2.6824399999999997]
["PVdC - blister","EU - Virgin Polyvinylidene chloride (PVdC)",{"$f":"VLOOKUP(B10,'FPX Reference Data'!B:D,3,FALSE)","v":4.4000000000000004},5.1824400000000006]
["PP - bottle",{"$f":"'FPX Reference Data'!B760","v":"EU - Virgin Polypropylene (injection moulded)"},{"$f":"VLOOKUP(B11,'FPX Reference Data'!B:D,3,FALSE)","v":4.4059114856022896},2.1930000000000002E-2,2.1930000000000002E-2]
["PP - film","EU - Virgin PP Resin",{"$f":"VLOOKUP(B12,'FPX Reference Data'!B:D,3,FALSE)","v":2},2.1930000000000002E-2,2.1930000000000002E-2]

{"sheet":"TRANSPORT ----->","index":13,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Transport EFs","index":14,"n_rows":46,"n_cols":5,"rows_kept":46,"cut":false,"hidden":true,"merged":[]}
["ASSUMPTIONS"]
[]
["Mode","Type","Value","Units","Source"]
["Air distance","Long Haul",9000,"km","Rounded Shanghai - Pu Dong to London Stanstead (taken from http://www.world-airport-codes.com/)"]
["Air distance","Short Haul",1500,"km","Rounded Warsaw - Frédéric Chopin to London Stanstead (taken from http://www.world-airport-codes.com/)"]
["Air distance","Domestic",400,"km","Rounded Newcastle to London Stanstead (taken from http://www.world-airport-codes.com/)"]
["Road distance","Long haul",2500,"km"]
["Road distance","Short haul",500,"km"]
["Road distance","Domestic",100,"km"]
["Sea Distance","Shanghai to Hull",19500,"km","www.searates.com"]
["Sea Distance","Nigeria to Hull",8000,"km","www.searates.com"]
["Sea Distance","Hamburg to Hull",700,"km","www.searates.com"]
[]
["EMISSION FACTORS"]
[]
["Mode","Type","Value","Units","Source"]
["Air EF","None",0,"kg CO2e/kg"]
["Air EF","Long Haul",{"$f":"('FPX Reference Data'!D1163*C4)/1000","v":0.74448000000000003},"kg CO2e/kg"]
["Air EF","Short Haul",{"$f":"('FPX Reference Data'!D1164*C5)/1000","v":3.518173640552996},"kg CO2e/kg"]
["Air EF","Domestic",{"$f":"('FPX Reference Data'!D1162*C6)/1000","v":7.2800000000000017E-2},"kg CO2e/kg"]
["Road EF","None",0,"kg CO2e/kg"]
["Road EF","Long haul",{"$f":"(C7*'FPX Reference Data'!$D$1299)/(1000*'FPX Reference Data'!$D$1287)","v":0.60209424083769636},"kg CO2e/kg"]
["Road EF","Short haul",{"$f":"(C8*'FPX Reference Data'!$D$1299)/(1000*'FPX Reference Data'!$D$1287)","v":0.12041884816753928},"kg CO2e/kg"]
["Road EF","Domestic",{"$f":"(C9*'FPX Reference Data'!$D$1299)/(1000*'FPX Reference Data'!$D$1287)","v":2.4083769633507855E-2},"kg CO2e/kg"]
["Sea EF","None",0,"kg CO2e/kg"]
["Sea EF","Long haul",{"$f":"('FPX Reference Data'!$D$1191*C10)/1000","v":9.4162354838709661E-2},"kg CO2e/kg"]
["Sea EF","Medium haul",{"$f":"('FPX Reference Data'!$D$1191*C11)/1000","v":3.8630709677419349E-2},"kg CO2e/kg"]
["Sea EF","Short haul",{"$f":"('FPX Reference Data'!$D$1191*C12)/1000","v":3.380187096774193E-3},"kg CO2e/kg"]
[]
[null,"FOR ROAD, USE ARTICULATED LORRY AVERAGE"]
[null,"MAKE ASSUMPTIONS ON RETURN JOURNEY?"]
[null,"CHECK WITH TOM CALDICOTT ABOUT HOW THE UTILISATION IS USED IN ROAD CALCULATOR"]
[]
[]
[]
[]
["Road EF (kg CO2(e)/tonne/km)","Lorry (articulated, >3.5-33t) - UK",0.18400000000000002,"kg CO2(e)/tonne/km","FPX"]
["Road EF (kg CO2(e)/tonne/km)","Lorry (rigid, >3.5-7.5t) - UK",0.79456000000000004,"kg CO2(e)/tonne/km","FPX"]
["Road EF (kg CO2(e)/tonne/km)","Lorry (rigid, >17t) - UK",0.24130000000000001,"kg CO2(e)/tonne/km","FPX"]
["Road average distance","Average length of haul by commodity - Chemicals",136,"km","FPX"]
["Air EF (kg CO2(e)/tonne/km)","Long Haul",0.71750809989597286,"kg CO2(e)/tonne/km","FPX"]
["Air EF (kg CO2(e)/tonne/km)","Short Haul",2.2472448409283112,"kg CO2(e)/tonne/km","FPX"]
["Air EF (kg CO2(e)/tonne/km)","Domestic (UK)",2.3454490937019972,"kg CO2(e)/tonne/km","FPX"]
[]
[]
["Sea EF (kg CO2(e)/tonne/km)","Cargo, general - average - GLO",1.5376129032258067E-2,"kg CO2(e)/tonne/km","FPX"]

{"sheet":"TransportDefaults - ctry to UK","index":15,"n_rows":70,"n_cols":8,"rows_kept":70,"cut":false,"hidden":true,"merged":[]}
["Country/Region","Air","Sea","Road","Region (for default buttons)"]
["Africa","None","Medium haul","Short haul","Africa",null,null,"United Kingdom"]
["Argentina ","None","Medium haul","Short haul","South America",null,null,"Western Europe"]
["Asia subcontinent","None","Long haul","Short haul","Asia",null,null,"Eastern Europe"]
["Australia","None","Long haul","Short haul","Australasia",null,null,"North America"]
["Austria","None","Short haul","Short haul","Western Europe",null,null,"South America"]
["Bangladesh ","None","Long haul","Short haul","Asia",null,null,"Asia"]
["Belgium ","None","Short haul","Short haul","Western Europe",null,null,"Middle East"]
["Brazil ","None","Medium haul","Short haul","South America",null,null,"Australasia"]
["Bulgaria ","None","Short haul","Long haul","Eastern Europe",null,null,"Africa"]
["Canada ","None","Medium haul","Short haul","North America"]
["Central/Eastern Europe","None","Short haul","Long haul","Eastern Europe"]
["Chile","None","Medium haul","Domestic (UK)","South America"]
["China ","None","Long haul","Short haul","Asia"]
["Colombia ","None","Medium haul","Domestic (UK)","South America"]
["Costa Rica ","None","Medium haul","Domestic (UK)","South America"]
["Cyprus","None","Medium haul","Domestic (UK)","Eastern Europe"]
["Czech Republic","None","Short haul","Long haul","Eastern Europe"]
["Denmark","None","Short haul","Short haul","Western Europe"]
["Ecuador ","None","Medium haul","Short haul","South America"]
["Egypt","None","Medium haul","Short haul","Africa"]
["EU 27","None","Short haul","Short haul","Western Europe"]
["Finland ","None","Short haul","Short haul","Western Europe"]
["France ","None","Short haul","Short haul","Western Europe"]
["Germany ","None","Short haul","Short haul","Western Europe"]
["Greece ","None","Short haul","Long haul","Eastern Europe"]
["Guatemala ","None","Medium haul","Short haul","South America"]
["Hungary ","None","Short haul","Long haul","Eastern Europe"]
["India ","None","Long haul","Short haul","Asia"]
["Indonesia ","None","Long haul","Short haul","Asia"]
["Ireland (Republic of) ","None","Short haul","Short haul","Western Europe"]
["Israel ","None","Medium haul","Short haul","Middle East"]
["Italy ","None","Short haul","Long haul","Western Europe"]
["Japan ","None","Long haul","Domestic (UK)","Asia"]
["Kenya ","None","Medium haul","Long haul","Africa"]
["Latin America","None","Medium haul","Short haul","South America"]
["Latvia","None","Short haul","Long haul","Eastern Europe"]
["Malaysia ","None","Long haul","Domestic (UK)","Asia"]
["Malta ","None","Medium haul","Domestic (UK)","Eastern Europe"]
["Mexico ","None","Medium haul","Short haul","South America"]
["Middle East","None","Medium haul","Short haul","Middle East"]
["Netherlands ","None","Short haul","Short haul","Western Europe"]
["New Zealand ","None","Long haul","Short haul","Australasia"]
["North America","None","Medium haul","Long haul","North America"]
["Norway ","None","None","Short haul","Western Europe"]
["Pakistan","None","Long haul","Short haul","Asia"]
["Panama","None","Medium haul","None","South America"]
["Peru","None","Medium haul","Long haul","South America"]
["Philippines","None","Long haul","Domestic (UK)","Asia"]
["Poland ","None","Short haul","Long haul","Eastern Europe"]
["Portugal ","None","Short haul","Short haul","Western Europe"]
["Romania ","None","Short haul","Long haul","Eastern Europe"]
["Russia ","None","Medium haul","Long haul","Eastern Europe"]
["Saudi Arabia","None","Medium haul","Long haul","Middle East"]
["Serbia ","None","Short haul","Long haul","Eastern Europe"]
["Singapore ","None","Long haul","Short haul","Asia"]
["South Africa ","None","Medium haul","Long haul","Africa"]
["South East Asia","None","Long haul","Short haul","Asia"]
["South Korea ","None","Long haul","Short haul","Asia"]
["Spain ","None","Short haul","Short haul","Western Europe"]
["Sweden ","None","Short haul","Short haul","Western Europe"]
["Taiwan","None","Long haul","Domestic (UK)","Asia"]
["Thailand","None","Long haul","Short haul","Asia"]
["Turkey ","None","Short haul","Long haul","Eastern Europe"]
["Ukraine ","None","Short haul","Long haul","Eastern Europe"]
["United Arab Emirates (UAE)","None","Medium haul","Short haul","Middle East"]
["United Kingdom","None","None","Domestic (UK)","United Kingdom"]
["US Average","None","Medium haul","Long haul","United Kingdom"]
["Vietnam ","None","Long haul","Short haul","Asia"]
["World average","None","Medium haul","Short haul","Asia"]

{"sheet":"TransportDefault - between ctrs","index":16,"n_rows":38,"n_cols":12,"rows_kept":38,"cut":false,"hidden":true,"merged":[[29,1,37,1],[1,3,1,11],[3,1,11,1],[14,3,14,11],[16,1,24,1],[27,3,27,11]]}
[]
[null,"AIR",null,"DESTINATION"]
[null,null,null,"United Kingdom","Western Europe","Eastern Europe","North America","South America","Asia","Middle East","Australasia","Africa"]
[null,"SOURCE","United Kingdom","None","None","None","None","None","None","None","None","None"]
[null,null,"Western Europe","None","None","None","None","None","None","None","None","None"]
[null,null,"Eastern Europe","None","None","None","None","None","None","None","None","None"]
[null,null,"North America","None","None","None","None","None","None","None","None","None"]
[null,null,"South America","None","None","None","None","None","None","None","None","None"]
[null,null,"Asia","None","None","None","None","None","None","None","None","None"]
[null,null,"Middle East","None","None","None","None","None","None","None","None","None"]
[null,null,"Australasia","None","None","None","None","None","None","None","None","None"]
[null,null,"Africa","None","None","None","None","None","None","None","None","None"]
[]
[]
[null,"SEA",null,"DESTINATION"]
[null,null,null,"United Kingdom","Western Europe","Eastern Europe","North America","South America","Asia","Middle East","Australasia","Africa"]
[null,"SOURCE","United Kingdom","None","Short haul","Short haul","Medium haul","Medium haul","Long haul","Medium haul","Long haul","Medium haul"]
[null,null,"Western Europe","Short haul","None","None","Medium haul","Medium haul","Long haul","Medium haul","Long haul","Medium haul"]
[null,null,"Eastern Europe","Short haul","None","None","Medium haul","Medium haul","Long haul","None","Long haul","Medium haul"]
[null,null,"North America","Medium haul","Medium haul","Medium haul","None","Medium haul","Long haul","Long haul","Long haul","Medium haul"]
[null,null,"South America","Medium haul","Medium haul","Medium haul","Medium haul","None","Long haul","Long haul","Long haul","Medium haul"]
[null,null,"Asia","Long haul","Long haul","Long haul","Long haul","Long haul","None","Medium haul","Medium haul","Medium haul"]
[null,null,"Middle East","Medium haul","Medium haul","None","Long haul","Long haul","Medium haul","None","Medium haul","Medium haul"]
[null,null,"Australasia","Long haul","Long haul","Long haul","Long haul","Long haul","Medium haul","Medium haul","None","Medium haul"]
[null,null,"Africa","Medium haul","Medium haul","Medium haul","Medium haul","Medium haul","Medium haul","Medium haul","Medium haul","None"]
[]
[]
[null,"ROAD",null,"DESTINATION"]
[null,null,null,"United Kingdom","Western Europe","Eastern Europe","North America","South America","Asia","Middle East","Australasia","Africa"]
[null,"SOURCE","United Kingdom","Domestic","Short haul","Long haul","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul"]
[null,null,"Western Europe","Short haul","Domestic","Long haul","Short haul","Short haul","Short haul","Long haul","Short haul","Short haul"]
[null,null,"Eastern Europe","Long haul","Long haul","Domestic","Long haul","Long haul","Long haul","Long haul","Long haul","Short haul"]
[null,null,"North America","Short haul","Short haul","Long haul","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul"]
[null,null,"South America","Short haul","Short haul","Long haul","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul"]
[null,null,"Asia","Short haul","Short haul","Long haul","Short haul","Short haul","Long haul","Short haul","Short haul","Short haul"]
[null,null,"Middle East","Short haul","Long haul","Long haul","Short haul","Short haul","Short haul","Domestic","Short haul","Short haul"]
[null,null,"Australasia","Short haul","Short haul","Long haul","Short haul","Short haul","Short haul","Short haul","Domestic","Short haul"]
[null,null,"Africa","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul","Short haul"]

{"sheet":"TransDefaults - Input to form","index":17,"n_rows":4,"n_cols":4,"rows_kept":4,"cut":false,"hidden":true,"merged":[]}
[null,"Air","Sea","Road"]
["API","None","Long haul","Domestic"]
["Excipient","None","None","Domestic"]
["Packaging","None","None","Domestic"]